(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 0)
    (zones 0)
    (modules 15)
    (nets 27)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /GND)
  (net 2 "Net-(P1-Pad3)")
  (net 3 "Net-(P1-Pad2)")
  (net 4 /3.3V)
  (net 5 "Net-(P2-Pad3)")
  (net 6 "Net-(P2-Pad2)")
  (net 7 /out)
  (net 8 "Net-(P3-Pad2)")
  (net 9 "Net-(SJ1-Pad2)")
  (net 10 "Net-(SJ3-Pad2)")
  (net 11 "Net-(SJ5-Pad2)")
  (net 12 "Net-(SJ7-Pad2)")
  (net 13 "Net-(U1-Pad5)")
  (net 14 "Net-(U1-Pad3)")
  (net 15 "Net-(U1-Pad2)")
  (net 16 "Net-(U1-Pad1)")
  (net 17 "Net-(U2-Pad5)")
  (net 18 "Net-(U2-Pad6)")
  (net 19 "Net-(U2-Pad7)")
  (net 20 "Net-(U2-Pad9)")
  (net 21 "Net-(U2-Pad10)")
  (net 22 "Net-(U2-Pad11)")
  (net 23 "Net-(U2-Pad12)")
  (net 24 "Net-(U2-Pad13)")
  (net 25 /sdl)
  (net 26 /sda)

  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /GND)
    (add_net /out)
    (add_net /sda)
    (add_net /sdl)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(SJ1-Pad2)")
    (add_net "Net-(SJ3-Pad2)")
    (add_net "Net-(SJ5-Pad2)")
    (add_net "Net-(SJ7-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
  )

  (module R:RM065 (layer F.Cu) (tedit 5CB48354) (tstamp 61112976)
    (at 113 35)
    (path /611109DA)
    (fp_text reference VR1 (at 0 -6.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Poten (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.81 -5.08) (end -3.81 -5.08) (layer F.SilkS) (width 0.15))
    (fp_arc (start 0 0) (end -3.81 -5.08) (angle -286.2602047) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.5 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 0 -2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 1 thru_hole circle (at -2.5 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3V))
  )

  (module U:SO16 (layer F.Cu) (tedit 5D88D7C8) (tstamp 6111296D)
    (at 117 50.5)
    (path /6112038F)
    (fp_text reference U2 (at 6.985 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PCF8574 (at -0.127 -0.127) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start -5.969 0) (end -5.842001 0.761999) (angle -161.0753556) (layer F.SilkS) (width 0.17))
    (fp_line (start 5.95 5.725) (end -5.95 5.725) (layer F.SilkS) (width 0.17))
    (fp_line (start 5.95 -5.725) (end 5.95 5.725) (layer F.SilkS) (width 0.17))
    (fp_line (start -5.95 -5.725) (end 5.95 -5.725) (layer F.SilkS) (width 0.17))
    (fp_line (start -5.95 5.725) (end -5.95 -5.725) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -4.445 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(SJ7-Pad2)"))
    (pad 2 smd rect (at -3.175 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(SJ5-Pad2)"))
    (pad 3 smd rect (at -1.905 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SJ1-Pad2)"))
    (pad 4 smd rect (at -0.635 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /out))
    (pad 5 smd rect (at 0.635 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at 1.905 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 3.175 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 4.445 4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 9 smd rect (at 4.445 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 3.175 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 1.905 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 0.635 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at -0.635 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at -1.905 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 25 /sdl))
    (pad 15 smd rect (at -3.175 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 26 /sda))
    (pad 16 smd rect (at -4.445 -4.4) (size 0.7 2.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V))
  )

  (module U:SOP8 (layer F.Cu) (tedit 5D9B0CDC) (tstamp 61112954)
    (at 104.5 50.5 180)
    (path /6111685C)
    (fp_text reference U1 (at 4.2 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM393 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center -1.9 1.9) (end -1.9 2.2) (layer F.SilkS) (width 0.17))
    (fp_line (start -2.54 2.54) (end -2.54 -2.54) (layer F.SilkS) (width 0.17))
    (fp_line (start 3.175 2.54) (end -2.54 2.54) (layer F.SilkS) (width 0.17))
    (fp_line (start 3.175 -2.54) (end 3.175 2.54) (layer F.SilkS) (width 0.17))
    (fp_line (start -2.54 -2.54) (end 3.175 -2.54) (layer F.SilkS) (width 0.17))
    (pad 8 smd rect (at -1.905 -3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V))
    (pad 7 smd rect (at -0.635 -3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /out))
    (pad 6 smd rect (at 0.635 -3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P3-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at 1.905 3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at 0.635 3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -0.635 3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -1.905 3.7 180) (size 0.55 1.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
  )

  (module Jumper:SolderStrap0603 (layer B.Cu) (tedit 5D9C8DE1) (tstamp 61112943)
    (at 140 54.25)
    (path /61123FB7)
    (fp_text reference SJ8 (at -2.2 0 -90) (layer B.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -0.9) (layer B.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)) (justify mirror))
    )
    (fp_poly (pts (xy -1.1 0.6) (xy 1.1 0.6) (xy 1.1 -0.6) (xy -1.1 -0.6)) (layer B.Mask) (width 0))
    (fp_poly (pts (xy -0.05 0.5) (xy 1.1 0.5) (xy 1.1 -0.5) (xy -0.05 -0.5)
      (xy 0.3 0)) (layer B.Cu) (width 0))
    (fp_poly (pts (xy -1.1 0.5) (xy -0.35 0.5) (xy 0 0) (xy -0.35 -0.5)
      (xy -1.1 -0.5)) (layer B.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 0.5) (angle -180) (layer B.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 -0.5) (angle -180) (layer B.SilkS) (width 0.3))
    (fp_line (start -1.1 0.5) (end 1.1 0.5) (layer B.SilkS) (width 0.3))
    (fp_line (start 1.1 -0.5) (end -1.1 -0.5) (layer B.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(SJ7-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer B.Cu) (tedit 5D9C8DE1) (tstamp 61112936)
    (at 139.905 56.005)
    (path /6112161F)
    (fp_text reference SJ7 (at -2.2 0 -90) (layer B.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)) (justify mirror))
    )
    (fp_text value Jumper (at 0 -0.9) (layer B.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)) (justify mirror))
    )
    (fp_poly (pts (xy -1.1 0.6) (xy 1.1 0.6) (xy 1.1 -0.6) (xy -1.1 -0.6)) (layer B.Mask) (width 0))
    (fp_poly (pts (xy -0.05 0.5) (xy 1.1 0.5) (xy 1.1 -0.5) (xy -0.05 -0.5)
      (xy 0.3 0)) (layer B.Cu) (width 0))
    (fp_poly (pts (xy -1.1 0.5) (xy -0.35 0.5) (xy 0 0) (xy -0.35 -0.5)
      (xy -1.1 -0.5)) (layer B.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 0.5) (angle -180) (layer B.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 -0.5) (angle -180) (layer B.SilkS) (width 0.3))
    (fp_line (start -1.1 0.5) (end 1.1 0.5) (layer B.SilkS) (width 0.3))
    (fp_line (start 1.1 -0.5) (end -1.1 -0.5) (layer B.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(SJ7-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 4 /3.3V) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 61112929)
    (at 134.5 45.25)
    (path /6112D439)
    (fp_text reference SJ6 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(SJ5-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 6111291C)
    (at 134.5 43.5)
    (path /6112D433)
    (fp_text reference SJ5 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(SJ5-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 6111290F)
    (at 134.5 41.25)
    (path /61157566)
    (fp_text reference SJ4 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(SJ3-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 61112902)
    (at 134.5 39.5)
    (path /6115756E)
    (fp_text reference SJ3 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(SJ3-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 611128F5)
    (at 134.5 35.5)
    (path /6112DB43)
    (fp_text reference SJ2 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SJ1-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module Jumper:SolderStrap0603 (layer F.Cu) (tedit 5D9C8DE1) (tstamp 611128E8)
    (at 134.5 37.25)
    (path /6112DB3D)
    (fp_text reference SJ1 (at -2.2 0 90) (layer F.SilkS)
      (effects (font (size 0.9 0.7) (thickness 0.17)))
    )
    (fp_text value Jumper (at 0 0.9) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_poly (pts (xy -1.1 -0.6) (xy 1.1 -0.6) (xy 1.1 0.6) (xy -1.1 0.6)) (layer F.Mask) (width 0))
    (fp_poly (pts (xy -0.05 -0.5) (xy 1.1 -0.5) (xy 1.1 0.5) (xy -0.05 0.5)
      (xy 0.3 0)) (layer F.Cu) (width 0))
    (fp_poly (pts (xy -1.1 -0.5) (xy -0.35 -0.5) (xy 0 0) (xy -0.35 0.5)
      (xy -1.1 0.5)) (layer F.Cu) (width 0))
    (fp_arc (start 1.1 0) (end 1.1 -0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_arc (start -1.1 0) (end -1.1 0.5) (angle 180) (layer F.SilkS) (width 0.3))
    (fp_line (start -1.1 -0.5) (end 1.1 -0.5) (layer F.SilkS) (width 0.3))
    (fp_line (start 1.1 0.5) (end -1.1 0.5) (layer F.SilkS) (width 0.3))
    (pad 2 smd circle (at 1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SJ1-Pad2)") (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
    (pad 1 smd circle (at -1.1 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V) (solder_mask_margin 0.1) (solder_paste_margin_ratio -0.5))
  )

  (module R:0805 (layer F.Cu) (tedit 5D9C976A) (tstamp 611128DB)
    (at 110.5 61)
    (path /611147E9)
    (fp_text reference R2 (at 0 1.4 180) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value R (at -0.875 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P3-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5D9C976A) (tstamp 611128D3)
    (at 146.714999 51.13)
    (path /6111CB48)
    (fp_text reference R1 (at 0 1.4 180) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10K (at -0.875 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /out) (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /3.3V) (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Bornier:Bornier2.54_1x4 (layer F.Cu) (tedit 5B3CCB63) (tstamp 611128CB)
    (at 118.5 23.5 180)
    (path /6110FA61)
    (fp_text reference P2 (at -6.096 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value I2C_OUT (at 0 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.31 -2.95) (end 5.31 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 -2.95) (end -5.31 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 -2.95) (end 5.31 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.31 2.54) (end -5.31 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 3.35) (end 5.31 3.35) (layer F.SilkS) (width 0.15))
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /3.3V))
  )

  (module Bornier:Bornier2.54_1x4 (layer F.Cu) (tedit 5B3CCB63) (tstamp 611128BE)
    (at 106.5 23.5 180)
    (path /6110F825)
    (fp_text reference P1 (at -6.096 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value I2C_IN (at 0 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.31 -2.95) (end 5.31 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 -2.95) (end -5.31 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 -2.95) (end 5.31 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.31 2.54) (end -5.31 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.31 3.35) (end 5.31 3.35) (layer F.SilkS) (width 0.15))
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /3.3V))
  )

  (gr_line (start 100 60) (end 100 20) (layer Edge.Cuts) (width 0.05) (tstamp 61112CE3))
  (gr_line (start 125 60) (end 100 60) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 20) (end 125 60) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 20) (end 125 20) (layer Edge.Cuts) (width 0.05))

)
