(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "/GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "/3.3V")
  (net 5 "/nrst")
  (net 6 "/boot0")
  (net 7 "Net-(C14-Pad1)")
  (net 8 "/12V")
  (net 9 "Net-(C17-Pad1)")
  (net 10 "Net-(C18-Pad1)")
  (net 11 "/5V")
  (net 12 "/OUT_230V_3")
  (net 13 "Net-(JP1-Pad3)")
  (net 14 "Net-(JP1-Pad2)")
  (net 15 "/OUT_230V_1")
  (net 16 "Net-(JP2-Pad3)")
  (net 17 "Net-(JP2-Pad2)")
  (net 18 "/OUT_230V_2")
  (net 19 "Net-(JP3-Pad3)")
  (net 20 "Net-(JP3-Pad2)")
  (net 21 "/OUT_230V_4")
  (net 22 "Net-(JP4-Pad3)")
  (net 23 "Net-(JP4-Pad2)")
  (net 24 "Net-(D1-Pad2)")
  (net 25 "/230V")
  (net 26 "Net-(D2-Pad2)")
  (net 27 "Net-(D3-Pad2)")
  (net 28 "Net-(D4-Pad2)")
  (net 29 "Net-(R9-Pad2)")
  (net 30 "/Flo_HAUT")
  (net 31 "Net-(R7-Pad2)")
  (net 32 "Net-(R10-Pad2)")
  (net 33 "/Flo_BAS")
  (net 34 "Net-(R8-Pad2)")
  (net 35 "Net-(R13-Pad2)")
  (net 36 "/Full_HAUT")
  (net 37 "Net-(R11-Pad2)")
  (net 38 "Net-(R14-Pad2)")
  (net 39 "/Full_BAS")
  (net 40 "Net-(R12-Pad2)")
  (net 41 "Net-(R19-Pad2)")
  (net 42 "/Cro_HAUT")
  (net 43 "Net-(R17-Pad2)")
  (net 44 "Net-(R20-Pad2)")
  (net 45 "/Cro_BAS")
  (net 46 "Net-(R18-Pad2)")
  (net 47 "Net-(R23-Pad1)")
  (net 48 "Net-(R24-Pad1)")
  (net 49 "Net-(R25-Pad1)")
  (net 50 "Net-(R26-Pad1)")
  (net 51 "Net-(R2-Pad1)")
  (net 52 "Net-(R3-Pad1)")
  (net 53 "Net-(R5-Pad2)")
  (net 54 "/mode")
  (net 55 "/Flo_HAUT_IN")
  (net 56 "/Flo_BAS_IN")
  (net 57 "/Full_HAUT_IN")
  (net 58 "/Full_BAS_IN")
  (net 59 "/12V_3_IN")
  (net 60 "Net-(Q5-Pad1)")
  (net 61 "/12V_1_IN")
  (net 62 "Net-(Q6-Pad1)")
  (net 63 "/Cro_HAUT_IN")
  (net 64 "/Cro_BAS_IN")
  (net 65 "/12V_4_IN")
  (net 66 "Net-(Q10-Pad1)")
  (net 67 "/12V_2_IN")
  (net 68 "Net-(Q14-Pad1)")
  (net 69 "/230V_3_IN")
  (net 70 "/230V_1_IN")
  (net 71 "/230V_2_IN")
  (net 72 "/230V_4_IN")
  (net 73 "/Vent1_IN")
  (net 74 "Net-(Q15-Pad1)")
  (net 75 "/Vent2_IN")
  (net 76 "Net-(Q16-Pad1)")
  (net 77 "unconnected-(U1-Pad9)")
  (net 78 "/TX")
  (net 79 "/RX")
  (net 80 "unconnected-(U1-Pad20)")
  (net 81 "unconnected-(U1-Pad19)")
  (net 82 "unconnected-(U1-Pad14)")
  (net 83 "unconnected-(U1-Pad13)")
  (net 84 "unconnected-(U1-Pad12)")
  (net 85 "unconnected-(U1-Pad11)")
  (net 86 "unconnected-(U1-Pad10)")
  (net 87 "unconnected-(U1-Pad7)")
  (net 88 "unconnected-(U1-Pad6)")
  (net 89 "unconnected-(U1-Pad5)")
  (net 90 "unconnected-(U1-Pad4)")
  (net 91 "unconnected-(U1-Pad2)")
  (net 92 "/IN9")
  (net 93 "/IN8")
  (net 94 "unconnected-(U2-Pad57)")
  (net 95 "unconnected-(U2-Pad56)")
  (net 96 "/sda")
  (net 97 "unconnected-(U2-Pad50)")
  (net 98 "/swclk")
  (net 99 "/swdio")
  (net 100 "unconnected-(U2-Pad45)")
  (net 101 "unconnected-(U2-Pad36)")
  (net 102 "unconnected-(U2-Pad35)")
  (net 103 "unconnected-(U2-Pad34)")
  (net 104 "unconnected-(U2-Pad33)")
  (net 105 "/sdl")
  (net 106 "unconnected-(U2-Pad28)")
  (net 107 "/IN7")
  (net 108 "/IN6")
  (net 109 "/IN5")
  (net 110 "/IN4")
  (net 111 "/IN3")
  (net 112 "/IN2")
  (net 113 "/IN1")
  (net 114 "/IN0")
  (net 115 "unconnected-(U2-Pad11)")
  (net 116 "unconnected-(U2-Pad10)")
  (net 117 "unconnected-(U2-Pad9)")
  (net 118 "unconnected-(U2-Pad8)")
  (net 119 "unconnected-(U2-Pad4)")
  (net 120 "unconnected-(U2-Pad3)")
  (net 121 "unconnected-(U2-Pad2)")
  (net 122 "Net-(U2-Pad1)")

  (footprint "C:0603" (layer "F.Cu")
    (tedit 60D1E9C0) (tstamp 00000000-0000-0000-0000-000061711c84)
    (at 162 63.5)
    (property "Partkeepr" "600")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b548")
    (attr through_hole)
    (fp_text reference "C1" (at 0 1.27 180) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 0835881f-80f4-4cdb-8d53-f83549bfb081)
    )
    (fp_text value "22pF" (at -0.7 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 7acb8e30-6415-4807-86e5-377173be0b1b)
    )
    (fp_line (start -0.28 -0.49) (end 0.28 -0.49) (layer "F.SilkS") (width 0.17) (tstamp 986eb6c8-1def-4c3b-b0df-5af2c2ae25db))
    (fp_line (start 0.28 0.49) (end -0.28 0.49) (layer "F.SilkS") (width 0.17) (tstamp bff94bc2-6c68-474a-a752-dd397f1aa7e2))
    (pad "1" smd rect locked (at 0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c0e19891-9f31-4c40-92bd-83d23e80826e))
    (pad "2" smd rect locked (at -0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f0cca973-b13a-411a-8d07-4d4de69df246))
    (model "${MY_PATH}/3D/C.3dshapes/0603.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0603" (layer "F.Cu")
    (tedit 60D1E9C0) (tstamp 00000000-0000-0000-0000-000061711c8c)
    (at 165.1 63.5)
    (property "Partkeepr" "600")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b541")
    (attr through_hole)
    (fp_text reference "C2" (at 0 1.27 180) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 0515369f-f5f9-41e1-9744-24600ebe638a)
    )
    (fp_text value "22pF" (at -0.7 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp b71d3753-7b12-47db-909c-b7f305cbc6de)
    )
    (fp_line (start 0.28 0.49) (end -0.28 0.49) (layer "F.SilkS") (width 0.17) (tstamp 5769c88e-f67d-421a-97e8-7483882fb4b3))
    (fp_line (start -0.28 -0.49) (end 0.28 -0.49) (layer "F.SilkS") (width 0.17) (tstamp 9db31994-0ecf-4487-a817-55996c6af3ec))
    (pad "1" smd rect locked (at 0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f1b0b9d5-c2c7-41a4-bae6-67c8050c6bcc))
    (pad "2" smd rect locked (at -0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8d7ce050-b231-4bab-b9a8-892493d1d0cf))
    (model "${MY_PATH}/3D/C.3dshapes/0603.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711c94)
    (at 186.42 46.46)
    (property "Partkeepr" "607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b5a2")
    (attr through_hole)
    (fp_text reference "C3" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 856922a7-6a83-4003-927c-f51f162c92c2)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp c1a0d706-43e5-464d-a60f-7ae36cb3dd0b)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp a8dead2b-b456-4e54-9246-96f872a4d543))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp b3c6c6e7-f97e-4e72-b506-a3dac61c99c7))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 449dd29f-f81f-4c35-978b-cf2af336793c))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7c16c0d2-95ac-4e86-9267-a7a7f9704e15))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711c9c)
    (at 175.1 56.66)
    (property "Partkeepr" "0607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f17c")
    (attr through_hole)
    (fp_text reference "C4" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 687fbf6c-fbce-429d-b131-3a2bac9efb0a)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d52d93fb-cffc-4239-8461-3f8acbf39d1a)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 3da02167-9960-4e63-8c30-10582b7eca06))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 91f4a8b4-d0d7-499b-8ea3-54d85a6ade42))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ac63da04-5ea8-46e0-93bb-aee46b63a5b0))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d5ca2d70-657b-4226-863f-54407c9795d2))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711ca4)
    (at 181.9 52.92)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b4f8")
    (attr through_hole)
    (fp_text reference "C5" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 191f7881-1cfd-4476-8d52-2d84129bbf93)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 7a683a66-0151-4f1e-b6ed-23e164375a45)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 535e1450-3011-4c58-8b3e-0ed2926d9a9a))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 99c89364-716b-49c5-b380-f32b6d2432ec))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 2fa98770-25c9-4c7b-8fc0-7d35948996f4))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/nrst") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 059e4405-890f-4f1f-bc59-eb304b95e644))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cac)
    (at 206.61 25.63)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b526")
    (attr through_hole)
    (fp_text reference "C6" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp d945ff0c-a2a4-4ee5-8cd4-2ae2373c5682)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e3d91144-acb6-41d2-9737-d24e6aa6c5e8)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 5ff7ec13-4252-4c06-b97a-4a747df37b58))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 9f4285c2-658b-4121-aefd-b7ec835469a4))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 91ebebfd-ac26-43f5-a623-aff57bffb2cb))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 808ecfac-0740-4618-8003-367cfff61f50))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cb4)
    (at 172.35 60.04)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f14b")
    (attr through_hole)
    (fp_text reference "C7" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 1e00d311-0cd3-4f42-996d-d1555b94fd8c)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 6b5257f5-a79a-4f78-9ac4-6374b022fddb)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp a2b88b67-fdc7-4bb5-8838-768dd3439466))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp fcada150-2b90-41fc-b778-f0e0e8a466d4))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 48718af9-9f7e-4625-85f4-b3e0e40c8967))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp a5578c02-8089-4420-9f98-23793f22773f))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cbc)
    (at 143.42 63.6)
    (property "Partkeepr" "606")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b574")
    (attr through_hole)
    (fp_text reference "C8" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 76ff2955-e9b2-4da0-8993-7f4095608092)
    )
    (fp_text value "1µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp c6d2848f-891c-45b1-bc0b-0b5950c89bc0)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 92821857-3622-409d-b38d-68859214958b))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp d9553616-0fa8-4e52-bb3c-2fb8b0dc8cfa))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f5f1e654-5bf9-4d29-b0df-b47bf871381f))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c1bc5f37-c805-4a57-8a6d-2d539ce8d864))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cc4)
    (at 194.66 35.71)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b56b")
    (attr through_hole)
    (fp_text reference "C9" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 8d58eee7-562c-458f-844b-8d2ec1974ef6)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 1b602461-98dc-4e49-bca1-1e8ef98b8afe)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 611c2071-c1ad-4fd9-ae32-2740f9476adc))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp c0bde2cd-afba-40a1-a1a9-cfd579d573d7))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ce0d9fa2-c7b0-498f-9f0b-72ca20a45bd1))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d1883c04-520d-4973-aa6b-ec667a5ca031))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711ccc)
    (at 193.59 38.55)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b562")
    (attr through_hole)
    (fp_text reference "C10" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp e982ee8b-69a9-41ca-b6f2-3ce2dda31338)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 2af86464-0b78-455a-82cd-4f9219380f15)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp c550355a-a9b8-48b4-9c0d-087ed2c3fd87))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp c779cf7f-9fb2-48be-b5ce-301fdfd58606))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 74ead818-cf5a-4390-9b50-82826ead3a61))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7b815d47-a723-4e28-a719-7ef8cfc4c990))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cd4)
    (at 185.6 49.18)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b551")
    (attr through_hole)
    (fp_text reference "C11" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b5308b86-5935-4272-b203-a824430a18a6)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp b40cb1ce-a941-4894-a500-7e547fcd9cb5)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 68cd1d89-f6cf-434b-bf89-93df0b57933e))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp c50f2233-0c1e-47ff-a432-f5a949c60d24))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 81125efa-28f4-4f28-be6d-5c99eae4a0f0))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8aaceaef-72c4-4502-81aa-46adbcb73290))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cdc)
    (at 199.67 35.3)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b50a")
    (attr through_hole)
    (fp_text reference "C12" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 8d7a5f17-0239-4f6c-8939-e63cfabe5f55)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 25b9a349-0ce9-4f28-ada3-69652797ea16)
    )
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp a2145377-3424-49eb-ba64-b67c1075d792))
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp dc2abac7-5958-4ab1-afd3-2b9e75a2d609))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c340deb7-35a5-43a0-ad5a-7aebb5d8b69c))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/boot0") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 10194679-7a5d-43ef-a4de-03029bf1a19d))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711ce4)
    (at 172.35 62.69)
    (property "Partkeepr" "605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b559")
    (attr through_hole)
    (fp_text reference "C13" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 73777ce3-7fd8-4b9b-9e70-6cd182ff2a3b)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e0b9b56a-2527-40bd-9968-f4adaaa0e0f7)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 72030f10-60f5-4307-a092-773736892529))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp bbf814c5-0f25-4f1a-983f-0951816251b0))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 2549c970-d410-49fc-beef-8f620710d545))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp bb7ed91a-bb34-4d8e-8b57-c075e8ce1eb0))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 00000000-0000-0000-0000-000061711cec)
    (at 193.59 41.2)
    (property "Partkeepr" "607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b57b")
    (attr through_hole)
    (fp_text reference "C14" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 1e0eb125-9996-4b0a-b116-443c2efee987)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 44818094-a2be-4779-a529-bf16fc241a18)
    )
    (fp_line (start 0.4 0.74) (end -0.4 0.74) (layer "F.SilkS") (width 0.17) (tstamp 3dedbe33-5aae-4203-8de9-f391175648cc))
    (fp_line (start 0.4 -0.74) (end -0.4 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 7afde38a-7a0e-4a7a-b15b-b8df30a1c221))
    (pad "1" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C14-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp bfabc5dc-37fc-49fa-b3d1-ec1666cc490f))
    (pad "2" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 0025b1a4-2008-4611-85f9-4ecb10e6fa81))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:3216-18" (layer "F.Cu")
    (tedit 60D1EA0D) (tstamp 00000000-0000-0000-0000-000061711cf9)
    (at 188.705001 39.56)
    (property "Partkeepr" "0610")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085c90")
    (attr through_hole)
    (fp_text reference "C15" (at 0 1.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33a5fdc1-c63f-48b7-b9ce-23adf83bc163)
    )
    (fp_text value "100nF" (at 0 -2.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e40cb8eb-f2f7-4813-8bf9-5910528fa1cd)
    )
    (fp_line (start 2.5 -0.75) (end -2.5 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 1379b8d6-6f5f-4e1a-b1b6-7d27b1765415))
    (fp_line (start -2.5 -0.75) (end -2.5 0.75) (layer "F.SilkS") (width 0.17) (tstamp 28499bd9-e2c9-46a7-86c7-b0a8ee422853))
    (fp_line (start -2.5 -1.25) (end -2.5 1.25) (layer "F.SilkS") (width 0.17) (tstamp 303225d9-f769-4e61-90cf-d3ee19059142))
    (fp_line (start -1.5 -1.5) (end -1 -1.5) (layer "F.SilkS") (width 0.17) (tstamp 311c8831-ca08-42f7-a0e3-f3f4deaf0d73))
    (fp_line (start -1.25 -1.75) (end -1.25 -1.25) (layer "F.SilkS") (width 0.17) (tstamp 85d96c97-db80-4871-8777-edafcd1cf3db))
    (fp_line (start 2.5 0.75) (end 2.5 -0.75) (layer "F.SilkS") (width 0.17) (tstamp ba052a0d-1fbf-47ad-b283-05c55b7686c4))
    (fp_line (start -2.5 0.75) (end 2.5 0.75) (layer "F.SilkS") (width 0.17) (tstamp f78e470f-2fbf-445b-b1f2-b9a708170d74))
    (pad "1" smd rect locked (at -1.41 0) (size 2.2 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/12V") (pintype "passive") (tstamp b6dc720b-71a5-40ef-bf99-66790a993cfd))
    (pad "2" smd rect locked (at 1.41 0) (size 2.2 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp b5f11549-110e-4c79-9690-bce6e41fba9b))
    (model "${MY_PATH}/3D/C.3dshapes/3216-18.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:3216-18" (layer "F.Cu")
    (tedit 60D1EA0D) (tstamp 00000000-0000-0000-0000-000061711d06)
    (at 209.395001 18.73)
    (property "Partkeepr" "0610")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085ce4")
    (attr through_hole)
    (fp_text reference "C16" (at 0 1.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3029fd4a-8584-4037-a7d4-f200cfaf7c37)
    )
    (fp_text value "100nF" (at 0 -2.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fc3f68ad-2ca1-43f3-9de9-a3b8f3605371)
    )
    (fp_line (start -2.5 -0.75) (end -2.5 0.75) (layer "F.SilkS") (width 0.17) (tstamp 2f706b0d-cc12-452d-acff-99ea57ed693c))
    (fp_line (start -2.5 0.75) (end 2.5 0.75) (layer "F.SilkS") (width 0.17) (tstamp 5d464318-9816-4290-a35b-5bd97b2422b5))
    (fp_line (start -1.5 -1.5) (end -1 -1.5) (layer "F.SilkS") (width 0.17) (tstamp 73a8a31f-5005-44a8-8ae8-c215f60285dd))
    (fp_line (start 2.5 -0.75) (end -2.5 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 880d9d2b-d1ab-4343-9ed0-21d62b5184b7))
    (fp_line (start -1.25 -1.75) (end -1.25 -1.25) (layer "F.SilkS") (width 0.17) (tstamp a0deabcb-2781-4902-9d0a-7af376573164))
    (fp_line (start -2.5 -1.25) (end -2.5 1.25) (layer "F.SilkS") (width 0.17) (tstamp aeff7257-5903-4eb0-a75f-62c035cfd877))
    (fp_line (start 2.5 0.75) (end 2.5 -0.75) (layer "F.SilkS") (width 0.17) (tstamp c4b92748-89f2-43f9-812d-ac14f74a6147))
    (pad "1" smd rect locked (at -1.41 0) (size 2.2 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/12V") (pintype "passive") (tstamp 381a15c4-3174-41b0-bcd8-a8d407bc68a1))
    (pad "2" smd rect locked (at 1.41 0) (size 2.2 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp 45341e68-92ec-47e8-b432-56851b9ff5b9))
    (model "${MY_PATH}/3D/C.3dshapes/3216-18.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:CP_CMS5X5.8" (layer "F.Cu")
    (tedit 60D1EA38) (tstamp 00000000-0000-0000-0000-000061711d12)
    (at 198.47 19.98)
    (property "Partkeepr" "609")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085c86")
    (attr through_hole)
    (fp_text reference "C17" (at 0 -4 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b9a4321-6d42-4588-9d7b-94c5179475a5)
    )
    (fp_text value "10µF" (at 0 3.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b2e0062-1d12-47b9-843c-c1b1ee511bdd)
    )
    (fp_line (start -2.75 -2.5) (end -2.25 -3) (layer "F.SilkS") (width 0.17) (tstamp 266fc06b-2fcd-4c7e-9067-34b3c1e7cf28))
    (fp_line (start -2.25 -3) (end 2.75 -3) (layer "F.SilkS") (width 0.17) (tstamp 37603aea-0144-421a-a678-3defaa5d4600))
    (fp_line (start 2.75 -3) (end 2.75 3) (layer "F.SilkS") (width 0.17) (tstamp 45e4f3d4-6dd0-4f60-9673-a529f7e4d395))
    (fp_line (start -2.25 3) (end 2.75 3) (layer "F.SilkS") (width 0.17) (tstamp 9a02bdc0-8807-4345-b999-216f495ff777))
    (fp_line (start -2.75 2.5) (end -2.25 3) (layer "F.SilkS") (width 0.17) (tstamp bc37e142-8157-44c4-8971-05f45d3b3b69))
    (fp_line (start -2.75 2.5) (end -2.75 -2.5) (layer "F.SilkS") (width 0.17) (tstamp f09f418a-af79-4c22-bf4c-eda66079c5be))
    (pad "1" smd rect locked (at -2.5 0 90) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C17-Pad1)") (pintype "passive") (tstamp 38dc8e4a-f5d6-43fa-bbac-c5afdf8f8899))
    (pad "2" smd rect locked (at 2.5 0 90) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp 359b5f9b-f6de-43ae-8526-328d08a8c422))
    (model "${MY_PATH}/3D/C.3dshapes/CP_CMS5X5.8.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:CP_CMS5X5.8" (layer "F.Cu")
    (tedit 60D1EA38) (tstamp 00000000-0000-0000-0000-000061711d1e)
    (at 180.47 44.27)
    (property "Partkeepr" "609")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085cda")
    (attr through_hole)
    (fp_text reference "C18" (at 0 -4 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a7bd932-ecef-4130-9c7f-db269a87914e)
    )
    (fp_text value "10µF" (at 0 3.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1e54a28-4037-450c-af11-52df15b6b2ad)
    )
    (fp_line (start -2.75 2.5) (end -2.25 3) (layer "F.SilkS") (width 0.17) (tstamp 03426eb6-c7d3-481a-93c0-e82e12c8a553))
    (fp_line (start -2.25 -3) (end 2.75 -3) (layer "F.SilkS") (width 0.17) (tstamp 06bb113e-2107-46dc-a796-52cac4babebc))
    (fp_line (start -2.75 2.5) (end -2.75 -2.5) (layer "F.SilkS") (width 0.17) (tstamp 1f227d39-74d2-4459-8c9d-e59abee5016e))
    (fp_line (start -2.75 -2.5) (end -2.25 -3) (layer "F.SilkS") (width 0.17) (tstamp 3e37adac-eaa6-4709-bfd9-6eab1f089f95))
    (fp_line (start -2.25 3) (end 2.75 3) (layer "F.SilkS") (width 0.17) (tstamp 83f5aa8f-88fe-436d-8bdc-500c0a2ff48c))
    (fp_line (start 2.75 -3) (end 2.75 3) (layer "F.SilkS") (width 0.17) (tstamp 900407e3-c718-43ab-9983-6f335f1ffb43))
    (pad "1" smd rect locked (at -2.5 0 90) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C18-Pad1)") (pintype "passive") (tstamp cc0179e1-f685-4bd5-afe0-69b33666a8fb))
    (pad "2" smd rect locked (at 2.5 0 90) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp f8c73c29-ef9c-4af6-bd61-e17ab9e87456))
    (model "${MY_PATH}/3D/C.3dshapes/CP_CMS5X5.8.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:CP_CMS4X5.8" (layer "F.Cu")
    (tedit 60D1EA29) (tstamp 00000000-0000-0000-0000-000061711d2a)
    (at 173 51.64)
    (property "Partkeepr" "608")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085cb4")
    (attr through_hole)
    (fp_text reference "C19" (at 0 -4 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c272a4d5-f1d3-4953-a4f1-8681bb182f01)
    )
    (fp_text value "1µF" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f838760a-94de-4e63-8c4a-340370e9777d)
    )
    (fp_line (start -2.75 -2.25) (end -2.75 2.25) (layer "F.SilkS") (width 0.17) (tstamp 18777b86-0cf4-4c6e-92db-951b24af95f1))
    (fp_line (start -2.25 -2.75) (end -2.75 -2.25) (layer "F.SilkS") (width 0.17) (tstamp 370c179d-f17d-4618-80ee-bc0f61765820))
    (fp_line (start 2.75 -2.75) (end -2.25 -2.75) (layer "F.SilkS") (width 0.17) (tstamp 4724e751-e266-4110-abbc-75bb5f91de39))
    (fp_line (start 2.75 2.75) (end 2.75 -2.75) (layer "F.SilkS") (width 0.17) (tstamp 4d179fb4-7ccc-42ca-baa7-69b8de50724f))
    (fp_line (start -2.75 2.25) (end -2.25 2.75) (layer "F.SilkS") (width 0.17) (tstamp db5ace36-9093-40a6-8b05-0c4b8a1ad691))
    (fp_line (start -2.25 2.75) (end 2.75 2.75) (layer "F.SilkS") (width 0.17) (tstamp f8ba000a-708c-4c46-81ae-9854a4d8d074))
    (pad "1" smd rect locked (at -1.7 0 90) (size 1 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (tstamp f78f1b0a-4733-41ea-ab79-693deca14c7b))
    (pad "2" smd rect locked (at 1.7 0 90) (size 1 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp 6234472b-d5ca-4d92-9e96-f3f6048d3ba7))
    (model "${MY_PATH}/3D/C.3dshapes/CP_CMS4X5.8.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:CP_CMS4X5.8" (layer "F.Cu")
    (tedit 60D1EA29) (tstamp 00000000-0000-0000-0000-000061711d36)
    (at 201.41 26.9)
    (property "Partkeepr" "608")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085d08")
    (attr through_hole)
    (fp_text reference "C20" (at 0 -4 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a17e50e0-dd9a-4c2b-8b55-3ed266ba926c)
    )
    (fp_text value "1µF" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9dd6518-2103-4500-99cb-991d3a8ab64d)
    )
    (fp_line (start -2.25 -2.75) (end -2.75 -2.25) (layer "F.SilkS") (width 0.17) (tstamp 0bf6ecef-185c-4961-81fa-e02080ededb1))
    (fp_line (start 2.75 2.75) (end 2.75 -2.75) (layer "F.SilkS") (width 0.17) (tstamp 370e0b7b-4f18-4087-b3f6-0d40275389bd))
    (fp_line (start -2.75 2.25) (end -2.25 2.75) (layer "F.SilkS") (width 0.17) (tstamp 8c8c71ec-f5d4-48a2-86ea-51f91b68cc58))
    (fp_line (start -2.25 2.75) (end 2.75 2.75) (layer "F.SilkS") (width 0.17) (tstamp b2f696f5-4327-4132-a704-9bd98d85208d))
    (fp_line (start 2.75 -2.75) (end -2.25 -2.75) (layer "F.SilkS") (width 0.17) (tstamp c9b3f519-89f4-4195-9b4f-9df4c379008a))
    (fp_line (start -2.75 -2.25) (end -2.75 2.25) (layer "F.SilkS") (width 0.17) (tstamp ef81f5ee-6646-4a6d-bf6d-ae040d03b27e))
    (pad "1" smd rect locked (at -1.7 0 90) (size 1 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/5V") (pintype "passive") (tstamp 02981f2f-7ae5-46c1-917d-d7050d5ca328))
    (pad "2" smd rect locked (at 1.7 0 90) (size 1 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (tstamp 9c709b03-92c6-4f7f-bad1-cce475af6ffc))
    (model "${MY_PATH}/3D/C.3dshapes/CP_CMS4X5.8.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SMA" (layer "F.Cu")
    (tedit 60D1DE13) (tstamp 00000000-0000-0000-0000-000061711d41)
    (at 138.035001 61.72)
    (property "Partkeepr" "1302")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085cc2")
    (attr through_hole)
    (fp_text reference "D5" (at 0 2.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.17)))
      (tstamp 47ba74d5-9445-4d44-b50d-7e30a1e0d486)
    )
    (fp_text value "D" (at 0 -2.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e05a1dfe-2645-4e84-8699-5acd36d735cc)
    )
    (fp_line (start 3 -1.2) (end 3 1.2) (layer "F.SilkS") (width 0.17) (tstamp 21eb17cb-3860-4ac7-a215-8a42348bfefb))
    (fp_line (start -3 -1.6) (end -3 1.6) (layer "F.SilkS") (width 0.17) (tstamp 9e5a4b70-e9b5-426d-9667-d48f5cc5b67e))
    (fp_line (start -3.4 -2.6) (end -2.6 -2.6) (layer "F.SilkS") (width 0.17) (tstamp d20a438d-c619-4ce7-a3cb-146f931fd251))
    (fp_line (start -3 -1.2) (end 3 -1.2) (layer "F.SilkS") (width 0.17) (tstamp dee74514-b6bd-49fa-9784-957a26efefe1))
    (fp_line (start 3 1.2) (end -3 1.2) (layer "F.SilkS") (width 0.17) (tstamp fe54d415-b25b-49cd-b3fd-d30938b068a0))
    (pad "1" smd rect locked (at -2.015 0) (size 1.4 1.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "K") (pintype "passive") (tstamp b58095ae-a4fd-4a76-bd7c-7ea55355a637))
    (pad "2" smd rect locked (at 2.015 0) (size 1.4 1.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C17-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 1fbd7c47-3959-4732-a429-0098f1cdb9ab))
    (model "${KISYS3DMOD}/D.3dshapes/SMA.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SMA" (layer "F.Cu")
    (tedit 60D1DE13) (tstamp 00000000-0000-0000-0000-000061711d4c)
    (at 130.465001 61.72)
    (property "Partkeepr" "1302")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085d16")
    (attr through_hole)
    (fp_text reference "D6" (at 0 2.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.17)))
      (tstamp 9310ec4b-b41a-4eaf-8b14-f2b7274f61e1)
    )
    (fp_text value "D" (at 0 -2.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed5bcb05-9bbd-4f58-afb4-a617ea3a2587)
    )
    (fp_line (start 3 -1.2) (end 3 1.2) (layer "F.SilkS") (width 0.17) (tstamp 35ba699f-20ff-4150-bdb3-081f639d68ce))
    (fp_line (start -3 -1.6) (end -3 1.6) (layer "F.SilkS") (width 0.17) (tstamp 706ad78c-851f-4b0d-a5d8-e8daf42a3385))
    (fp_line (start -3 -1.2) (end 3 -1.2) (layer "F.SilkS") (width 0.17) (tstamp 7f4552c5-fb84-4fd7-9260-2b3e9805520e))
    (fp_line (start 3 1.2) (end -3 1.2) (layer "F.SilkS") (width 0.17) (tstamp b57821b3-9540-42e4-8dd2-c3582378c6c7))
    (fp_line (start -3.4 -2.6) (end -2.6 -2.6) (layer "F.SilkS") (width 0.17) (tstamp c63c2717-3753-4487-b0c5-fe8107f8a1ee))
    (pad "1" smd rect locked (at -2.015 0) (size 1.4 1.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/5V") (pinfunction "K") (pintype "passive") (tstamp b598bcfb-9fca-4846-a53f-2230ed0021cc))
    (pad "2" smd rect locked (at 2.015 0) (size 1.4 1.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C18-Pad1)") (pinfunction "A") (pintype "passive") (tstamp 7f4de3bf-aa09-4d2f-ae63-b071459877f5))
    (model "${KISYS3DMOD}/D.3dshapes/SMA.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 60D1AA45) (tstamp 00000000-0000-0000-0000-000061711d99)
    (at 155 100)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1ce")
    (attr through_hole)
    (fp_text reference "K1" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 2988c339-1223-43b0-935c-08a09c07ddc5)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp fe6ba2f0-5276-48a9-af2e-9906d241c905)
    )
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 4e86b41b-a99e-43eb-a4ef-c6bc6970dae2))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 5839b181-26ed-4d26-a48d-3d064742d677))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 834fc62d-0446-42cf-a564-0064f3b5f17f))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 8d83b797-1651-4922-80e5-c74c94cbef37))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 24 "Net-(D1-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 4edd0360-952a-47b0-903f-e3e03b2dec03))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 4 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp e58b51f5-6172-41b2-80cc-31bcd0f8f50f))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 25 "/230V") (pinfunction "COM") (pintype "input") (tstamp 6440e859-3873-4ca8-85ff-e3fac5913f17))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 14 "Net-(JP1-Pad2)") (pinfunction "NO") (pintype "input") (tstamp 272d6d6c-a73f-43b7-b37e-b8e47701ae92))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 97557994-bdaa-4721-9dd8-1a24d4c5e266))
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 60D1AA45) (tstamp 00000000-0000-0000-0000-000061711da6)
    (at 179.615001 99.73)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bd02")
    (attr through_hole)
    (fp_text reference "K2" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp c244e004-0cbd-471e-bc57-73a2ea619a3e)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 76d7facc-40ad-4efe-99fc-9ab57a7ac110)
    )
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 2a0c155a-b056-41e0-b970-717ab5a41b55))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 387ec953-df65-4cc2-80e3-82c7ab118639))
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 55926c4a-d246-4db3-8ba5-59f5fdf6811f))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp f314daa3-4874-42c9-91a3-49caf162730b))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 26 "Net-(D2-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 318123e5-a9c2-4924-93e2-9b393b6de419))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 4 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp 6845d308-bf70-43b8-9fa3-5d06cbed0843))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 25 "/230V") (pinfunction "COM") (pintype "input") (tstamp 30f68d64-e6e9-4945-91f0-10786812a38b))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 17 "Net-(JP2-Pad2)") (pinfunction "NO") (pintype "input") (tstamp 845107af-eb98-4e34-a352-be4f4baa0ddf))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 16 "Net-(JP2-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 73255b09-0d92-4af9-a5b2-6ee9d8989cd9))
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 60D1AA45) (tstamp 00000000-0000-0000-0000-000061711db3)
    (at 155 120)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d67")
    (attr through_hole)
    (fp_text reference "K3" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp a9ca6ae3-0446-431c-ba14-31fbbc9b8f99)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 048f89bd-eabd-4463-8fb4-588dcd818968)
    )
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 3fe8e104-7dbc-41d9-a3ea-cbb0dafeb039))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 6e9e8138-9ced-487f-8d4e-1d1b84d4a24f))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp a6ee8cdf-3699-46cb-96b1-2f1d96c3a424))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp aebafb55-1e1b-4500-82d6-e3baa4a393ca))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 27 "Net-(D3-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 4ae8d06d-b393-48d0-b76e-0359d42bf1ca))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 4 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp 08b0858b-e458-48bd-bf64-c5f593ceb922))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 25 "/230V") (pinfunction "COM") (pintype "input") (tstamp 32274676-aba7-44b8-ba76-8753cb26be68))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 20 "Net-(JP3-Pad2)") (pinfunction "NO") (pintype "input") (tstamp 2d5061bf-9597-4df2-94aa-877c07cf2a70))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 19 "Net-(JP3-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 971cbc41-e974-4e03-b14c-17dad8a816f7))
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 60D1AA45) (tstamp 00000000-0000-0000-0000-000061711dc0)
    (at 180 120)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa9a")
    (attr through_hole)
    (fp_text reference "K4" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 766e0039-1eea-484c-8414-2d3c182510b4)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp bd4246ac-928e-48b7-84c0-03a54cb73ad3)
    )
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 5ca859b4-85cd-4ef5-85d4-a87cff31ecb3))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 8e90e297-5a63-49a5-8fce-addf0254153d))
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 911a8444-a449-4cd7-9359-c8b613f74849))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp f99e3d9a-fa71-4de6-bc97-4bec6c52286e))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 28 "Net-(D4-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 5afb2f88-58ad-4bc3-83bf-f302e18706d6))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 4 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp 1b325764-d0cc-4185-bdca-02644d09f8f7))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 25 "/230V") (pinfunction "COM") (pintype "input") (tstamp 35a75c76-a531-4990-8001-361aa7e91a09))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 23 "Net-(JP4-Pad2)") (pinfunction "NO") (pintype "input") (tstamp fd215b63-e43d-4187-bafe-39e458dd18d1))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 22 "Net-(JP4-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 7870d899-9efa-446e-a746-880d6d8106c5))
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711dc7)
    (at 181.951 49.725999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250101")
    (attr through_hole)
    (fp_text reference "Q1" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 6572ae06-320a-4736-ae99-faafa4e03213)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d42281b-9cda-4c56-b6ba-d71450e250c8)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(R7-Pad2)") (pintype "input") (tstamp 87b7c348-46b7-4138-9e29-600c81dcbc15))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/Flo_HAUT") (pintype "input") (tstamp 23c52b46-4551-4f3a-b235-da726f1abfce))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R9-Pad2)") (pintype "input") (tstamp 46418040-b7de-4362-bbab-d793499a4e08))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711dce)
    (at 178.251 49.725999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061127f03")
    (attr through_hole)
    (fp_text reference "Q2" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp bdd1e53e-30ca-4995-ba5d-80ab9230fc7e)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a4917ec4-9689-48a9-b524-6528dd0fd56e)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(R8-Pad2)") (pintype "input") (tstamp a6308601-c0a4-4cf6-8d08-348aeb7b7b1a))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/Flo_BAS") (pintype "input") (tstamp cb03686c-246c-4747-a26a-423804347682))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R10-Pad2)") (pintype "input") (tstamp 1a09fada-9a7a-4118-9361-7798024daea4))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711dd5)
    (at 171.451 56.845999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250115")
    (attr through_hole)
    (fp_text reference "Q3" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 2a52c168-4cf2-4762-8054-3252ed72c263)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af81b6db-8ce4-4795-98f6-063082859de7)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(R11-Pad2)") (pintype "input") (tstamp 1c5b0314-ed17-4da2-af08-7e57107aa3bc))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/Full_HAUT") (pintype "input") (tstamp 0bff734b-f597-4b0b-9b99-04b2d52bd008))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R13-Pad2)") (pintype "input") (tstamp 7d7b3399-4074-4aa6-b298-e2a8bdb443b3))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711ddc)
    (at 186.471 43.265999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608ae")
    (attr through_hole)
    (fp_text reference "Q4" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 0a72c9a4-5570-4c82-9323-abdd7a07c15e)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e35d510b-a344-4975-bd68-a4087f214a81)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R12-Pad2)") (pintype "input") (tstamp d16a4c9d-d481-4b31-b8d1-8bf3b50430d9))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/Full_BAS") (pintype "input") (tstamp d332e6aa-a27e-4c92-a826-0a7ab71e922e))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R14-Pad2)") (pintype "input") (tstamp 6a9bc32c-cc62-47e9-b339-98a905ff9e49))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711de3)
    (at 208.161 22.435999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250129")
    (attr through_hole)
    (fp_text reference "Q7" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp f15257b6-adcf-4e6a-ae0b-d86a68470622)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 65d5ae0a-7825-4848-beed-ad85a76dbc4d)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(R17-Pad2)") (pintype "input") (tstamp 2f52f781-c415-4449-b32e-c6e54e5dd0cd))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/Cro_HAUT") (pintype "input") (tstamp d5196f55-f4c0-4340-902f-99e1b4ba73a1))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R19-Pad2)") (pintype "input") (tstamp ba3bc608-6634-47b5-99f9-e85914ca20bd))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711dea)
    (at 196.021 32.515999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654dd")
    (attr through_hole)
    (fp_text reference "Q8" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp d79987cb-43ec-4bd7-9827-b80cfb20abd9)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c81407f-4c93-4343-9fdd-c7cf0004f14c)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(R18-Pad2)") (pintype "input") (tstamp af98ad10-e802-4202-b58d-b220c24d3f12))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/Cro_BAS") (pintype "input") (tstamp 790de9b8-2646-4eb3-ac44-e986e81f13d2))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R20-Pad2)") (pintype "input") (tstamp 1ddaf887-e274-4cd9-8ea8-322634a63634))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711df1)
    (at 178.251 53.465999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1b4")
    (attr through_hole)
    (fp_text reference "Q9" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp cb0504ca-2858-42b0-aaa2-c8e9107195be)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 533369f8-5970-424a-80c9-ee8be94fccbe)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(R23-Pad1)") (pintype "input") (tstamp 034c6631-3f37-4b44-9f85-a3532de0c5b1))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp 29863aaa-d556-433b-bcbe-dc1e732462ed))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D1-Pad2)") (pintype "input") (tstamp 01ae4952-b109-457d-a45c-7ef0a47735ad))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711df8)
    (at 168.701 60.625999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/14a26789-33a4-4b2d-ad64-2339c90d97f7")
    (attr through_hole)
    (fp_text reference "Q11" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 8bc134df-8c6e-4075-9387-ec0d1a544e44)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97f7c2ec-ec36-41f5-b1e3-93530786fac4)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(R24-Pad1)") (pintype "input") (tstamp 66ae2a1b-69db-412f-bd9d-074dc01de8a2))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp 0e1a2205-22cb-4761-a4c0-1b3729d6ca68))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(D2-Pad2)") (pintype "input") (tstamp 90836f2b-ca4f-4390-81a4-f0027f4710d6))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711dff)
    (at 143.471 60.405999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d4d")
    (attr through_hole)
    (fp_text reference "Q12" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 8d4300bd-7cc5-454b-b26b-2603ab3d1cd8)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0949f93-63e7-4703-a030-2f30c8aa706b)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R25-Pad1)") (pintype "input") (tstamp 2df87508-8149-4e22-b124-4a03187509c9))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp 18776d1a-13fe-4e60-a201-8cb340978ffc))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(D3-Pad2)") (pintype "input") (tstamp b8789a7c-33d0-46a5-8b74-19d91bbb492b))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 57E1263D) (tstamp 00000000-0000-0000-0000-000061711e06)
    (at 199.861 32.105999)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa7e")
    (attr through_hole)
    (fp_text reference "Q13" (at 0 0) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp f8025d52-3609-4b3a-9c6d-ad384f9c1a3c)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f12739b4-1583-4a56-a6f7-059368e923bd)
    )
    (pad "1" smd rect locked (at -0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R26-Pad1)") (pintype "input") (tstamp 95c874fe-ccc5-4e09-b9d6-f5319e1c05b9))
    (pad "2" smd rect locked (at 0.95 0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp 3f992d71-44c6-4954-8626-842196a39ba9))
    (pad "3" smd rect locked (at 0 -0.885) (size 0.802 0.972) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(D4-Pad2)") (pintype "input") (tstamp 147a10f6-21b1-47e7-bcbb-e6cfa4196c99))
    (model "${KIPRJMOD}/../packages3d/None-SOT23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e0e)
    (at 183.15 58.25)
    (property "Partkeepr" "910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b501")
    (attr through_hole)
    (fp_text reference "R1" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 71c98124-54de-4437-9de1-55548dfe2660)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 0e877f1a-c6f6-4aa1-a591-f0558909382e)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 12c5a7a1-4e9d-4032-bf97-031a81d60900))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 432099ab-f9f5-40f7-8a66-ee5601bee210))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 51960ddd-e55a-4f34-afd7-3cddeaf203c3))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/nrst") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6586b58f-745d-4f9d-90e6-b1e8dac6be61))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e16)
    (at 183.15 60.92)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f12f")
    (attr through_hole)
    (fp_text reference "R2" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp ebb87563-58e8-4334-b568-8b9df679ad4e)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp c34420a1-9e26-40fe-a64a-d99ba403d370)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3c490dc0-6a38-4ae6-b3c0-8f7549ae3f1a))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 3e7a89ce-b750-4515-86cd-413c98d31113))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(R2-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 562c748c-a3b9-46b7-9394-a7e8223c37dc))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 2e050958-448f-4f36-8e64-f004b805c23b))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e1e)
    (at 210.71 33.65)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f136")
    (attr through_hole)
    (fp_text reference "R3" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 8f6547a0-b819-4b4e-807f-b048f1c2e284)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 081377a1-0250-4c27-a747-063627edd5ed)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 2cd687e7-5b1c-47a8-afc0-aedc05494a6e))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 5d9ed8d8-672e-4d3b-ac68-cee9b5958ece))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(R3-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp dc45cf5a-5a88-4fbe-8752-1068be2a81e5))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f26f737e-b538-44e9-b9ab-c0145d5dfa32))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e26)
    (at 204.39 37.98)
    (property "Partkeepr" "910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b4f0")
    (attr through_hole)
    (fp_text reference "R4" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 7767bbd9-9d4e-4d10-8e47-fe8983c874b6)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 1d58708c-4302-4901-a16c-aa58707190e8)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 1e3862e0-4f0c-4eee-a0a9-4d6b76e2a54f))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp d1225b1e-be5d-4b62-84e2-6592c8d0ec6d))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 00b93b5f-ea71-4b82-9719-46494be6b5ef))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/boot0") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 67e2a671-4c7f-4088-afae-b6af924cb8f1))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e2e)
    (at 210.21 28.31)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f154")
    (attr through_hole)
    (fp_text reference "R5" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 3cb6331c-b530-443d-b6d4-d0e4b2a185a2)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e6f3cc6b-0d49-42b4-ab27-991125b2b9f7)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp bc14833d-8ed0-4677-8ab9-103edb424587))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp d0c49122-70df-46f5-9c51-e8c3b7c363b4))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 2d1ab203-259c-4708-863c-4f899e0a6aeb))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(R5-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1bc5ac42-d85b-4270-81d7-093aaf43fa05))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e36)
    (at 197.19 38.37)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f15d")
    (attr through_hole)
    (fp_text reference "R6" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 96b54b68-e27b-4f71-944f-73cdc020db00)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 9260df69-3401-4ff4-86e8-9a9076896d59)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 05a13802-6732-4591-a57f-3660492f1a49))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 75848791-1924-4c61-8ce8-98aca2d70350))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 4c7ed387-9381-4776-8147-cae7e570df79))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/mode") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp b6619bb3-001e-4357-a4e8-984e35b77894))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e3e)
    (at 178.7 56.67)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125010e")
    (attr through_hole)
    (fp_text reference "R7" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b8eed457-f071-4014-bcbd-af4a76ce8ad3)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 90ef6cd8-75ac-4559-9e97-b3849b326510)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 2bd55c6e-30df-429f-9e1f-198a4536d752))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 635ececf-3d89-4be1-a70b-91e8fff6484f))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/Flo_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 78caf342-1a01-4548-a4e9-ec311328e990))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(R7-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 60012c76-af39-406d-bea2-b949276c2134))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e46)
    (at 175.95 59.34)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061154d7b")
    (attr through_hole)
    (fp_text reference "R8" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp e66b1b7a-369a-4787-968d-54908bbf02b8)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 79bf778d-363c-4c06-a077-dabfcf8d11bd)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 6389e302-4384-4940-88bb-da01bd68e940))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp d988b1cd-4319-42b1-8dcc-138b94a662fd))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/Flo_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp af9f6a6d-7e4d-42a8-bd4e-cdf4722593ff))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(R8-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 419c5c7e-3ca5-4468-8ac7-42ce45359d17))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e4e)
    (at 210.21 25.64)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250107")
    (attr through_hole)
    (fp_text reference "R9" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 3fef7f06-1f46-46a8-962b-93dd2030990b)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d43cc8f6-2069-418d-aa55-e8ac5a365ca9)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 9c29faa1-f1de-45d8-bfc1-da6ab94f391c))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp d075a764-e038-4847-a1bb-4351294fe9f4))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 228c5820-cc7b-4965-bc25-d7600d40cc32))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R9-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7945baaf-b1e7-48d6-9545-790edae47bf5))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e56)
    (at 185.6 51.84)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006113f020")
    (attr through_hole)
    (fp_text reference "R10" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp a83c0eaa-85c8-48b6-84f8-51be3b70975f)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 701e41f0-fdab-483f-880f-517ceeede9c3)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 006d522b-704e-4d30-a298-14a9ce8b2b6e))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp c0ba1923-054d-4821-bfb8-9292a4354aaf))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f6f14ad2-c30d-4f57-9409-885df026718e))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R10-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 841aa9d0-ebfe-469d-bbea-dc6cca60455e))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e5e)
    (at 206.61 28.29)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250122")
    (attr through_hole)
    (fp_text reference "R11" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 7cfbedaa-14b5-4e50-a191-d90ef9b79475)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 3f6b5cb8-3de3-49e1-acc1-ebf63189b0d0)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 410133b3-4e06-4389-8af3-776d60d222ac))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 48138d58-4d7e-4ae1-81d6-d93ed10c035f))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/Full_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7ebdcbd3-2735-4acd-8b37-f20b1adfa662))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(R11-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 2d09e1a6-0f75-402a-a55e-6aa0b8804503))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e66)
    (at 203.27 35.31)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608bb")
    (attr through_hole)
    (fp_text reference "R12" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 12662c1c-1eb4-46c1-bf6e-f7d3717f6e50)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 8ced03e5-4f0b-4d70-ac27-fb5152d3e723)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp edea23e2-4a17-479f-8a1e-59cc0aeb3290))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp fa6e9c3b-4629-416a-91c9-3918d826fb3e))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/Full_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c775f883-0621-4feb-843c-2f574ddc04c2))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R12-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d010de82-cb3c-4275-8b84-911058ea4d9a))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e6e)
    (at 203.51 31.57)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125011b")
    (attr through_hole)
    (fp_text reference "R13" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp d012c50f-1d94-47c3-b579-96f1a4896f0c)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 81925ad5-d800-42e8-b984-480e409bf550)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 0351e034-0ea6-4e5d-923f-9d9a262e0591))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 972dff4c-96b1-4d25-8869-c526d5535c27))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 0b28dbd1-10f9-4266-9c4b-ace5e7aba733))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R13-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 21e23076-ee7a-458f-80b2-620efe0ec5e5))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e76)
    (at 175.95 62.01)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608b4")
    (attr through_hole)
    (fp_text reference "R14" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 0fabf3d8-db9b-48af-b053-b44a082e94fa)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 474a4b34-9a30-436d-b5a4-afb9b29ae049)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp c9be342c-a459-416e-8428-25c839133fce))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp fc61da38-e1f5-4144-8c7c-97118b665f7a))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 92342467-8ce6-4ec3-aef5-efffe2b6e133))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R14-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7c63210a-9626-445b-9325-6abfe3c71ddd))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e7e)
    (at 197.19 41.04)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182abc5")
    (attr through_hole)
    (fp_text reference "R15" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 965a410a-0c8f-48cc-ac3d-a111c4495d8d)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 514d3c50-8fb4-41c2-b308-6bed27177f5a)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 34c8f1db-c1b8-4a08-b51f-545a265d6ee4))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 70d13656-7066-45a2-a4c6-0bfb85dd20bb))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(Q5-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 479fb1e4-0580-4c55-9382-8e850db3542f))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/12V_3_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 5434ccce-930d-4ad3-9062-19a0ebebde74))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e86)
    (at 189.2 49.14)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182afa3")
    (attr through_hole)
    (fp_text reference "R16" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp c288e763-ae40-4081-872a-6173d7cf7e03)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 5d3e1a55-b518-4e70-a6dc-36850d1bda04)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 02cc244a-5ab3-4791-a0d4-cac010c4bf7c))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 19298ec5-b3e0-4712-b214-7d5345650c53))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(Q6-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8192e532-29ed-4cc3-93af-df7bac398fff))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/12V_1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7e8f950f-1bc3-4c81-8f3e-3ace858677ed))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e8e)
    (at 207.11 30.98)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250136")
    (attr through_hole)
    (fp_text reference "R17" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 4f74af00-cddf-4d79-bf96-d3a53766a286)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 5c9dedce-81c9-43e2-91bc-3018a4f4789e)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 91dec8d7-45d1-4cbb-86f0-608d3ca3d20a))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp c2565fb6-3f17-4d5d-9de3-7beed8570769))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Cro_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 00e4d746-7dc3-4913-b904-37b85f573d65))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(R17-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 96415028-ea60-42a8-905b-c3658e4a740a))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e96)
    (at 200.79 37.98)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654ea")
    (attr through_hole)
    (fp_text reference "R18" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 439fab90-796a-4a24-839a-deca374803ee)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 98c3c91c-f9db-44f4-8b12-8cc46a26590a)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3f391381-2bef-4c22-85ee-7d2c62da6c4c))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 4acc4d59-bdb0-48d1-8512-d2703fb319c8))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/Cro_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c77a3dd3-c1b7-4fe2-b18b-1293075ed73b))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(R18-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp b28108d5-0851-41a1-bad7-d37e1c8187ec))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711e9e)
    (at 179.55 59.34)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125012f")
    (attr through_hole)
    (fp_text reference "R19" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 6182c8ca-f5cd-4682-b374-b0ab1ceeb8fe)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp ab91b169-ca47-4bff-8846-8f4fc7bfc25e)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp c88543b5-2a24-4c9f-8d02-476d1ea5ba2c))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp e3df8bb2-5a56-47f1-afb8-2370ab6d034b))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp eadf485e-b59f-41e9-baa9-626fbe7e27d9))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R19-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 26ffcca1-c35b-4d7d-a459-2b8de288b59f))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ea6)
    (at 182.3 55.58)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654e3")
    (attr through_hole)
    (fp_text reference "R20" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp fc36ed88-d9da-47e1-b772-18f51d8d8d3b)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 3c88a53e-bd09-4233-a1c4-ca4f0d099d31)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 4a985698-f61c-456b-8838-48e5a5514b16))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 5f1e5e3a-d6c7-40c8-b1f4-bb6b6d686263))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 80e142fd-4805-4633-982b-6bf4ad8284c1))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R20-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 4e694d55-7527-4f2c-8f41-e00ee72e9b5b))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711eae)
    (at 190.02 46.47)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182a897")
    (attr through_hole)
    (fp_text reference "R21" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b1be1828-acd7-4490-af46-55a75e7532a2)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp a550d1c5-2510-4862-aca2-019af5c14bfc)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 2b1e38bb-1fae-4074-92a4-cdb124ce1037))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp ecc719df-b566-4954-b8b6-b80ef0e57027))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(Q10-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6066c6ea-c5e5-4389-bc19-ff2805fb195a))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/12V_4_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp b676e39e-47c4-47ca-b17b-22f4258542b1))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711eb6)
    (at 189.2 51.81)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061829ada")
    (attr through_hole)
    (fp_text reference "R22" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 61e3d7b8-16af-4fce-abde-5d3c316239eb)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp eaad3da7-f3bd-4a8f-a11d-10a5166c0f96)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 8953115f-ba9c-4b48-af57-7bc0a53255d8))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp f6db126f-5fe6-4c35-9d6b-e3bda3e48b75))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(Q14-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 029d7e25-7e4a-47e0-a0c5-f4cedbe795d6))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/12V_2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9867bd59-f5a4-4077-8174-388883077f2d))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ebe)
    (at 193.62 46.53)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1ad")
    (attr through_hole)
    (fp_text reference "R23" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp a8295147-c942-4084-86f0-b8616f2d9d68)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp a9d0b2b7-f230-4256-b593-13b2a2191b39)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 76005905-8923-4efb-8df5-eac66f8a4d1b))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp ea9eaa19-5ea3-4b9d-bba0-b6eaf8811a02))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(R23-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1ece8c86-363e-455b-ba45-931e0dd88c55))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/230V_3_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d3675753-38f8-4cd6-b560-d8c1555c8225))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ec6)
    (at 207.11 33.65)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bce1")
    (attr through_hole)
    (fp_text reference "R24" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b5144732-de00-4a53-83be-9f7ea91fe7e8)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 799aa4f0-0de1-425a-9c0a-82cf25fa691e)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 41372b05-d490-44e8-aea7-cb370a58a10b))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 69df9568-6e2c-4348-908d-b75ef76a4ca2))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(R24-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d5c43ada-5282-49fb-b7b4-415c6eb64a5b))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/230V_1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6b07f425-3ce4-45c1-8b50-f2e2d65f02bb))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ece)
    (at 197.22 43.71)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d46")
    (attr through_hole)
    (fp_text reference "R25" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp c12a7fc4-32d7-4214-9ead-1a9421ff332d)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 3c00eb26-c2f2-44ed-9ed3-3c0a50bf27cc)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 177f0dc1-8c92-4cb3-ba54-45c9a3ad8fd8))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp dcdca271-d779-4ec3-923b-e13387f6dfb5))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R25-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp bad04416-cd10-4f12-954f-43255802acc2))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/230V_2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8fa97a5d-70d8-4c15-8ad9-71fccca845ba))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ed6)
    (at 185.9 54.51)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa77")
    (attr through_hole)
    (fp_text reference "R26" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 7a47dcc3-b646-4229-bd03-91d66c4ae3f9)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d4a65e12-a603-4f05-a313-1ae225c6f1f1)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp c10e9a64-59b1-4344-9fab-b428d8b59cf8))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp e3918554-e860-4bdb-9b71-1a877f558e93))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R26-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d2080a9d-8fc9-42a9-bbec-976c4eb59e17))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/230V_4_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d6736451-9b8a-4871-b81c-ef40a50bb075))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ede)
    (at 179.55 62.01)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611b737b")
    (attr through_hole)
    (fp_text reference "R31" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 25167f36-d581-474b-9849-aa44394592a4)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e3d78484-204b-4018-97c4-fe68707fc7bb)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 1f72d7be-249d-4871-9645-7e5bd2b40b1c))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 304c7716-51dd-4ed6-ad85-72aad926152d))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(Q15-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1e1ae3b3-2aa8-4887-a258-3e62cefb07f3))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/Vent1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8392b7b3-53a9-4695-960d-cc65514d0f63))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ee6)
    (at 200.79 40.65)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611b9a4d")
    (attr through_hole)
    (fp_text reference "R32" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 0cd5fcf2-7ffa-4098-add5-a10b1faea19c)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 85d1843a-444a-4765-a849-1ad68850f13b)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 44b2f0e8-8289-4115-8ef1-ae5a19e24e29))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 50c7fb4e-ba61-4275-a7c1-bba2f8def458))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(Q16-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 49b04a81-1617-4644-810e-7f6a6e108608))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/Vent2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 194357c4-cdf9-4be5-9e39-fb0c22e75feb))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711eee)
    (at 210.71 30.98)
    (property "Partkeepr" "913")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085c78")
    (attr through_hole)
    (fp_text reference "R33" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp fe8d49fe-cd53-44cd-b7c0-2f435255bd6d)
    )
    (fp_text value "510" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 6b5aebd6-881a-4504-a430-416066b0b287)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 1dcc25f6-4775-423b-9aa4-4db7fa529a73))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 33aeaa2c-923a-4e73-82e6-f94b6de2e35a))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C17-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp b6b8859d-4d55-4f2e-93fd-73c91a188cc7))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 67f5b7f7-35f5-4961-8308-ec8afe403760))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711ef6)
    (at 193.62 43.86)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085ccc")
    (attr through_hole)
    (fp_text reference "R34" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 4cb31a17-9566-46ba-902f-a91964fd9139)
    )
    (fp_text value "1K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 0bf41421-e105-477b-a7ff-0e36403c572d)
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 00d1a047-13c2-40cf-901e-b8bfa2e7ae0c))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3ff7d0fd-1aed-4d0e-adc5-e920c0fe6952))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C18-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 581c11a0-0087-4b8b-b39e-978c5b00478c))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 016a0c16-7e26-4d14-96b2-7448b9604370))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711efe)
    (at 192.8 49.2)
    (property "Partkeepr" "914")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085c7f")
    (attr through_hole)
    (fp_text reference "R35" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 086154dd-a303-4912-bec6-1d7165133e20)
    )
    (fp_text value "330" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d854ce72-8888-4280-9559-c0de13cc11cc)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 02a8238a-67db-4642-a53d-68f66b782895))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp 41b10d00-605b-45d0-8623-ebfc852eb9e5))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp a6b52a33-104f-4a02-8b09-52cf8cb4f6e6))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C17-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp e607a66e-9f6f-4cfb-bcf8-78ee95fed11c))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 5D9C976A) (tstamp 00000000-0000-0000-0000-000061711f06)
    (at 197.22 46.38)
    (property "Partkeepr" "914")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061085cd3")
    (attr through_hole)
    (fp_text reference "R36" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 2be1e3ec-5c2b-4f5c-a4df-7b4e3b483472)
    )
    (fp_text value "330" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 9d42944b-f167-42c5-89eb-b4b9002ae5ae)
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer "F.SilkS") (width 0.17) (tstamp a5875d7a-2fee-4f3d-b344-f1f2ff3a6a04))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer "F.SilkS") (width 0.17) (tstamp b92641e7-a0a1-41b6-89e8-ad6353e55d45))
    (pad "1" smd rect locked (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/5V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1f3126ed-2900-4231-a6ab-24cf000f90cf))
    (pad "2" smd rect locked (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C18-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp b59970bb-b48b-4cea-ab7a-41c3876f7889))
    (model "${KIPRJMOD}/../packages3d/None-R0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:Jumper_2.54mm" (layer "F.Cu")
    (tedit 5885DD74) (tstamp 00000000-0000-0000-0000-000061711f10)
    (at 189.243001 35.134)
    (property "Partkeepr" "0100")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f169")
    (attr through_hole)
    (fp_text reference "SJ1" (at 0 2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp afb854f0-66a1-42ac-8e85-820b59fdd6af)
    )
    (fp_text value "Mode" (at -0.1 -2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 757d7eaa-220d-4c2e-8340-160b90f9a472)
    )
    (fp_line (start 3.048 -1.524) (end 3.048 1.524) (layer "F.SilkS") (width 0.15) (tstamp 060ac10d-477c-4d22-9491-dcd3a829bb09))
    (fp_line (start -3.048 1.524) (end -3.048 -1.524) (layer "F.SilkS") (width 0.15) (tstamp 41745501-2a82-46bd-82aa-889442723f47))
    (fp_line (start 3.048 1.524) (end -3.048 1.524) (layer "F.SilkS") (width 0.15) (tstamp 8da0edaf-fc60-446d-9548-15f67d00dfaf))
    (fp_line (start -3.048 -1.524) (end 3.048 -1.524) (layer "F.SilkS") (width 0.15) (tstamp e7fb4eaf-0717-4722-aba9-389869a61b5e))
    (pad "1" thru_hole rect locked (at -1.27 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/mode") (pintype "passive") (tstamp c3b6ed49-d96e-4700-a1d6-6e6555ae45f8))
    (pad "2" thru_hole circle locked (at 1.27 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/GND") (pintype "passive") (tstamp 4ef2327a-da7f-4301-9793-da73e7634324))
  )

  (footprint "SW:SW" (layer "F.Cu")
    (tedit 57260B93) (tstamp 00000000-0000-0000-0000-000061711f1a)
    (at 196.165001 29.644999)
    (property "Partkeepr" "200")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b4e9")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -6.985) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8442db21-d58c-4d96-af5b-950ec62229bf)
    )
    (fp_text value "reset" (at 0 -2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10531650-221d-4ad9-8eae-3529cbf8cb11)
    )
    (fp_line (start -1.27 -4.445) (end -1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp 015008ea-d10a-4cd7-9bdc-6565f7e4f6f1))
    (fp_line (start 1.27 -0.635) (end -1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp 8a7cb0f7-324a-479b-94ba-65d8ae65ee7a))
    (fp_line (start 1.27 -4.445) (end 1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp a39a5d17-340d-48e1-9815-c829a1695028))
    (fp_line (start -1.27 -4.445) (end 1.27 -4.445) (layer "F.SilkS") (width 0.15) (tstamp a7c177bd-a132-4c9b-9ee9-8e254e0be5ba))
    (pad "1" smd rect locked (at 0 0) (size 1.524 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/nrst") (pinfunction "1") (pintype "passive") (tstamp 8eda936b-2bf5-4dab-a229-5f1154838820))
    (pad "2" smd rect locked (at 0 -5.08) (size 1.524 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "2") (pintype "passive") (tstamp 10e85ef5-a896-4a6f-8315-2f2d7c7e4dfc))
  )

  (footprint "SW:SW" (layer "F.Cu")
    (tedit 57260B93) (tstamp 00000000-0000-0000-0000-000061711f24)
    (at 204.465001 22.474999)
    (property "Partkeepr" "200")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b511")
    (attr through_hole)
    (fp_text reference "SW2" (at 0 -6.985) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f4549470-e3be-40b5-abac-7d0e9335d499)
    )
    (fp_text value "boot" (at 0 -2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97d3acf2-5338-4bcb-83a7-71d841ac5f54)
    )
    (fp_line (start 1.27 -0.635) (end -1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp 1ed94466-39ee-405b-b251-1ea1ee2176a8))
    (fp_line (start 1.27 -4.445) (end 1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp 30b1649a-353d-4382-9557-9493a45ec36c))
    (fp_line (start -1.27 -4.445) (end -1.27 -0.635) (layer "F.SilkS") (width 0.15) (tstamp 8e054767-aff6-4f1d-8977-f7af90607097))
    (fp_line (start -1.27 -4.445) (end 1.27 -4.445) (layer "F.SilkS") (width 0.15) (tstamp d700bd67-dd28-4810-9916-9146e55ef8ec))
    (pad "1" smd rect locked (at 0 0) (size 1.524 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/boot0") (pinfunction "1") (pintype "passive") (tstamp ae7dc62b-781d-49ea-a99f-3773df09f3de))
    (pad "2" smd rect locked (at 0 -5.08) (size 1.524 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "2") (pintype "passive") (tstamp a30c965f-6e85-4f10-beb2-212738dbf56c))
  )

  (footprint "Module:ESP-12F" (layer "F.Cu")
    (tedit 5B3A1A94) (tstamp 00000000-0000-0000-0000-000061711f42)
    (at 75.25 37.5)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006103f18c")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -13) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3632aab-48b3-41d2-9159-d102dc2b00d4)
    )
    (fp_text value "ESP-12F" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f83fb8ce-8ac1-48e9-ad01-857c1cfa1b3e)
    )
    (fp_line (start -6.5 -12) (end 6.5 -12) (layer "F.SilkS") (width 0.15) (tstamp 7128d8be-f5c8-4ea3-8ad1-60d6dd546a04))
    (fp_line (start 6.5 10.5) (end -6.5 10.5) (layer "F.SilkS") (width 0.15) (tstamp aadba9f1-7bb3-4fd0-8239-9d2af688cbc5))
    (fp_line (start 6.5 -12) (end 6.5 10.5) (layer "F.SilkS") (width 0.15) (tstamp ca36916c-7ff6-488a-b736-622b4cc9f296))
    (fp_line (start -6.5 10.5) (end -6.5 -12) (layer "F.SilkS") (width 0.15) (tstamp d0922b9e-aeb4-44d8-86f0-e68056f8e6d1))
    (pad "1" smd rect locked (at -7.6 -3.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(R2-Pad1)") (pinfunction "RST") (pintype "input") (tstamp 0090a6e3-1f22-45d0-8630-32a64dd41a96))
    (pad "2" smd rect locked (at -7.6 -1.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "unconnected-(U1-Pad2)") (pinfunction "ADC") (pintype "input+no_connect") (tstamp fd1d1637-3110-49b4-8752-2ece1e6e1c1b))
    (pad "3" smd rect locked (at -7.6 0.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(R3-Pad1)") (pinfunction "EN") (pintype "input") (tstamp 09111597-f1c0-4dd6-ab67-92fe6d70b111))
    (pad "4" smd rect locked (at -7.6 2.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "unconnected-(U1-Pad4)") (pinfunction "GPIO16") (pintype "input+no_connect") (tstamp 6b6b5787-58a9-4c8c-bc47-8db4e0f17f1e))
    (pad "5" smd rect locked (at -7.6 4.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "unconnected-(U1-Pad5)") (pinfunction "GPIO14") (pintype "input+no_connect") (tstamp daef01bd-f163-4713-93c1-b883794ea974))
    (pad "6" smd rect locked (at -7.6 6.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "unconnected-(U1-Pad6)") (pinfunction "GPIO12") (pintype "input+no_connect") (tstamp 4e03e764-3eb5-4d99-a654-3bdc54b5c475))
    (pad "7" smd rect locked (at -7.6 8.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "unconnected-(U1-Pad7)") (pinfunction "GPIO13") (pintype "input+no_connect") (tstamp 9b723637-4cd3-4663-bc8e-ef10e2d31d02))
    (pad "8" smd rect locked (at -7.6 10.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VCC") (pintype "input") (tstamp 84607d4e-9517-484a-a74c-cde40e759bc4))
    (pad "9" smd rect locked (at -5 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "unconnected-(U1-Pad9)") (pinfunction "CS0") (pintype "input+no_connect") (tstamp 80a2d563-63fd-45c6-bd1d-c9e2f66b2fb2))
    (pad "10" smd rect locked (at -3 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "unconnected-(U1-Pad10)") (pinfunction "MISO") (pintype "input+no_connect") (tstamp af6071e2-06e4-4eac-b3fa-58076480ec43))
    (pad "11" smd rect locked (at -1 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "unconnected-(U1-Pad11)") (pinfunction "GPIO9") (pintype "input+no_connect") (tstamp bc787990-2cba-4bf0-9938-da42f730c96c))
    (pad "12" smd rect locked (at 1 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "unconnected-(U1-Pad12)") (pinfunction "GPIO10") (pintype "input+no_connect") (tstamp 641629e7-a060-4944-aca4-adcbe16d82db))
    (pad "13" smd rect locked (at 3 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "unconnected-(U1-Pad13)") (pinfunction "MOSI") (pintype "input+no_connect") (tstamp 0da77f0c-6e13-470e-8d0d-997c385f710c))
    (pad "14" smd rect locked (at 5 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "unconnected-(U1-Pad14)") (pinfunction "SCLK") (pintype "input+no_connect") (tstamp 2f2bd2e6-7664-410c-b335-71d50112eb29))
    (pad "15" smd rect locked (at 7.6 10.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "GND") (pintype "input") (tstamp 46d7866d-3dbf-4887-adc4-da636e36fef0))
    (pad "16" smd rect locked (at 7.6 8.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "GPIO15") (pintype "input") (tstamp 73f0bfec-855c-439b-9775-9942a109b8b3))
    (pad "17" smd rect locked (at 7.6 6.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(R5-Pad2)") (pinfunction "GPIO2") (pintype "input") (tstamp 962db1fa-2f02-49af-b09e-46f4e0728a74))
    (pad "18" smd rect locked (at 7.6 4.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/mode") (pinfunction "GPIO0") (pintype "input") (tstamp f99b11d8-5701-4fe9-9b2e-65cf5e535999))
    (pad "19" smd rect locked (at 7.6 2.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "unconnected-(U1-Pad19)") (pinfunction "GPIO4") (pintype "input+no_connect") (tstamp 9dfefbea-f340-46c7-81fb-bfaedd3c433b))
    (pad "20" smd rect locked (at 7.6 0.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "unconnected-(U1-Pad20)") (pinfunction "GPIO5") (pintype "input+no_connect") (tstamp 309f3f79-38d8-4f88-8e93-da1e8ad9f409))
    (pad "21" smd rect locked (at 7.6 -1.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/RX") (pinfunction "RXD") (pintype "input") (tstamp b9f5ba56-b5e2-4107-96eb-bb4d9edfea73))
    (pad "22" smd rect locked (at 7.6 -3.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/TX") (pinfunction "TXD") (pintype "input") (tstamp 262b7571-9fab-46e0-961c-b492c9f035ac))
  )

  (footprint "U:LQFP64" (layer "F.Cu")
    (tedit 592D6E71) (tstamp 00000000-0000-0000-0000-000061711f8b)
    (at 50 56.584999)
    (property "Partkeepr" "2102")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b52f")
    (attr through_hole)
    (fp_text reference "U2" (at 6.8 5.8) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 470c3d40-be43-40f9-900e-b028544c9d30)
    )
    (fp_text value "STM32F401RC" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ffa9fbb-d010-4198-b8a6-0a758f44bcaa)
    )
    (fp_line (start 5 -5) (end 5 5) (layer "F.SilkS") (width 0.17) (tstamp 1808343c-e841-4e12-bb34-94dddca5484e))
    (fp_line (start -5 5) (end 5 5) (layer "F.SilkS") (width 0.17) (tstamp 200d1848-aaa9-4220-857f-1ccb2dc21623))
    (fp_line (start 5 -5) (end -5 -5) (layer "F.SilkS") (width 0.17) (tstamp 6172abb8-c4e1-4f59-9afa-8d1689e42385))
    (fp_line (start -5 -5) (end -5 5) (layer "F.SilkS") (width 0.17) (tstamp c7eec5d0-2432-4630-8fc2-9a4c400b428b))
    (fp_circle (center -3.75 4.5) (end -3.6 4.5) (layer "F.SilkS") (width 0.17) (fill none) (tstamp 38f7c386-dd7a-47dc-8db9-3cadae1b864b))
    (pad "1" smd rect locked (at -3.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Net-(U2-Pad1)") (pinfunction "VBAT") (pintype "power_in") (tstamp 5ed8dd09-4981-49c5-b4af-29a4d66471f5))
    (pad "2" smd rect locked (at -3.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "unconnected-(U2-Pad2)") (pinfunction "PC13") (pintype "bidirectional+no_connect") (tstamp cb047a87-3057-4c6d-ae5d-c08a3b287533))
    (pad "3" smd rect locked (at -2.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "unconnected-(U2-Pad3)") (pinfunction "PC14") (pintype "bidirectional+no_connect") (tstamp 734edf73-d4fa-480f-b065-802589ecfd26))
    (pad "4" smd rect locked (at -2.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "unconnected-(U2-Pad4)") (pinfunction "PC15") (pintype "bidirectional+no_connect") (tstamp b91304ad-4ba7-42b3-a5fb-bbc084b1f6e3))
    (pad "5" smd rect locked (at -1.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "PH0") (pintype "bidirectional") (tstamp 1e906150-54eb-49da-b947-ac127fdcde7f))
    (pad "6" smd rect locked (at -1.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "PH1") (pintype "bidirectional") (tstamp 4e0a8c58-215c-4276-84ee-1ff489097863))
    (pad "7" smd rect locked (at -0.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/nrst") (pinfunction "NRST") (pintype "bidirectional") (tstamp 08b4173d-ee2e-4107-a719-6815652aa383))
    (pad "8" smd rect locked (at -0.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "unconnected-(U2-Pad8)") (pinfunction "PC0") (pintype "bidirectional+no_connect") (tstamp c91c36ed-a9a4-45bf-94c2-82345595fd96))
    (pad "9" smd rect locked (at 0.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "unconnected-(U2-Pad9)") (pinfunction "PC1") (pintype "bidirectional+no_connect") (tstamp 66e62909-cabb-41c9-9583-cc5cb354dc55))
    (pad "10" smd rect locked (at 0.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "unconnected-(U2-Pad10)") (pinfunction "PC2") (pintype "bidirectional+no_connect") (tstamp 0120a5dc-c93a-44a1-be8d-efd68f326d98))
    (pad "11" smd rect locked (at 1.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "unconnected-(U2-Pad11)") (pinfunction "PC3") (pintype "bidirectional+no_connect") (tstamp 936e6fda-ed9d-4f96-82e8-2cf2eade69cf))
    (pad "12" smd rect locked (at 1.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSSA") (pintype "power_in") (tstamp 64352ee1-d06d-488d-8e13-7a5de73a5f20))
    (pad "13" smd rect locked (at 2.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VDDA") (pintype "power_in") (tstamp ce86b0fc-7143-4e47-b666-5cdeb021fa37))
    (pad "14" smd rect locked (at 2.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/IN0") (pinfunction "PA0") (pintype "bidirectional") (tstamp 9e25b552-c442-4cda-b322-287a96b5c315))
    (pad "15" smd rect locked (at 3.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/IN1") (pinfunction "PA1") (pintype "bidirectional") (tstamp b850fd53-5306-4d1d-b07c-10669ffc940b))
    (pad "16" smd rect locked (at 3.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/IN2") (pinfunction "PA2") (pintype "bidirectional") (tstamp 1e5854e2-fe68-4092-97f6-aaf6f127cf99))
    (pad "17" smd rect locked (at 5.75 3.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/IN3") (pinfunction "PA3") (pintype "bidirectional") (tstamp d390e0a8-4723-4e46-a7a0-f267f5792604))
    (pad "18" smd rect locked (at 5.75 3.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp 45c06b86-695b-4dea-bb48-6fc4cacb3c2f))
    (pad "19" smd rect locked (at 5.75 2.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp 8c8da501-3192-47d6-8cd4-e470a78f98b7))
    (pad "20" smd rect locked (at 5.75 2.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/IN4") (pinfunction "PA4") (pintype "bidirectional") (tstamp b3fcbbfd-9cbe-4608-828f-ccd370458fe3))
    (pad "21" smd rect locked (at 5.75 1.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "/IN5") (pinfunction "PA5") (pintype "bidirectional") (tstamp c57f5340-5233-4eb6-bad7-be19aa84a0c8))
    (pad "22" smd rect locked (at 5.75 1.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "/IN6") (pinfunction "PA6") (pintype "bidirectional") (tstamp e2be1bef-bfb9-406f-ac66-391b3c9b0ebb))
    (pad "23" smd rect locked (at 5.75 0.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "/IN7") (pinfunction "PA7") (pintype "bidirectional") (tstamp 642c339d-254d-4a10-9465-6734aa6b01f1))
    (pad "24" smd rect locked (at 5.75 0.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/230V_1_IN") (pinfunction "PC4") (pintype "bidirectional") (tstamp 734452c3-2b9a-4be1-86ef-dd8280ae2e3c))
    (pad "25" smd rect locked (at 5.75 -0.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/230V_2_IN") (pinfunction "PC5") (pintype "bidirectional") (tstamp df9b4fd8-a5b7-41af-9304-03749feafa56))
    (pad "26" smd rect locked (at 5.75 -0.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/230V_3_IN") (pinfunction "PB0") (pintype "bidirectional") (tstamp 10bbbef4-9e6c-4d6f-af2b-5796322a75b1))
    (pad "27" smd rect locked (at 5.75 -1.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/230V_4_IN") (pinfunction "PB1") (pintype "bidirectional") (tstamp 424b283b-a4ea-428f-ab38-22d7a711a650))
    (pad "28" smd rect locked (at 5.75 -1.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U2-Pad28)") (pinfunction "PB2") (pintype "bidirectional+no_connect") (tstamp ea7c5f6c-37fd-4bd5-9469-d2d1540105b7))
    (pad "29" smd rect locked (at 5.75 -2.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "/sdl") (pinfunction "PB10") (pintype "passive") (tstamp fee19157-e8aa-4a06-a7b8-53db6bd44da1))
    (pad "30" smd rect locked (at 5.75 -2.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C14-Pad1)") (pinfunction "VCAP1") (pintype "power_in") (tstamp 7b26e552-7761-47c1-a311-f80aea1d3683))
    (pad "31" smd rect locked (at 5.75 -3.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp 59b6cdae-1164-4154-8c2e-2b98853446f3))
    (pad "32" smd rect locked (at 5.75 -3.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp c8b9b926-da70-4fe4-ad60-112569d3bda6))
    (pad "33" smd rect locked (at 3.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U2-Pad33)") (pinfunction "PB12") (pintype "bidirectional+no_connect") (tstamp 0a542b22-bcc0-457a-8f5f-a728d97a52a6))
    (pad "34" smd rect locked (at 3.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U2-Pad34)") (pinfunction "PB13") (pintype "bidirectional+no_connect") (tstamp 22d967f4-e8a7-4d35-abb8-10263a7d18fa))
    (pad "35" smd rect locked (at 2.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U2-Pad35)") (pinfunction "PB14") (pintype "bidirectional+no_connect") (tstamp 1d27f690-43cb-4b3a-96fa-543125a395ad))
    (pad "36" smd rect locked (at 2.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U2-Pad36)") (pinfunction "PB15") (pintype "bidirectional+no_connect") (tstamp 3f725490-aaa3-4c98-9b12-365b95c00a7a))
    (pad "37" smd rect locked (at 1.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/Vent2_IN") (pinfunction "PC6") (pintype "bidirectional") (tstamp f496a302-07b7-444e-a66e-719e545fd787))
    (pad "38" smd rect locked (at 1.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/Vent1_IN") (pinfunction "PC7") (pintype "bidirectional") (tstamp 892a960f-3c5b-4031-b333-aa6a53a8e330))
    (pad "39" smd rect locked (at 0.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/Full_HAUT_IN") (pinfunction "PC8") (pintype "bidirectional") (tstamp 4ea6a170-cc36-41c1-b07a-d3ae26bc2ab2))
    (pad "40" smd rect locked (at 0.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/Cro_HAUT_IN") (pinfunction "PC9") (pintype "bidirectional") (tstamp c504d881-948b-49c9-a60c-a439e13c36c5))
    (pad "41" smd rect locked (at -0.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/Flo_HAUT_IN") (pinfunction "PA8") (pintype "bidirectional") (tstamp 7d6072ad-f253-492c-a6d5-82c668776e18))
    (pad "42" smd rect locked (at -0.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/Cro_BAS_IN") (pinfunction "PA9") (pintype "bidirectional") (tstamp b7da07dc-f237-455d-826e-d3cff92c1729))
    (pad "43" smd rect locked (at -1.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/Full_BAS_IN") (pinfunction "PA10") (pintype "bidirectional") (tstamp f3425168-1593-4424-aeb0-89f332072bea))
    (pad "44" smd rect locked (at -1.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/Flo_BAS_IN") (pinfunction "PA11") (pintype "bidirectional") (tstamp cfbfbec4-dba5-43b2-8e76-594ffa4eb79f))
    (pad "45" smd rect locked (at -2.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U2-Pad45)") (pinfunction "PA12") (pintype "bidirectional+no_connect") (tstamp 38cb10e1-51cf-4cb7-8162-db961607e6fd))
    (pad "46" smd rect locked (at -2.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/swdio") (pinfunction "PA13") (pintype "bidirectional") (tstamp 52181c93-2f78-429d-a392-1ef9d2360361))
    (pad "47" smd rect locked (at -3.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VDD") (pintype "power_in") (tstamp 995b51ad-d565-4cd0-a47a-bfab4909d393))
    (pad "48" smd rect locked (at -3.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VSS") (pintype "power_in") (tstamp f3f9754b-69e1-49ea-8993-eee8e1cb9cc5))
    (pad "49" smd rect locked (at -5.75 -3.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/swclk") (pinfunction "PA14") (pintype "bidirectional") (tstamp 27a6bdf3-a86d-417a-a57b-75dcedd1d3d8))
    (pad "50" smd rect locked (at -5.75 -3.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U2-Pad50)") (pinfunction "PA15") (pintype "bidirectional+no_connect") (tstamp 53eae3a5-1ed9-4fb1-bc86-66dde678e62e))
    (pad "51" smd rect locked (at -5.75 -2.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/12V_4_IN") (pinfunction "PC10") (pintype "bidirectional") (tstamp 2d1926d6-8e3a-41e1-bebd-70571993fa38))
    (pad "52" smd rect locked (at -5.75 -2.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/12V_3_IN") (pinfunction "PC11") (pintype "bidirectional") (tstamp 4c029cf5-753b-48b0-bfb9-ba8a16e3c1eb))
    (pad "53" smd rect locked (at -5.75 -1.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/12V_2_IN") (pinfunction "PC12") (pintype "bidirectional") (tstamp c4a1f62f-5cd8-4646-87b0-27b8aef7ca92))
    (pad "54" smd rect locked (at -5.75 -1.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/12V_1_IN") (pinfunction "PD2") (pintype "bidirectional") (tstamp 3db1db2a-78e2-457a-8ae5-f0ee56a7f90d))
    (pad "55" smd rect locked (at -5.75 -0.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "/sda") (pinfunction "PB3") (pintype "bidirectional") (tstamp 51c89383-a2be-4c79-b981-5ee4fe2e6e99))
    (pad "56" smd rect locked (at -5.75 -0.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(U2-Pad56)") (pinfunction "PB4") (pintype "bidirectional+no_connect") (tstamp ca4e5489-9404-4e78-9fb3-d29feec00383))
    (pad "57" smd rect locked (at -5.75 0.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(U2-Pad57)") (pinfunction "PB5") (pintype "bidirectional+no_connect") (tstamp b25aaeeb-95e3-497a-b992-6a73301b8105))
    (pad "58" smd rect locked (at -5.75 0.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/RX") (pinfunction "PB6") (pintype "bidirectional") (tstamp af3e18c3-64f1-4d64-b3ab-e70ab4d2b6f8))
    (pad "59" smd rect locked (at -5.75 1.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/TX") (pinfunction "PB7") (pintype "bidirectional") (tstamp 8afeb9cf-8111-4d69-938d-54ee2eb1fea3))
    (pad "60" smd rect locked (at -5.75 1.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/boot0") (pinfunction "BOOT0") (pintype "input") (tstamp 7846a700-ddc2-4185-b722-8f5ca7499e90))
    (pad "61" smd rect locked (at -5.75 2.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "/IN8") (pinfunction "PB8") (pintype "bidirectional") (tstamp 24fb37f8-d133-4750-8786-1188d5204248))
    (pad "62" smd rect locked (at -5.75 2.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/IN9") (pinfunction "PB9") (pintype "bidirectional") (tstamp 772f58d3-36fb-4824-9eab-ba94cdab58f8))
    (pad "63" smd rect locked (at -5.75 3.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp 7390450b-1b88-411c-b821-09c347e8faad))
    (pad "64" smd rect locked (at -5.75 3.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp a9a10a4f-1668-48c9-a530-ee158d02d6f2))
  )

  (footprint "U:LM317" (layer "F.Cu")
    (tedit 5B3F782B) (tstamp 00000000-0000-0000-0000-000061711f97)
    (at 189.595001 28.526999)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000610a57a7")
    (attr through_hole)
    (fp_text reference "U4" (at 0 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 095e9215-92de-472c-a9cc-8a8af630bd68)
    )
    (fp_text value "LM317" (at 5 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fcd7f388-7499-47b3-999e-21ee13bbf56c)
    )
    (fp_line (start -4 2.25) (end -4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp 17eecd53-94ad-40dc-a14c-9095e1d10207))
    (fp_line (start 4 2.25) (end -4 2.25) (layer "F.SilkS") (width 0.15) (tstamp 235c27e7-a430-4647-ad56-60c8b524f40c))
    (fp_line (start 4 2.25) (end 4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp 6072d557-498b-495e-bb25-16b19ebec7a5))
    (fp_line (start -4 -2.25) (end 4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp 676498df-f1b0-4363-8646-66242268987f))
    (pad "1" smd rect locked (at -2.5 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C17-Pad1)") (pinfunction "Adj") (pintype "input") (tstamp 8f98c9d2-3b17-4235-97d8-49fc91a07f38))
    (pad "2" smd rect locked (at 0 -3.25) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "Vout") (pintype "power_out") (tstamp 41285b12-f028-4e50-9285-44eaae50952e))
    (pad "2" smd rect locked (at -0.2 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/3.3V") (pinfunction "Vout") (pintype "power_out") (tstamp 9f01108f-45aa-4802-87d5-677088256cd0))
    (pad "3" smd rect locked (at 2.1 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/12V") (pinfunction "Vin") (pintype "power_in") (tstamp 053e6986-80be-4db7-a980-efea41f642f5))
  )

  (footprint "U:LM317" (layer "F.Cu")
    (tedit 5B3F782B) (tstamp 00000000-0000-0000-0000-000061711fa3)
    (at 165.025001 54.246999)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000610a7c3b")
    (attr through_hole)
    (fp_text reference "U5" (at 0 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a99c147c-c364-4702-9405-14ebe86a7de7)
    )
    (fp_text value "LM317" (at 5 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f034b99-474f-481f-a252-e1bf6042bfad)
    )
    (fp_line (start -4 2.25) (end -4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp 37944a73-d63b-44b2-a157-28ecac189828))
    (fp_line (start -4 -2.25) (end 4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp 4bdfb496-dda2-4c63-b4d3-09f266c58605))
    (fp_line (start 4 2.25) (end -4 2.25) (layer "F.SilkS") (width 0.15) (tstamp 601f5e1d-c700-4d6b-a62c-6c9978351d7c))
    (fp_line (start 4 2.25) (end 4 -2.25) (layer "F.SilkS") (width 0.15) (tstamp da176eae-825c-45bf-b2e5-90494cd740b5))
    (pad "1" smd rect locked (at -2.5 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C18-Pad1)") (pinfunction "Adj") (pintype "input") (tstamp be62c91d-d451-4a89-a28b-0ef55a839e3d))
    (pad "2" smd rect locked (at 0 -3.25) (size 3.1 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/5V") (pinfunction "Vout") (pintype "power_out") (tstamp 41b2ac46-f206-43cc-9e43-d5687f1ed2c8))
    (pad "2" smd rect locked (at -0.2 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/5V") (pinfunction "Vout") (pintype "power_out") (tstamp 46f177c0-a1bf-4379-84e5-44d06c6c4dc8))
    (pad "3" smd rect locked (at 2.1 3.25) (size 0.84 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/12V") (pinfunction "Vin") (pintype "power_in") (tstamp 9ca9c2aa-9b82-4d8d-9607-515021dc867d))
  )

  (footprint "Y:5032" (layer "F.Cu")
    (tedit 592E7CF3) (tstamp 00000000-0000-0000-0000-000061711fab)
    (at 163.65 60.59)
    (property "Partkeepr" "1650")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b53a")
    (attr through_hole)
    (fp_text reference "Y1" (at 0 2.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ce83d77-b774-4cfc-9cf2-fca5f1114890)
    )
    (fp_text value "25Mhz" (at 0 -2.15) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba9dbdb5-e97e-475e-89c7-3fa700e4a15c)
    )
    (fp_line (start -0.75 -1.25) (end 0.75 -1.25) (layer "F.SilkS") (width 0.17) (tstamp 58557546-d41a-4526-a462-795b8cfa6645))
    (fp_line (start -0.75 1.25) (end 0.75 1.25) (layer "F.SilkS") (width 0.17) (tstamp 972d7841-557f-46b6-b0d0-5a9597de621b))
    (pad "1" smd rect locked (at -1.85 0) (size 1.7 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 4fc788c9-a909-47c6-98c0-8e688c92c6bc))
    (pad "2" smd rect locked (at 1.85 0) (size 1.7 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "2") (pintype "passive") (tstamp 412e0471-aef7-4015-ba0c-e9f65b0a9654))
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp 411129e3-cd41-4e30-9c65-7ba1fa026a49)
    (at 17.5 97.5)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/ed1f49ff-a910-4a9c-88e1-d8169056078d")
    (attr through_hole)
    (fp_text reference "P15" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 9ecbadc6-6387-43bb-8da2-bbdb137e1ac5)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 94938f98-1ab8-4d09-bc59-f0f6ce32dc97)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 69e14165-80b1-4cea-883a-b6a90c6fb976))
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp a5dada40-28f0-49a2-b755-ab5c8c379bcc)
    (at 97.5 17.5)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/4fc7d59e-2928-4cf2-8aff-3697086090ef")
    (attr through_hole)
    (fp_text reference "P12" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp f558dc7e-aa76-4a56-aced-9e6e49b0f3c8)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp b2fc09cb-c388-4044-a971-b54a76f14d1d)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 2326bf53-b8c6-461a-94a7-8901123457eb))
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp abdef57b-50b4-49ef-b7ab-7785b536c9d0)
    (at 97.5 97.5)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d80e9c10-efad-42ee-b325-38c1975517c6")
    (attr through_hole)
    (fp_text reference "P13" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp ba6a75b2-7388-43fd-8d12-c296453287ba)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 021157f3-1649-4e1b-bcb6-ce89c351f65c)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 04dc15fe-351d-4cd5-a494-16b9c4d9ba6b))
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp cec9e641-a0b5-431a-b562-b9424b849301)
    (at 17.5 17.5)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d7c047b2-dcd3-4c84-bce0-f88914740f32")
    (attr through_hole)
    (fp_text reference "P14" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 284bd55f-6894-43d7-811d-afaa9623d176)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 2d25b146-06ec-47e8-865d-279412fb9cf6)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 818a7a25-aa08-4095-a38c-649539d53923))
  )

  (footprint "Jumper:Jumper3X250V" (layer "B.Cu")
    (tedit 616418B8) (tstamp 00000000-0000-0000-0000-000061711d5c)
    (at 155 100)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1d4")
    (attr through_hole)
    (fp_text reference "JP1" (at 4.5 0 270) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 968524c4-7dbd-4e74-93ef-a1968d6d3d4e)
    )
    (fp_text value "Jumper3" (at 0 -4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cebcbdd3-30da-4685-9d20-c1ebd4a82e4c)
    )
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 266806d8-3cd9-4983-a083-b7d70a168f35))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1.75 -0.75)
        (xy 1.75 0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
        (xy 3.5 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp b9229cb0-8072-46cf-b1bf-fa595c0b53cf))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp cc41728f-b6ae-42d5-b6c7-564a52f0e4f3))
    (fp_line (start 1 -3.25) (end -0.75 -3.25) (layer "B.SilkS") (width 0.12) (tstamp 0d13b315-9353-4f3b-b3b3-01049caa4f47))
    (fp_line (start 0 3.25) (end -0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 271275ea-c4ad-4100-9dab-0dc824ab65a7))
    (fp_line (start 0 3.25) (end 0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 38ccadec-3563-4c43-bc13-117d5050182b))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 12717eb8-6a9b-45e2-bcfb-30f22091f008))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp c64e4f93-a96d-4c7f-a83b-2bd6d301a129))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp e5f1c2c2-eade-42f6-a607-b97a8769204f))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 12 "/OUT_230V_3") (pintype "passive") (tstamp 65c028d0-eaeb-4f28-abb7-2c3d6a33a29e))
    (pad "2" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 14 "Net-(JP1-Pad2)") (pintype "passive") (tstamp eb7a2857-de43-4bf9-8591-71927735b268))
    (pad "3" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 13 "Net-(JP1-Pad3)") (pintype "passive") (tstamp 98a3bf5f-9e00-4d5f-94aa-ecb0d06e7ec7))
  )

  (footprint "Jumper:Jumper3X250V" (layer "B.Cu")
    (tedit 616418B8) (tstamp 00000000-0000-0000-0000-000061711d6c)
    (at 180 100)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bd08")
    (attr through_hole)
    (fp_text reference "JP2" (at 4.5 0 -90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa43eb27-0a7a-401f-9ff4-afc2f3f043a6)
    )
    (fp_text value "Jumper3" (at 0 -4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp aecb25e4-2fa0-4f3c-8c81-0e782ae068d7)
    )
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 13c876b2-1d4e-4412-b994-ffea81e407e8))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 95d0595a-460e-4bbd-b653-cb76a08212cf))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1.75 -0.75)
        (xy 1.75 0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
        (xy 3.5 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp c3acd2f1-5d6e-46b1-b498-5456205f6ad2))
    (fp_line (start 1 -3.25) (end -0.75 -3.25) (layer "B.SilkS") (width 0.12) (tstamp 2dc60916-610f-44ef-9dbc-59d888737f86))
    (fp_line (start 0 3.25) (end -0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 55878480-d764-49dc-a6fb-ef45a27cbdcc))
    (fp_line (start 0 3.25) (end 0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 86e98b2b-10f5-484c-b056-2e4566394786))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 33ba8b3b-832e-4b32-b147-9a2320f41d45))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 7c0f1a71-2789-4c11-a6db-5199c163e401))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp c51827ab-abcf-4fab-bdb8-494cc8090a02))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 15 "/OUT_230V_1") (pintype "passive") (tstamp 3b5fc7bc-beb8-4a14-a8c2-a8b760db329e))
    (pad "2" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 17 "Net-(JP2-Pad2)") (pintype "passive") (tstamp 2db4bcc0-2d45-4d64-8b8a-215b9a0102b5))
    (pad "3" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 16 "Net-(JP2-Pad3)") (pintype "passive") (tstamp de6c16aa-8351-4215-85c9-4682be7a4be4))
  )

  (footprint "Jumper:Jumper3X250V" (layer "B.Cu")
    (tedit 616418B8) (tstamp 00000000-0000-0000-0000-000061711d7c)
    (at 155 120)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d6d")
    (attr through_hole)
    (fp_text reference "JP3" (at 4.5 0 -90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f88b4d6d-2f18-4898-be19-76767326df25)
    )
    (fp_text value "Jumper3" (at 0 -4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 011d7ea6-9bc7-462b-9795-efd01957ca4c)
    )
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1.75 -0.75)
        (xy 1.75 0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
        (xy 3.5 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 05164997-7062-4704-8bec-6ec2ae2d0aa0))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp a0a78c66-6e12-41a2-b1de-3270aef06e0e))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp fb08b385-8583-41c8-a19d-1443a4ca3665))
    (fp_line (start 0 3.25) (end -0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 71798e7a-247d-4411-a46b-9b525eae4af6))
    (fp_line (start 0 3.25) (end 0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp a39472cc-c01b-48d4-a78d-025688e3a1b2))
    (fp_line (start 1 -3.25) (end -0.75 -3.25) (layer "B.SilkS") (width 0.12) (tstamp e9f54d11-a464-488b-8e5a-cd8cec533887))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 683d40e5-14a5-4f5a-b555-5a6df4ec157b))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 70cf6e6d-5457-44cf-ba40-3036ba41ebab))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp dacaac6c-d369-4600-9a5f-86c16f2cf1f2))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 18 "/OUT_230V_2") (pintype "passive") (tstamp 8dce196e-ac27-4fb4-8d97-5f9d779098da))
    (pad "2" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 20 "Net-(JP3-Pad2)") (pintype "passive") (tstamp 64cf3a4b-b8ae-47e5-8c18-ede7472107e8))
    (pad "3" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 19 "Net-(JP3-Pad3)") (pintype "passive") (tstamp d68207a0-14bb-4c6c-906b-e8e1cd74e87a))
  )

  (footprint "Jumper:Jumper3X250V" (layer "B.Cu")
    (tedit 616418B8) (tstamp 00000000-0000-0000-0000-000061711d8c)
    (at 180 120)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006172bdbb")
    (attr through_hole)
    (fp_text reference "JP4" (at 4.5 0 270) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca1bef57-8728-4b64-a79c-abae28fae63c)
    )
    (fp_text value "Jumper3" (at 0 -4.5) (layer "B.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bed2e5bb-8cc1-4bc1-b859-eb077fe87bc4)
    )
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 43d74cb4-91d2-430a-b359-67b23ebd32ac))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp 8a4a3c40-64b3-4309-a455-18daa97e153e))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1.75 -0.75)
        (xy 1.75 0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
        (xy 3.5 3.25)
      ) (layer "B.Cu") (width 0.1) (fill solid) (tstamp fd782ba5-3469-453d-a5c6-e4ec3e650fac))
    (fp_line (start 0 3.25) (end 0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp 26175bd5-16e6-4aa1-91b0-f31d85c7e838))
    (fp_line (start 1 -3.25) (end -0.75 -3.25) (layer "B.SilkS") (width 0.12) (tstamp 6b62af81-7750-48fe-9453-c52e879dfd0e))
    (fp_line (start 0 3.25) (end -0.75 3.25) (layer "B.SilkS") (width 0.12) (tstamp f55a5df2-dd8d-47ba-b535-1ce592129315))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -3.25)
        (xy -3.5 -3.25)
        (xy -3.5 -0.75)
        (xy -0.75 -0.75)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp 67e7f12c-ce5f-459a-9fc6-f20e07c6e6bb))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 0.75)
        (xy -3.5 0.75)
        (xy -3.5 3.25)
        (xy -0.75 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp bab1e127-d6ee-4b4e-bc99-db931eae7a95))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 3.5 -3.25)
        (xy 1 -3.25)
        (xy 0 -2)
        (xy 1 -0.75)
        (xy 1 0.75)
        (xy 0 2)
        (xy 1 3.25)
      ) (layer "B.Mask") (width 0.1) (fill solid) (tstamp c1849639-4f8b-4e98-af82-e2c5060ec849))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 21 "/OUT_230V_4") (pintype "passive") (tstamp b5443b16-5e12-4193-b26f-e99337ee10ad))
    (pad "2" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 23 "Net-(JP4-Pad2)") (pintype "passive") (tstamp e39c372e-4bc2-44be-bae3-657b76cb53e8))
    (pad "3" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "B.Cu" "B.Mask")
      (net 22 "Net-(JP4-Pad3)") (pintype "passive") (tstamp d35d510c-8d53-4ad2-89f1-348a59b93e3e))
  )

  (gr_line (start 15 100) (end 15 15) (layer "Edge.Cuts") (width 0.05) (tstamp 00000000-0000-0000-0000-00006171310b))
  (gr_line (start 100 100) (end 15 100) (layer "Edge.Cuts") (width 0.05) (tstamp 02025100-3fcf-475b-850b-3d973bf723e7))
  (gr_line (start 100 15) (end 100 100) (layer "Edge.Cuts") (width 0.05) (tstamp 244c0e94-8cdc-4ddd-8929-6a087c54afb1))
  (gr_line (start 15 15) (end 100 15) (layer "Edge.Cuts") (width 0.05) (tstamp b955f3ca-2912-437b-9e0d-968a6658626e))

  (segment (start 186.1 114) (end 180.5 114) (width 0.25) (layer "B.Cu") (net 22) (tstamp 3faac5c6-41c4-4e0a-9563-0d8387efe43f))
  (segment (start 180.5 114) (end 176.5 118) (width 0.25) (layer "B.Cu") (net 22) (tstamp e2419d32-0795-47ba-8e42-36625c47de05))
  (segment (start 180.5 126) (end 176.5 122) (width 0.25) (layer "B.Cu") (net 23) (tstamp 01f0cb88-970d-45ea-aad4-d39150315b2e))
  (segment (start 186.1 126) (end 180.5 126) (width 0.25) (layer "B.Cu") (net 23) (tstamp 22827d74-fa7d-4639-89d6-3c20182817a2))

)
