(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "/3.3V")
  (net 2 "/GND")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 "/nrst")
  (net 7 "/boot0")
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(D3-Pad2)")
  (net 11 "Net-(D4-Pad2)")
  (net 12 "Net-(JP1-Pad2)")
  (net 13 "Net-(JP1-Pad3)")
  (net 14 "/OUT_230V_1")
  (net 15 "Net-(JP2-Pad2)")
  (net 16 "Net-(JP2-Pad3)")
  (net 17 "/OUT_230V_2")
  (net 18 "Net-(JP3-Pad2)")
  (net 19 "Net-(JP3-Pad3)")
  (net 20 "/OUT_230V_3")
  (net 21 "Net-(JP4-Pad2)")
  (net 22 "Net-(JP4-Pad3)")
  (net 23 "/OUT_230V_4")
  (net 24 "/230V")
  (net 25 "/TX")
  (net 26 "/RX")
  (net 27 "/GPIO0")
  (net 28 "/RST")
  (net 29 "/12V")
  (net 30 "/Neutre")
  (net 31 "/LDL")
  (net 32 "/LDA")
  (net 33 "/swclk")
  (net 34 "/swdio")
  (net 35 "/OUT_12V_1")
  (net 36 "Net-(Q1-Pad1)")
  (net 37 "/OUT_12V_2")
  (net 38 "Net-(Q2-Pad1)")
  (net 39 "unconnected-(Q3-Pad2)")
  (net 40 "unconnected-(Q3-Pad3)")
  (net 41 "Net-(Q3-Pad1)")
  (net 42 "/OUT_12V_4")
  (net 43 "Net-(Q4-Pad1)")
  (net 44 "Net-(Q5-Pad1)")
  (net 45 "/Vent1")
  (net 46 "Net-(Q6-Pad1)")
  (net 47 "/Vent2")
  (net 48 "Net-(Q7-Pad1)")
  (net 49 "Net-(Q8-Pad1)")
  (net 50 "Net-(Q9-Pad1)")
  (net 51 "Net-(Q10-Pad1)")
  (net 52 "Net-(Q11-Pad1)")
  (net 53 "/Flo_HAUT")
  (net 54 "Net-(Q11-Pad3)")
  (net 55 "Net-(Q12-Pad1)")
  (net 56 "/Full_HAUT")
  (net 57 "Net-(Q12-Pad3)")
  (net 58 "Net-(Q13-Pad1)")
  (net 59 "/Cro_HAUT")
  (net 60 "Net-(Q13-Pad3)")
  (net 61 "Net-(Q14-Pad1)")
  (net 62 "/Flo_BAS")
  (net 63 "Net-(Q14-Pad3)")
  (net 64 "Net-(Q15-Pad1)")
  (net 65 "/Full_BAS")
  (net 66 "Net-(Q15-Pad3)")
  (net 67 "Net-(Q16-Pad1)")
  (net 68 "/Cro_BAS")
  (net 69 "Net-(Q16-Pad3)")
  (net 70 "Net-(R1-Pad2)")
  (net 71 "/12V_1_IN")
  (net 72 "/12V_2_IN")
  (net 73 "Net-(R6-Pad2)")
  (net 74 "/12V_3_IN")
  (net 75 "/12V_4_IN")
  (net 76 "/Vent1_IN")
  (net 77 "/Vent2_IN")
  (net 78 "/230V_1_IN")
  (net 79 "/230V_2_IN")
  (net 80 "/230V_3_IN")
  (net 81 "/230V_4_IN")
  (net 82 "/sda")
  (net 83 "/sdl")
  (net 84 "/Flo_HAUT_IN")
  (net 85 "/Full_HAUT_IN")
  (net 86 "/Cro_HAUT_IN")
  (net 87 "/Flo_BAS_IN")
  (net 88 "/Full_BAS_IN")
  (net 89 "/Cro_BAS_IN")
  (net 90 "unconnected-(U1-Pad2)")
  (net 91 "unconnected-(U1-Pad4)")
  (net 92 "unconnected-(U1-Pad5)")
  (net 93 "unconnected-(U1-Pad6)")
  (net 94 "unconnected-(U1-Pad7)")
  (net 95 "unconnected-(U1-Pad10)")
  (net 96 "unconnected-(U1-Pad11)")
  (net 97 "unconnected-(U1-Pad12)")
  (net 98 "unconnected-(U1-Pad13)")
  (net 99 "unconnected-(U1-Pad14)")
  (net 100 "unconnected-(U1-Pad19)")
  (net 101 "unconnected-(U1-Pad20)")
  (net 102 "unconnected-(U1-Pad9)")
  (net 103 "Net-(BT1-Pad1)")
  (net 104 "unconnected-(U2-Pad2)")
  (net 105 "unconnected-(U2-Pad3)")
  (net 106 "unconnected-(U2-Pad4)")
  (net 107 "unconnected-(U2-Pad8)")
  (net 108 "unconnected-(U2-Pad9)")
  (net 109 "unconnected-(U2-Pad10)")
  (net 110 "unconnected-(U2-Pad11)")
  (net 111 "/IN0")
  (net 112 "/IN1")
  (net 113 "/IN2")
  (net 114 "/IN3")
  (net 115 "/IN4")
  (net 116 "/IN5")
  (net 117 "/IN6")
  (net 118 "/IN7")
  (net 119 "unconnected-(U2-Pad28)")
  (net 120 "unconnected-(U2-Pad33)")
  (net 121 "unconnected-(U2-Pad34)")
  (net 122 "unconnected-(U2-Pad35)")
  (net 123 "unconnected-(U2-Pad36)")
  (net 124 "unconnected-(U2-Pad45)")
  (net 125 "unconnected-(U2-Pad50)")
  (net 126 "unconnected-(U2-Pad56)")
  (net 127 "unconnected-(U2-Pad57)")
  (net 128 "/IN8")
  (net 129 "/IN9")
  (net 130 "unconnected-(U3-Pad1)")
  (net 131 "unconnected-(U3-Pad5)")

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 0299c169-92ed-4f8b-9edf-89274de35d26)
    (at 131.54 35.4)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d503674d-8a68-4394-8325-8cb954a0f48a")
    (attr through_hole)
    (fp_text reference "R6" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 9b471900-2b6d-4d81-a8aa-2d7ec289786b)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d58fc875-b7fd-432c-ae30-fb7063471d96)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 13d3f43c-304f-4887-b1cf-0e14e3d5a5c2))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 62d1e8a7-cb76-4969-a1e7-74310b76ee26))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1b3c8dfd-4e0b-491f-8111-288cc8aeeb18))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(R6-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 401a05ae-c2d1-4665-a76b-dd3515e0a6ae))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 02c6f1ee-40ee-460e-8f24-95f0ee4e9d1c)
    (at 122.07 41.99)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/a58c5dcd-9403-4d7b-a266-e91987bbe42a")
    (attr through_hole)
    (fp_text reference "R1" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 6873fee1-7512-4c92-94aa-888cd35b12bb)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 3cecce9f-3c01-4b17-a2f2-231c5cdeea52)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 2e660768-e191-4649-bbf5-e0366b26cfdb))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 86955e99-c029-48dd-b3b6-b5c0b6c9dd10))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3d5cf157-8782-41c0-ac52-693f95856b00))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R1-Pad2)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp edd836e7-cc34-465a-885f-cc9663de66eb))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp 0917f905-c2e1-4bb9-8d1e-bcf04b68fd4d)
    (at 106.55 45.325)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/ed1f49ff-a910-4a9c-88e1-d8169056078d")
    (attr through_hole)
    (fp_text reference "P10" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 61abda24-528e-445e-a44d-d62fad8125cd)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp af02df5d-a09d-44f2-8b83-b9be18f2de8b)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 23a581fe-0a1a-4e85-ae2d-30440ebdb5db))
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp 0b9703d8-413d-4cdf-ae95-ffb2186d1ac7)
    (at 111.06 44.675)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250115")
    (attr through_hole)
    (fp_text reference "Q12" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp b1f4dd95-4781-427b-bcea-e45a53aba32d)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c82ded1d-b6bc-42b3-9d9b-38b8cf118da1)
    )
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 17382a3e-2a36-412e-babc-a7f07d28a2f1))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 81eaf0eb-619f-4673-b14b-fef42b9bce8d))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 85076b03-d011-467e-9eed-c45c77f16d91))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp e1cf8d42-fc44-4b46-87c4-898ce570171c))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(Q12-Pad1)") (pintype "input") (tstamp eadd013e-1ac5-4fa5-b5de-eba035704bc0))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/Full_HAUT") (pintype "input") (tstamp 9d52d11e-daf7-49c5-bcd1-0437a2764964))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(Q12-Pad3)") (pintype "input") (tstamp a97e79f7-5643-44f2-be3a-134250da223a))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 0cf76c98-54ee-4708-a65f-5a793ec8cc9f)
    (at 114.87 48.51)
    (property "Partkeepr" "0607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b57b")
    (attr through_hole)
    (fp_text reference "C7" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 9ec608ae-d9ed-4b96-90cf-3780a111323d)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 92604a17-db94-4e40-8f26-7aab9dce1438)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 2ccb4fbe-060d-4524-9e85-c77ab87d122f))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp c0125466-ad8b-4e8e-95b0-89fec9f38e81))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C7-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6ee9d469-2bfe-4b37-b9f2-1f097c18d9dc))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 87999fe6-b1df-4b4a-9c75-f38075faae22))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 0e7958c9-8f23-48fc-a9bc-bac57f6d6c2e)
    (at 124.34 33.98)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125012f")
    (attr through_hole)
    (fp_text reference "R17" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 84b0ac3f-f897-48c7-bf84-44613fea17dd)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 888e5c0f-fbbb-4ccb-b276-5faa1516fc9e)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 2b34470c-4321-4960-9f0e-d438c877b60f))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 732c1bae-2082-462a-a4ed-04a57fae012a))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 4a686404-284d-4d82-9955-de4283674ee9))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(Q13-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 176e74bf-426c-4ed1-bd2f-e3cfdbc70e40))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 10f7693a-45f3-46fa-9597-832c454b0d28)
    (at 124.34 36.65)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1ad")
    (attr through_hole)
    (fp_text reference "R13" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp d43ec5d2-8d8c-45f1-87bd-2cb58a7d45cd)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 24c0fe4a-e10a-47bb-884f-68467a1a95e7)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp a9490ec2-6881-4e4b-ae72-163d0e5b4c0d))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp d5dc9b43-0c7d-4d08-81a9-9824b0124fc3))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(Q9-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 113e1997-5119-401b-8442-6813308da7ff))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/230V_3_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 0b97abe6-ef9b-47b2-81bf-e31f4a60c516))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 13919a35-28d3-4ba6-b15c-0bd01183111f)
    (at 127.94 33)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061829ada")
    (attr through_hole)
    (fp_text reference "R4" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 804bc79e-88ab-4e88-998c-4d14983e3ce3)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 83508a4c-f954-48ff-a1a1-cbf85eeba6eb)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 6559811a-225a-4be0-918b-524758322e41))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp b855dece-8e03-4e58-b0e4-6632b5c3cbec))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(Q2-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 4fe6107e-f821-4ba0-8be2-2e6880d13d57))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/12V_2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 35cb4b51-06eb-4d90-8012-1f773d148e8e))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 14a252b7-2b6f-4262-b546-888e4109a6d9)
    (at 127.94 38.32)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125011b")
    (attr through_hole)
    (fp_text reference "R16" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 0381381f-cae5-48f8-94dc-45b7b69c1f81)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 1d5d936d-856d-454c-9cea-8eb19f1988f8)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp b3462c7b-43e4-4f0c-9fe2-bee49e21e4c2))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp c10e68ca-12aa-4340-8f25-70677fa65ab5))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9d588f62-e4ec-4de7-b9f7-c9f75a91c96a))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(Q12-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp aa9c0581-a779-4201-a572-0b34e059c9c0))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 1b002893-856d-44a2-81fa-156d85bf2b5f)
    (at 112.1 54.23)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611b9a4d")
    (attr through_hole)
    (fp_text reference "R10" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 970351e0-25d4-411e-ac7f-fcf56d635243)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 18c3651a-6e1d-4afb-b52f-f2797c230e02)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 27471980-2784-4828-bbb3-bb637411fa46))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 80f23266-fd33-46ba-9843-bcbc58360349))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(Q6-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 5ea0ae1b-8b81-422d-9894-9b095167662d))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/Vent2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 392ed931-d989-46bc-9a5c-965996b76e74))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 1de923e4-c6f8-4b0d-a093-1fcef28e6176)
    (at 118.47 48.5)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250107")
    (attr through_hole)
    (fp_text reference "R15" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp c31fed29-bb8e-4f06-8e77-6014bf6c3acc)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 095cf4b8-207b-4413-b464-8deb19deedf5)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp e7d63d78-d638-4343-b659-6472c5647102))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp f375c8a3-e33c-419e-83b1-8deb9023f0f0))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 09974af4-4882-457b-83f4-74dd715b8a81))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(Q11-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6936b167-2c41-43d4-b715-a25e690c9cf7))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp 1e274faf-7cb6-49f1-906c-767d7002389d)
    (at 95.96 57.745)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250129")
    (attr through_hole)
    (fp_text reference "Q13" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp b6b86140-2ffb-461a-9a21-ae49e952c471)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c8ca9494-d919-4209-95d7-89929e90e280)
    )
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 2ed7109e-64d8-4d0a-897e-10c798e2ed1e))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 7492c449-2c48-4e53-912f-46e6b1e7926c))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 95db3f55-dfe9-4463-8914-60e75323d7b5))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp eab582e9-96b8-48f3-9e61-eca690334440))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(Q13-Pad1)") (pintype "input") (tstamp cd36af12-83da-49c2-9c76-21b3c82044e8))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/Cro_HAUT") (pintype "input") (tstamp 7990d2b6-0e86-4b6d-8eca-0350d00a8d2b))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(Q13-Pad3)") (pintype "input") (tstamp aac73141-017a-40cb-a5df-f931489c4ced))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Bornier:Bornier2.54_1x4" (layer "F.Cu")
    (tedit 5B3CCB63) (tstamp 2336244d-5d03-4552-a8b5-a67934e90a96)
    (at 62.865 75.59)
    (property "Partkeepr" "0006")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006149f313")
    (attr through_hole)
    (fp_text reference "P15" (at -6.096 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 27387f34-f63f-4b22-9a8d-237c89025346)
    )
    (fp_text value "Humid" (at 0 -3.81) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9cf0e7c9-66a6-4f15-9a3f-6d15f9d60822)
    )
    (fp_line (start -5.31 -2.95) (end -5.31 3.35) (layer "F.SilkS") (width 0.15) (tstamp 03ff2e31-b21c-4a18-ac72-855f2c8f6667))
    (fp_line (start 5.31 -2.95) (end 5.31 3.35) (layer "F.SilkS") (width 0.15) (tstamp 1408ba83-d443-4f92-b401-c3987b751ba6))
    (fp_line (start -5.31 3.35) (end 5.31 3.35) (layer "F.SilkS") (width 0.15) (tstamp 924721e0-bcea-4c2b-a7e3-ed7dbb354112))
    (fp_line (start -5.31 -2.95) (end 5.31 -2.95) (layer "F.SilkS") (width 0.15) (tstamp d6afd154-0781-4bfc-a936-80c1b33faf7a))
    (fp_line (start 5.31 2.54) (end -5.31 2.54) (layer "F.SilkS") (width 0.15) (tstamp da19bd46-a73f-4c36-a5da-e010ae07a3ab))
    (pad "1" thru_hole rect (at -3.81 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "/3.3V") (pinfunction "P1") (pintype "passive") (tstamp 0aa80c50-9acf-46bf-bf3e-3a057f51c58e))
    (pad "2" thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask "F.SilkS")
      (net 31 "/LDL") (pinfunction "P2") (pintype "passive") (tstamp 0b9e4e05-72ab-4c4e-a282-f70cf7582c98))
    (pad "3" thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask "F.SilkS")
      (net 32 "/LDA") (pinfunction "P3") (pintype "passive") (tstamp 4da7cc36-7109-4f11-9720-1d286a8f03bf))
    (pad "4" thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "/GND") (pinfunction "P4") (pintype "passive") (tstamp 99e7f3d4-cfca-466d-abf0-e39ed3f05ac0))
    (model "${MY_PATH}/3D/Bornier.3dshapes/Bornier2.54_1x4.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 61B9B972) (tstamp 2461b847-1bf2-4139-9a04-c1058f8c75fe)
    (at 71.395 33.36)
    (property "Partkeepr" "0350")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa9a")
    (attr through_hole)
    (fp_text reference "K4" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp d05dc10f-0e01-4547-bb43-c04090683ef0)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp f54cf59a-0047-405a-8d34-7ec65e192ab2)
    )
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 391a07db-17a4-41bb-9416-8ff4844cec8a))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 6bc1dcd8-eb84-4f5e-8dfa-fc312c76d419))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp bada59b6-dcbc-456d-be4d-dca08f95bb91))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp fe932519-d8d0-453a-9439-05ff0807f46a))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 11 "Net-(D4-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 322294fe-6fb1-4e17-932d-44a47ad36c14))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp f238d0c5-93ce-4154-a984-0191c45a5479))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 24 "/230V") (pinfunction "COM") (pintype "input") (tstamp 24fafd78-1d6a-4f31-b202-b7ca8d150008))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 21 "Net-(JP4-Pad2)") (pinfunction "NO") (pintype "input") (tstamp a5f83a0b-488f-48ac-aafa-ca1258e2deb6))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 22 "Net-(JP4-Pad3)") (pinfunction "NC") (pintype "input") (tstamp d380b89f-301a-4527-b4af-bebb3eeafffb))
    (model "${MY_PATH}/3D/relay.3dshapes/SRD-XXVDC-SL-C.step"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 2a5184b5-2caa-4ab4-911e-f2ec076a4727)
    (at 92.35 67.09)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b4f0")
    (attr through_hole)
    (fp_text reference "R26" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp d9fb7c4e-101f-47e4-bca9-d82c953d9884)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 95a33d5a-3979-452b-a39c-506a12fff825)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 4db20a3f-c403-48f9-ac0e-3cde08d3e492))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp a1b8b6d9-edfb-409c-8b88-e38bfb1e8ad7))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 32cf9e1c-48e0-48e5-a412-ead1a04edd2b))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/boot0") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d86f1a58-fbd0-444f-adfd-fe4e84b92559))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 61B9B972) (tstamp 2c10fb11-e860-4475-84cb-80ad166e8ab3)
    (at 73.665 50.03)
    (property "Partkeepr" "0350")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1ce")
    (attr through_hole)
    (fp_text reference "K3" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 11c5c684-6bbc-4b2e-8f26-45380e0d2ac6)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp c0bc8363-d5bf-44a4-ab0a-d0b15a34ee9d)
    )
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 25f598b8-6cf1-455f-b551-06cc30d2c977))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 7e35c13b-2e92-461e-9d5d-ec4bc68f23bd))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 86daf07a-d107-4def-9f56-aa3067b3b14a))
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp cf815586-14d6-4e08-a5fc-6cd3b1e95971))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 10 "Net-(D3-Pad2)") (pinfunction "A1") (pintype "input") (tstamp 8008a459-7ba1-452c-ad3d-d24ca12f052c))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp 9b0e06ad-7a67-4f15-9f86-46a9b2b1bc08))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 24 "/230V") (pinfunction "COM") (pintype "input") (tstamp 8eed6b7b-ecda-415c-969f-04fa57f5a4de))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 18 "Net-(JP3-Pad2)") (pinfunction "NO") (pintype "input") (tstamp d573781a-21a5-4bcf-ae6e-da8b320c27ed))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 19 "Net-(JP3-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 0d5bee32-05c6-4801-9187-9bb4fbd52f60))
    (model "${MY_PATH}/3D/relay.3dshapes/SRD-XXVDC-SL-C.step"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 316e2ad2-7229-4ff8-99dc-0e46e204214a)
    (at 93.65 72.61)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/f1abc8eb-b52d-43d8-9d1d-08719d139daa")
    (attr through_hole)
    (fp_text reference "C6" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 3b43bad9-aa8a-4e0a-91bf-7eafc561cecf)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 2a84048e-0240-479b-8e30-2afcc13ab69c)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 27bf764d-a376-4b4c-8653-b55c02507e17))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 5b08ef35-1368-4ee2-92cf-f61ef322bf0b))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 26522ce7-8b9a-4ba2-8d55-67aadbe4f654))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3485bd92-13a6-4a38-9301-ae889d74218d))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp 328432fd-9180-4eda-838d-a0764b9f7678)
    (at 125.94 29.815)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250101")
    (attr through_hole)
    (fp_text reference "Q11" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 1eecaca0-5386-4a60-8211-7271ff254fbf)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ac5c11b-e5a1-48f6-a5d0-15e0c5346bb6)
    )
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 1b034fdf-9b85-41c3-a793-ef0418041bc7))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 40ffe08c-c1e0-4881-91bd-0c1ca396923d))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 8107f8e2-7abe-477a-8502-40c981d4888b))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp af00174f-1829-4e8d-addf-645d46d6400d))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(Q11-Pad1)") (pintype "input") (tstamp f47a53ef-f05a-4bff-ab5e-956611200d43))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/Flo_HAUT") (pintype "input") (tstamp 3f6ac61e-dc3f-4a5d-a739-3e9136e24ef1))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(Q11-Pad3)") (pintype "input") (tstamp d2721383-74e4-4733-9952-16627510b060))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 35bc5c7e-b246-4ca8-b315-3b9b125790f8)
    (at 86.45 73.46)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b501")
    (attr through_hole)
    (fp_text reference "R25" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 7638611f-12d7-49cc-a62a-2d2c1c3439e3)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e4ce440f-47d0-4d96-ac03-9c483fc31a33)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 6f031aa9-0f95-4527-be38-7d3d158f8dd0))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp bc962300-64ff-49ec-922d-87e667242925))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9fb264a6-5404-495e-a22e-11475bd930b2))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/nrst") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 504d1f07-fb1b-4a31-9175-b3945efa2bcf))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 36194c71-a829-41d7-938f-067004cbefb9)
    (at 136.95 29.03)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654ea")
    (attr through_hole)
    (fp_text reference "R32" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 8927b3d5-72db-49f3-a5b0-0c9ac98ba234)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp e1f21418-cc3d-4d99-b929-b84bfe3f9bd7)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp a3799b0a-c03a-4e55-b85c-0e805a1c252a))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp eb7d5d23-4134-40a1-b76c-219186f1abfd))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/Cro_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9599eaf9-370b-4a0a-b019-e495cb83592b))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(Q16-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp e7164870-cc9e-43b0-9de8-485e2f9678e6))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 3810f8c4-ef2d-4483-9b92-9db519a91ab7)
    (at 99.77 60.92)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b559")
    (attr through_hole)
    (fp_text reference "C14" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 33b34987-0c26-4174-96a4-12f46b2eb494)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 2474c688-063c-47ae-a538-0c0341165918)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 1d372a00-d2ed-4cb2-97a4-caf6eac74783))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 1e939e55-9878-4e1f-93cc-aeeb38defb51))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8c2a1d06-dc83-482f-947a-f93de3182a3e))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 61eedd4b-8b15-4f19-8c56-7edc4acaa8ab))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 61B9B972) (tstamp 3b179a10-c3c0-4a36-8d94-c93e5d434963)
    (at 53.395 58.83)
    (property "Partkeepr" "0350")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bd02")
    (attr through_hole)
    (fp_text reference "K1" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 5d8ce756-f534-4ac7-bba4-cf087d8cbfcd)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp e13e8b7e-12a3-45bb-834b-f3f04917ffd0)
    )
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 2bc775ae-1eec-4918-9f0b-c43b9a4c5c65))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 2e259ce7-3ef8-47fe-a3b2-6f65822cd5f0))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 30716a5f-0aa6-4f1f-9db4-2bc4e8bb09fe))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp a2c41daa-81f6-4ae6-90fa-c6a37aceada6))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)") (pinfunction "A1") (pintype "input") (tstamp d47e4ced-1d12-4844-8769-4fd0de1fc330))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp 6f12b4ed-5615-4aac-8141-2a51c99c3d8b))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 24 "/230V") (pinfunction "COM") (pintype "input") (tstamp 35f1b7b6-ec1f-420c-99de-ad3f22106845))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 12 "Net-(JP1-Pad2)") (pinfunction "NO") (pintype "input") (tstamp f4df62c9-789f-49c8-bd52-de4f13579d99))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 4dcaccaa-9b70-4dfb-a96d-4b181101a404))
    (model "${MY_PATH}/3D/relay.3dshapes/SRD-XXVDC-SL-C.step"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 3be08a5f-0ad3-4c14-b926-54fd9213d3b3)
    (at 104.9 55.52)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b526")
    (attr through_hole)
    (fp_text reference "C9" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 936d3cb3-3da3-43b4-beea-0d0564be2fac)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp f7cf9240-ca29-4cf3-9ced-485062f30cdf)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 8fe23727-4f11-4747-8ac4-78d87dc2ebc9))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp ca413dee-0123-4172-99ef-3eef26792923))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3955c6a5-6f8c-41a5-a5e2-53d97b2dcab0))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp eb721b89-da67-4ce3-b149-8b1b698735a1))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 3f9e8570-65ef-4439-859d-041c56155127)
    (at 112.1 51.56)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/93bccfe8-37fc-4057-b60e-b7fbdc320720")
    (attr through_hole)
    (fp_text reference "R20" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b5f35777-b961-41eb-a6f2-da1746da6e56)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 067e3fb4-b330-4ae4-bc80-37a8eb8d3856)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 7fcddbea-29f0-41de-9d68-a619a666d9e3))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp e13b1652-38c9-4c8d-90fa-14de8c800b0c))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 271741ff-b243-4247-a69f-32fb087e6750))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/sda") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 067c2a68-2c56-4f40-8b77-fd8d16fa060b))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT-223" (layer "F.Cu")
    (tedit 61B9BBA8) (tstamp 52dc2a56-bedb-400a-99f9-dca74107ce02)
    (at 80.94 70.585)
    (property "Partkeepr" "2004")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/0e4f29ea-a17c-47cf-a5c4-43aaee5fa749")
    (attr through_hole)
    (fp_text reference "Q1" (at 4.5 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e77b06d2-a839-4092-8a33-d34b0373301f)
    )
    (fp_text value "IRLL2705" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp a364a323-cb42-43cb-a260-dcc667e7b321)
    )
    (fp_line (start 3.15 -1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 141f6901-6782-4225-b095-27705b7e1370))
    (fp_line (start -3.15 -1.75) (end -3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 21501221-368d-4121-b93d-f1fc68982034))
    (fp_line (start -3.15 -1.75) (end 3.15 -1.75) (layer "F.SilkS") (width 0.12) (tstamp 9cf34e1e-4d3d-4987-8d85-ce72ad6611c2))
    (fp_line (start -3.15 1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp af4aeca4-fc6b-4622-b71e-0387243bbe65))
    (pad "1" smd rect locked (at -2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input") (tstamp 26f49f4c-7c11-49cf-a316-899c777179de))
    (pad "2" smd rect locked (at 0 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/OUT_12V_1") (pinfunction "D") (pintype "input") (tstamp 1265cbf7-48dc-49d0-a812-1311c7725aa8))
    (pad "2" smd rect locked (at 0 -3.25) (size 4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/OUT_12V_1") (pinfunction "D") (pintype "input") (tstamp f4588403-6cd5-4f9f-ab03-e15e5dcafe57))
    (pad "3" smd rect locked (at 2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "S") (pintype "input") (tstamp eb4ca951-0fb5-44d4-9219-203c1ee7f766))
    (model "${MY_PATH}/3D/U.3dshapes/SOT-223.step"
      (offset (xyz -0.35 -11.5 -8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 5430d127-f437-49e2-8e3e-35d5756c499f)
    (at 114.87 45.85)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bce1")
    (attr through_hole)
    (fp_text reference "R11" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b3081ad9-fbb5-4bd5-b69f-88dac2672b39)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 9ed13c7c-eca5-4d2b-80bd-7bd8d576b641)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 3811db83-ba6e-4dcb-a2a9-c58ddcd878dd))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp fa7baff5-c466-4df2-a1d3-98ebe9d8713c))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(Q7-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ca00c944-f734-4a4a-a805-860c86e7e170))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/230V_1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 5215af6c-7ad1-4500-91c9-98f1c9903cf4))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 54e2eda1-fe09-40d8-9946-bf827bb8e701)
    (at 108.5 55.5)
    (property "Partkeepr" "0607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/6ee18453-e24f-4380-85f0-aee1d5d207a4")
    (attr through_hole)
    (fp_text reference "C1" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp aab39220-8a24-47f2-a4f4-706787b3aa99)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 961d4f0a-cfca-435b-95dc-cdce4df5413b)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp aa31ebaa-cf21-4fbc-a02f-339ad7310a71))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp e9fc7e9f-38e6-4136-8216-60ded93d5aae))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 217f7a40-5c82-44f5-bd62-ca4aa71cddfa))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 632b9235-1ead-4e7a-9e1b-662edfd563e3))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SOD-123" (layer "F.Cu")
    (tedit 61B9B30C) (tstamp 55470b47-e596-4a7c-a7ee-16f2d4ae5265)
    (at 60.34 68.725)
    (property "Partkeepr" "1300")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bcfa")
    (attr through_hole)
    (fp_text reference "D1" (at 0 1.6) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 617c8514-a9c3-44fc-9dda-a7ba3ec2924d)
    )
    (fp_text value "1N4148W" (at 0 -0.0127) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
      (tstamp 964b577f-9a5e-40c6-9726-210f2a59616d)
    )
    (fp_line (start -2.6 -1) (end -2.6 -0.6) (layer "F.SilkS") (width 0.12) (tstamp 16c1413f-4b87-4276-874a-bfa2e0b02ec4))
    (fp_line (start -2.8 -0.8) (end -2.4 -0.8) (layer "F.SilkS") (width 0.12) (tstamp 7a622b0e-6811-42bf-be56-a135285bc1f9))
    (fp_line (start 1.08 -0.8) (end 1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp dae289dc-24de-4c0e-abef-d5a8724ffc95))
    (fp_line (start 1.905 -0.762) (end 2.159 -0.762) (layer "F.SilkS") (width 0.17) (tstamp f4f88f07-6297-4264-9fda-e4f5758d1017))
    (fp_line (start -1.08 -0.8) (end -1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp f84428eb-2758-421e-9eeb-589cd91d99d9))
    (pad "1" smd rect locked (at -1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "K") (pintype "passive") (tstamp e55f760e-6276-4658-a902-08692d558701))
    (pad "2" smd rect locked (at 1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp dadc6f07-07b3-4fe0-9f43-504ada73e077))
    (model "${MY_PATH}/3D/D.3dshapes/SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 5601623d-ad21-4a66-9efe-9189b0f44881)
    (at 95.95 67.29)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b56b")
    (attr through_hole)
    (fp_text reference "C11" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 0a6e9674-40f8-410f-897f-d9edbf74563d)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d575fbfd-c7d0-4c60-85e0-0248df41de02)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 06e23baf-04ff-4912-85bc-f144d5eea85a))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp a7e9d643-82aa-4464-9494-d2bc4710963e))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8c5d4fe7-9d16-43e4-968c-ce0ea99c1c79))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c05a6c42-4c58-4dfd-8737-128e6048b5fa))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp 56d5e0b2-38fc-4028-9245-86dc9141b3ac)
    (at 99.98 57.745)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/cb89690f-d8ef-4d2f-9046-55f7fc612f2c")
    (attr through_hole)
    (fp_text reference "Q5" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 6f0c4931-c6b0-4136-803a-a05c16588599)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7edcfdca-4f9a-4771-a91b-485dd1d967be)
    )
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 0aa1408d-5dc3-45be-bc36-a9718c25627c))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 19dfde0d-8106-4707-8f68-ffd8192c10fe))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp e57e9730-c5f9-44af-906b-184e229a4c2a))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp e71c07f4-64ef-4851-a69a-b3cad42db683))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(Q5-Pad1)") (pintype "input") (tstamp 57b11d64-f6f4-4e54-b1d5-18532a110d10))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "input") (tstamp 8d3fa2ee-d7d3-4583-b3f6-5548fb572cdd))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/Vent1") (pintype "input") (tstamp 35d5e73e-655d-4b12-b01c-d4f449236339))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 57dc6237-6d06-49bf-bf89-919e6b908437)
    (at 124.34 39.32)
    (property "Champ4" "0931")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/65ed4be8-35ec-4ef4-9d14-85bd6eab983b")
    (attr through_hole)
    (fp_text reference "R19" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 54fc90a1-1057-4d89-8f88-4ce416fd4d99)
    )
    (fp_text value "4.7K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 66ebc8d9-f915-47ef-aee5-cb9147dacf4a)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 56986602-7cf3-42d5-8951-0a01219646c5))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp bbc224b1-b290-4b75-90c4-4ad6376bff47))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp fbd81db6-7e1a-43d5-8df9-c1e59f873212))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/LDA") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 5ac3c5df-18c4-4941-860d-b9fd95258d24))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT-223" (layer "F.Cu")
    (tedit 61B9BBA8) (tstamp 5d42b238-5a9d-4e55-9900-c26918fcaad4)
    (at 100.34 46.295)
    (property "Partkeepr" "2004")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/a91007b9-0549-4dcc-abe3-72ebff7ca76c")
    (attr through_hole)
    (fp_text reference "Q2" (at 4.5 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed813a01-d34d-4d4a-902b-2d2b16d9060b)
    )
    (fp_text value "IRLL2705" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 7187491c-eb3e-429f-bd74-bee7f4b329c4)
    )
    (fp_line (start -3.15 -1.75) (end 3.15 -1.75) (layer "F.SilkS") (width 0.12) (tstamp 18b95486-30d2-41d9-9086-37648fec26e6))
    (fp_line (start 3.15 -1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 21e7f9eb-a2a3-4221-acab-ed5c13ed7f6c))
    (fp_line (start -3.15 -1.75) (end -3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp ad98476f-fd36-47ec-b971-49bc501ec2b7))
    (fp_line (start -3.15 1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp f084a60c-6aa7-48a7-b911-bf4cfa8e8f74))
    (pad "1" smd rect locked (at -2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(Q2-Pad1)") (pinfunction "G") (pintype "input") (tstamp 2ffc08f2-f337-45bf-8693-1eb8a6f7f6a8))
    (pad "2" smd rect locked (at 0 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/OUT_12V_2") (pinfunction "D") (pintype "input") (tstamp 492b996d-69f3-4ae1-a532-74d10715145b))
    (pad "2" smd rect locked (at 0 -3.25) (size 4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/OUT_12V_2") (pinfunction "D") (pintype "input") (tstamp 94b373ad-527d-4298-8bc6-d3db49b24ffe))
    (pad "3" smd rect locked (at 2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "S") (pintype "input") (tstamp 0f8730f8-6236-46f2-9619-da19e55cdcf0))
    (model "${MY_PATH}/3D/U.3dshapes/SOT-223.step"
      (offset (xyz -0.35 -11.5 -8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "relay:SRD-XXVDC-SL-C" (layer "F.Cu")
    (tedit 61B9B972) (tstamp 5f6f0941-d53c-451f-8756-7c76febc0434)
    (at 91.665 33.36)
    (property "Partkeepr" "0350")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d67")
    (attr through_hole)
    (fp_text reference "K2" (at 8 8.5) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 61db4e1b-21cc-4e23-a8ba-e189c7f787a2)
    )
    (fp_text value "SRD-03VDC-SL-C" (at -10.5 0 90) (layer "F.Fab")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 6ab9ba5d-d99b-417a-af98-50006ad25f74)
    )
    (fp_line (start -9.55 -7.75) (end 9.55 -7.75) (layer "F.SilkS") (width 0.17) (tstamp 2d461733-b048-4049-9fb7-c4b7d069c061))
    (fp_line (start 9.55 -7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 390cf7aa-cee2-4140-97c4-41d90d0767e7))
    (fp_line (start -9.55 -7.75) (end -9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 6cd38023-59f1-422b-b6e8-7d13f7e2db9e))
    (fp_line (start -9.55 7.75) (end 9.55 7.75) (layer "F.SilkS") (width 0.17) (tstamp 74c1fe4e-cb10-4d3b-85e4-aab7ac5254b6))
    (pad "1" thru_hole circle locked (at -6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)") (pinfunction "A1") (pintype "input") (tstamp b1ff857f-779f-4078-8180-94076b8e8ed6))
    (pad "2" thru_hole circle locked (at -6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 "/3.3V") (pinfunction "A2") (pintype "input") (tstamp fa81e67d-3547-4dcb-97ce-06dc6cfce056))
    (pad "3" thru_hole circle locked (at -7.5 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 24 "/230V") (pinfunction "COM") (pintype "input") (tstamp 674f17bf-c2e3-45d2-9875-616ba15175cc))
    (pad "4" thru_hole circle locked (at 6.1 6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad2)") (pinfunction "NO") (pintype "input") (tstamp 03ce43a8-7d9d-4e74-9f60-0caef4d6573a))
    (pad "5" thru_hole circle locked (at 6.1 -6) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask)
      (net 16 "Net-(JP2-Pad3)") (pinfunction "NC") (pintype "input") (tstamp 850b0b45-f4af-4239-9adc-5dad86d6efc5))
    (model "${MY_PATH}/3D/relay.3dshapes/SRD-XXVDC-SL-C.step"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 6512d2c9-075a-49bc-b8c6-2555dfc2d576)
    (at 85.72 79.19)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608b4")
    (attr through_hole)
    (fp_text reference "R28" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b25101fb-46b3-4557-b355-89a15f3ea9ee)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 04ff5195-971b-4a68-95ef-6253e493fda6)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 98402c99-3983-4a55-a3e3-b34d45db7cdb))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp d5ee4152-5cd2-47cc-a4b4-0fd91c5d6c79))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ea8a21f7-da85-4f18-97fc-d04e20064c3e))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(Q15-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1ae2b47c-5ba2-41f8-8cd0-a39169355afd))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 6576a16b-a164-47f8-8455-ff2cb1d8e071)
    (at 99.77 63.57)
    (property "Partkeepr" "606")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b574")
    (attr through_hole)
    (fp_text reference "C10" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp b164be95-7094-4e09-aa1c-c6a7890aac39)
    )
    (fp_text value "1µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 6d69a7cd-7fe7-4bcd-ad48-6abf81f5085b)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 1fb4a958-104d-46af-a7bf-4640fd1670d6))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 6ae9f79f-1be6-4b84-8f49-b29542937673))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 94db5251-4cb3-4b0f-ab92-a388f36f1063))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8750f1fb-45e8-4867-9f08-899fdd69e47c))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:LQFP64" (layer "F.Cu")
    (tedit 61B9BA88) (tstamp 66bad858-2f50-4030-9b51-007ae7b23245)
    (at 70.38 65.215)
    (property "Partkeepr" "2102")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b52f")
    (attr through_hole)
    (fp_text reference "U2" (at 6.8 5.8) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 7672e82f-bb66-40cc-adb5-3452fc793a61)
    )
    (fp_text value "STM32F401RC" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f634b8b6-1dfa-48cc-bc4d-c51e16ef90fa)
    )
    (fp_line (start 5 -5) (end 5 5) (layer "F.SilkS") (width 0.17) (tstamp 030efd5c-2c98-4a6b-86e7-fbd91f1c8724))
    (fp_line (start 5 -5) (end -5 -5) (layer "F.SilkS") (width 0.17) (tstamp 725d2b55-b723-4104-82f2-ecf1a7b35ba4))
    (fp_line (start -5 5) (end 5 5) (layer "F.SilkS") (width 0.17) (tstamp 77c1b200-5244-4e98-a1ea-b3fcae7f7cf4))
    (fp_line (start -5 -5) (end -5 5) (layer "F.SilkS") (width 0.17) (tstamp ae40c385-4ba2-4e0b-b387-3c622c9f3f86))
    (fp_circle (center -3.75 4.5) (end -3.6 4.5) (layer "F.SilkS") (width 0.17) (fill none) (tstamp 96d2f13e-85f2-4781-899e-a93e329a1567))
    (pad "1" smd rect locked (at -3.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(BT1-Pad1)") (pinfunction "VBAT") (pintype "power_in") (tstamp d121e033-9beb-452c-a583-fe74ddb2693d))
    (pad "2" smd rect locked (at -3.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U2-Pad2)") (pinfunction "PC13") (pintype "bidirectional+no_connect") (tstamp bdfc470b-c3e6-41bc-a4e4-7192d722171f))
    (pad "3" smd rect locked (at -2.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "unconnected-(U2-Pad3)") (pinfunction "PC14") (pintype "bidirectional+no_connect") (tstamp 743162c2-4412-4f39-8d75-4e5837a6ff13))
    (pad "4" smd rect locked (at -2.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U2-Pad4)") (pinfunction "PC15") (pintype "bidirectional+no_connect") (tstamp 57a7e5bb-2ac6-4d7d-8dc6-06259db7e412))
    (pad "5" smd rect locked (at -1.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad1)") (pinfunction "PH0") (pintype "bidirectional") (tstamp c005580e-a6d8-4187-9144-91f9a099fb7c))
    (pad "6" smd rect locked (at -1.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C4-Pad1)") (pinfunction "PH1") (pintype "bidirectional") (tstamp cadc8325-0c15-44e6-bf30-b8b5156dcb9e))
    (pad "7" smd rect locked (at -0.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/nrst") (pinfunction "NRST") (pintype "bidirectional") (tstamp 81e2fa35-bb36-4f6e-90d9-cbd5b247eacd))
    (pad "8" smd rect locked (at -0.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "unconnected-(U2-Pad8)") (pinfunction "PC0") (pintype "bidirectional+no_connect") (tstamp 91bd325b-4340-42bf-9382-174f9f026895))
    (pad "9" smd rect locked (at 0.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "unconnected-(U2-Pad9)") (pinfunction "PC1") (pintype "bidirectional+no_connect") (tstamp dceeff2e-d0fc-46fe-af52-9b41914d766f))
    (pad "10" smd rect locked (at 0.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "unconnected-(U2-Pad10)") (pinfunction "PC2") (pintype "bidirectional+no_connect") (tstamp c0159431-b277-4124-9e81-13d49f7bac2e))
    (pad "11" smd rect locked (at 1.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "unconnected-(U2-Pad11)") (pinfunction "PC3") (pintype "bidirectional+no_connect") (tstamp bec977aa-3094-4375-b357-3b7a8e29e1c0))
    (pad "12" smd rect locked (at 1.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSSA") (pintype "power_in") (tstamp 26d16da2-7afc-4bb4-b941-6cc90ce236f9))
    (pad "13" smd rect locked (at 2.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VDDA") (pintype "power_in") (tstamp d9092b0a-e217-4114-9955-b6c0f1da7a0f))
    (pad "14" smd rect locked (at 2.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/IN0") (pinfunction "PA0") (pintype "bidirectional") (tstamp 45561a2a-084b-4c07-b34f-1f97464dcb92))
    (pad "15" smd rect locked (at 3.25 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/IN1") (pinfunction "PA1") (pintype "bidirectional") (tstamp b17c4866-164b-4e79-b616-d8b6f7c46868))
    (pad "16" smd rect locked (at 3.75 5.75) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/IN2") (pinfunction "PA2") (pintype "bidirectional") (tstamp d618dca8-04de-4d0a-9ce3-4f73a62def97))
    (pad "17" smd rect locked (at 5.75 3.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/IN3") (pinfunction "PA3") (pintype "bidirectional") (tstamp d9d7dea5-4a7e-42d7-831b-dfb239c5dbbf))
    (pad "18" smd rect locked (at 5.75 3.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp 434f585c-b9be-4964-84bb-006224149650))
    (pad "19" smd rect locked (at 5.75 2.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp b5b60a50-0779-4590-9319-8904c8de2e84))
    (pad "20" smd rect locked (at 5.75 2.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/IN4") (pinfunction "PA4") (pintype "bidirectional") (tstamp 2f3454c7-2caf-4cae-985a-d3851f669c9e))
    (pad "21" smd rect locked (at 5.75 1.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/IN5") (pinfunction "PA5") (pintype "bidirectional") (tstamp 8e4f3c7c-8cbb-45bd-8c91-8c3aa5631a25))
    (pad "22" smd rect locked (at 5.75 1.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/IN6") (pinfunction "PA6") (pintype "bidirectional") (tstamp ff9cf1e0-df7d-4388-8b91-e9d93d5814c3))
    (pad "23" smd rect locked (at 5.75 0.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/IN7") (pinfunction "PA7") (pintype "bidirectional") (tstamp 1b46ec2e-4d59-47b4-8c85-1506258c5171))
    (pad "24" smd rect locked (at 5.75 0.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/230V_1_IN") (pinfunction "PC4") (pintype "bidirectional") (tstamp 43adb082-658a-436b-9161-10d6d3164234))
    (pad "25" smd rect locked (at 5.75 -0.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/230V_2_IN") (pinfunction "PC5") (pintype "bidirectional") (tstamp 265f8b75-f7ac-4541-ac79-f95339c1aad6))
    (pad "26" smd rect locked (at 5.75 -0.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/230V_3_IN") (pinfunction "PB0") (pintype "bidirectional") (tstamp bcabf357-8aac-41a4-9055-a329f25b9042))
    (pad "27" smd rect locked (at 5.75 -1.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/230V_4_IN") (pinfunction "PB1") (pintype "bidirectional") (tstamp 8a74b69f-b200-4bca-bcab-dba76007080c))
    (pad "28" smd rect locked (at 5.75 -1.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "unconnected-(U2-Pad28)") (pinfunction "PB2") (pintype "bidirectional+no_connect") (tstamp d194fb89-2c75-41c4-af74-6843d5d87084))
    (pad "29" smd rect locked (at 5.75 -2.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/sdl") (pinfunction "PB10") (pintype "passive") (tstamp d0c956a3-e6ae-412b-b2bf-44c045ccbc65))
    (pad "30" smd rect locked (at 5.75 -2.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C7-Pad1)") (pinfunction "VCAP1") (pintype "power_in") (tstamp 0183bdfa-77ba-4fef-8770-419f0ad82777))
    (pad "31" smd rect locked (at 5.75 -3.25 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp f70f6b56-cfa8-4068-a67e-e72f672ff182))
    (pad "32" smd rect locked (at 5.75 -3.75 90) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp 9eb8d898-ae4d-4c71-9837-83714f2150d9))
    (pad "33" smd rect locked (at 3.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "unconnected-(U2-Pad33)") (pinfunction "PB12") (pintype "bidirectional+no_connect") (tstamp 0370bb91-3280-4dbe-bd17-09a93bd09f19))
    (pad "34" smd rect locked (at 3.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "unconnected-(U2-Pad34)") (pinfunction "PB13") (pintype "bidirectional+no_connect") (tstamp 3cfbc9a2-6e3f-4587-8f5d-10a6024803f1))
    (pad "35" smd rect locked (at 2.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "unconnected-(U2-Pad35)") (pinfunction "PB14") (pintype "bidirectional+no_connect") (tstamp 763e438a-6676-40bc-99b7-552c536de0da))
    (pad "36" smd rect locked (at 2.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "unconnected-(U2-Pad36)") (pinfunction "PB15") (pintype "bidirectional+no_connect") (tstamp 56f141db-05f6-4907-89cc-7788d59efb13))
    (pad "37" smd rect locked (at 1.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/Vent2_IN") (pinfunction "PC6") (pintype "bidirectional") (tstamp ec34151f-6239-42c3-8eff-71737911b32a))
    (pad "38" smd rect locked (at 1.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/Vent1_IN") (pinfunction "PC7") (pintype "bidirectional") (tstamp 5cf95023-f836-4f29-aa29-d9aadd1d9641))
    (pad "39" smd rect locked (at 0.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/Full_HAUT_IN") (pinfunction "PC8") (pintype "bidirectional") (tstamp dffaab66-82d0-4f2f-9f46-dd07deeb2796))
    (pad "40" smd rect locked (at 0.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/Cro_HAUT_IN") (pinfunction "PC9") (pintype "bidirectional") (tstamp 6b489584-2ad1-4fbb-acbe-1b966a7414a1))
    (pad "41" smd rect locked (at -0.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/Flo_HAUT_IN") (pinfunction "PA8") (pintype "bidirectional") (tstamp 937b74a0-fd34-4952-b763-3ce72ba546f9))
    (pad "42" smd rect locked (at -0.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/Cro_BAS_IN") (pinfunction "PA9") (pintype "bidirectional") (tstamp 781e9f4c-60ba-41d8-a30c-3da08a83bab5))
    (pad "43" smd rect locked (at -1.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/Full_BAS_IN") (pinfunction "PA10") (pintype "bidirectional") (tstamp 828ad196-6b5f-47a3-be2b-d94f1b9a08a6))
    (pad "44" smd rect locked (at -1.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/Flo_BAS_IN") (pinfunction "PA11") (pintype "bidirectional") (tstamp d20e04a2-ae01-4ad8-aa86-9bf34ca8a05d))
    (pad "45" smd rect locked (at -2.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "unconnected-(U2-Pad45)") (pinfunction "PA12") (pintype "bidirectional+no_connect") (tstamp 4728a894-4f8f-447d-9aed-b240970f144b))
    (pad "46" smd rect locked (at -2.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/swdio") (pinfunction "PA13") (pintype "bidirectional") (tstamp 874fd4dc-1dd6-4a3d-8192-e96d10ba6fbf))
    (pad "47" smd rect locked (at -3.25 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VDD") (pintype "power_in") (tstamp 97e3eca2-1dc5-4d7e-8c51-fccab335d4eb))
    (pad "48" smd rect locked (at -3.75 -5.75 180) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VSS") (pintype "power_in") (tstamp 6d33c85a-29aa-4240-acb6-d2d9a5de82c6))
    (pad "49" smd rect locked (at -5.75 -3.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/swclk") (pinfunction "PA14") (pintype "bidirectional") (tstamp d158e028-38d5-4c3a-bd96-0fef268718a6))
    (pad "50" smd rect locked (at -5.75 -3.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "unconnected-(U2-Pad50)") (pinfunction "PA15") (pintype "bidirectional+no_connect") (tstamp 9c84ad56-aa04-4266-80c5-2d865706f7e7))
    (pad "51" smd rect locked (at -5.75 -2.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/12V_4_IN") (pinfunction "PC10") (pintype "bidirectional") (tstamp b3f351d7-c87f-40b5-ae9c-9744e8b496fc))
    (pad "52" smd rect locked (at -5.75 -2.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/12V_3_IN") (pinfunction "PC11") (pintype "bidirectional") (tstamp 6d296abd-3404-488a-b01e-905709878f9e))
    (pad "53" smd rect locked (at -5.75 -1.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/12V_2_IN") (pinfunction "PC12") (pintype "bidirectional") (tstamp 38e4630d-aed8-4603-aacb-cfa3b395652f))
    (pad "54" smd rect locked (at -5.75 -1.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/12V_1_IN") (pinfunction "PD2") (pintype "bidirectional") (tstamp 1404aa71-abbc-4cf2-b97c-28c1f7f97766))
    (pad "55" smd rect locked (at -5.75 -0.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/sda") (pinfunction "PB3") (pintype "bidirectional") (tstamp 74cc8bc5-38d7-4e22-9c6e-0a6d843fd5c3))
    (pad "56" smd rect locked (at -5.75 -0.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "unconnected-(U2-Pad56)") (pinfunction "PB4") (pintype "bidirectional+no_connect") (tstamp c7e7c33e-3cbb-4f50-b58e-a1d7ca355559))
    (pad "57" smd rect locked (at -5.75 0.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "unconnected-(U2-Pad57)") (pinfunction "PB5") (pintype "bidirectional+no_connect") (tstamp b3035346-178a-4295-be08-8ac52b59b21b))
    (pad "58" smd rect locked (at -5.75 0.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/RX") (pinfunction "PB6") (pintype "bidirectional") (tstamp a69065ce-fffd-436f-bd4f-34b178b67347))
    (pad "59" smd rect locked (at -5.75 1.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/TX") (pinfunction "PB7") (pintype "bidirectional") (tstamp e8a22b0d-dfee-41ae-b156-10867e7736ea))
    (pad "60" smd rect locked (at -5.75 1.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/boot0") (pinfunction "BOOT0") (pintype "input") (tstamp 96741217-2f30-40f3-ba7b-55dbd71daf56))
    (pad "61" smd rect locked (at -5.75 2.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "/IN8") (pinfunction "PB8") (pintype "bidirectional") (tstamp cc05c52f-b850-4d81-8b7b-262d7c7fa811))
    (pad "62" smd rect locked (at -5.75 2.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "/IN9") (pinfunction "PB9") (pintype "bidirectional") (tstamp bc8bb920-1b13-4e40-a7f5-302b3089aea6))
    (pad "63" smd rect locked (at -5.75 3.25 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "VSS") (pintype "power_in") (tstamp 2c903ebb-e411-4699-83b4-1200487bc25a))
    (pad "64" smd rect locked (at -5.75 3.75 270) (size 0.3 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VDD") (pintype "power_in") (tstamp 34cab8c3-0182-4bc3-9706-053486b838fc))
    (model "${MY_PATH}/3D/U.3dshapes/LQFP64.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp 6c75e09b-dcad-4c0d-88f0-65f4255cca2a)
    (at 77.4 77.685)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d80e9c10-efad-42ee-b325-38c1975517c6")
    (attr through_hole)
    (fp_text reference "P9" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp bc6de62f-6df4-409f-94bd-fc34dad9e329)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 39795d94-a5e5-4360-bda1-a5fb91d24399)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 5f9e3317-d7cd-4218-896b-b3545a185b45))
  )

  (footprint "Jumper:Jumper3X250V" (layer "F.Cu")
    (tedit 616418B8) (tstamp 6d3ea940-2d7c-4a41-8665-3febba0bf3f4)
    (at 89.05 52.745)
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006172bdbb")
    (attr through_hole)
    (fp_text reference "JP4" (at 4.5 0 90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ef727cc-e2df-4e4a-93c7-9646948f8b2d)
    )
    (fp_text value "Jumper3" (at 0 4.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 03240ddb-4f4a-413f-a7a4-805e88ac9cff)
    )
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1.75 0.75)
        (xy 1.75 -0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
        (xy 3.5 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 2427239c-f632-439e-93aa-8de2b6e7f904))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp c8c1d569-dd8d-46d1-852a-b0ce990e5c66))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp e556ba31-d58d-4b6c-9a14-e40698e0f173))
    (fp_line (start 1 3.25) (end -0.75 3.25) (layer "F.SilkS") (width 0.12) (tstamp 0d6e78bb-5836-4362-8566-a6fdc55b693b))
    (fp_line (start 0 -3.25) (end 0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 822c709a-0b4b-4b55-9971-9205bdffaea8))
    (fp_line (start 0 -3.25) (end -0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp efeab511-50da-41c5-855c-fc198cb12a91))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 1d5ec969-5df8-4013-8979-83acfc62aadb))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 92d0e5b1-bf26-41a7-b378-af3361b92ff1))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp bfca2791-2c34-45c6-8f68-b2172ab89f27))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 23 "/OUT_230V_4") (pintype "passive") (tstamp a6664c4f-9a0b-4170-9579-a15fc81864c8))
    (pad "2" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(JP4-Pad2)") (pintype "passive") (tstamp 86bc39bb-a7a0-47e2-81f5-2655d34c7660))
    (pad "3" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(JP4-Pad3)") (pintype "passive") (tstamp 45b153b4-9104-4edb-811b-f2d41ab43852))
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 6d56919c-c62d-4f63-9d85-e241eaabfb6b)
    (at 127.94 35.66)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/42f7a41f-b35b-4d0c-a2ee-79d6021e4ac6")
    (attr through_hole)
    (fp_text reference "C5" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp d9ffbd23-4c06-40e8-a629-8ea2b3635b53)
    )
    (fp_text value "1µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp f5ac48af-76ca-4233-b215-dcc737e15a73)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 6201ecdc-5fc7-4f4f-9572-e68b26bdbe5e))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp e5a2c596-72d4-4cce-9015-bca7211296a4))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d2954650-267c-46cf-bf62-f4d566bd0529))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 32188abd-0a1b-4dc4-a434-bce06ed297fb))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Bornier:Bornier5_1x2" (layer "F.Cu")
    (tedit 5B362772) (tstamp 6dc06c23-3818-420f-b71e-6835c4cd8d5d)
    (at 108.09 28.14)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000618c09bc")
    (attr through_hole)
    (fp_text reference "P4" (at 0.381 4.572) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 610e51a1-68b9-4dd7-b68a-7428e11e48f4)
    )
    (fp_text value "Power" (at 0.381 -3.556) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7451d2b5-7d09-44bc-8286-3c13bc90a089)
    )
    (fp_line (start -5.667 -2.5) (end -5.667 3.5) (layer "F.SilkS") (width 0.15) (tstamp 4a68dc96-848d-410e-ad01-53c2b3ff858e))
    (fp_line (start 5.969 2.54) (end -5.715 2.54) (layer "F.SilkS") (width 0.15) (tstamp 4cab33d9-da0b-4cb2-8359-3cf94b25890f))
    (fp_line (start -5.715 -2.54) (end 5.969 -2.54) (layer "F.SilkS") (width 0.15) (tstamp 9166f9d3-9bc5-42c7-96b7-c02f4849e8e4))
    (fp_line (start -5.715 3.556) (end 5.969 3.556) (layer "F.SilkS") (width 0.15) (tstamp aac282f7-ac07-4484-b4c9-3b688cbb81ee))
    (fp_line (start 5.969 -2.54) (end 5.969 3.556) (layer "F.SilkS") (width 0.15) (tstamp c8cb3ac6-fc3f-4e88-bd39-a239df6710c4))
    (pad "1" thru_hole rect locked (at -2.667 0) (size 4 4) (drill 1.1) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "/GND") (pintype "power_out") (tstamp 6723f7a4-6545-40e0-b485-32eb62a956a6))
    (pad "2" thru_hole circle locked (at 2.413 0) (size 4 4) (drill 1.1) (layers *.Cu *.Mask "F.SilkS")
      (net 29 "/12V") (pintype "power_out") (tstamp 5fc228bc-526d-4627-84d1-ea3120ecbddc))
  )

  (footprint "Jumper:Jumper3X250V" (layer "F.Cu")
    (tedit 616418B8) (tstamp 6efc89cb-52d6-4dbb-ac01-108b8a483322)
    (at 82.48 62.175)
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d6d")
    (attr through_hole)
    (fp_text reference "JP2" (at 4.5 0 90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3da5a3d2-9d54-4c26-bc35-c140de8f8a45)
    )
    (fp_text value "Jumper3" (at 0 4.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp be6d4870-02a3-4f9d-bf9c-d316a965d9db)
    )
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 4ae2125e-79e5-4e24-9063-9438d2ba24e1))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1.75 0.75)
        (xy 1.75 -0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
        (xy 3.5 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 7aaaec5a-b8c1-4427-a2bb-9629f6906e69))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp f173073d-c725-4a93-892b-3b4eb31a4a54))
    (fp_line (start 1 3.25) (end -0.75 3.25) (layer "F.SilkS") (width 0.12) (tstamp 4014a824-b583-4419-b3db-304373dc03ba))
    (fp_line (start 0 -3.25) (end 0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 66ca847d-3697-4c5a-99f1-049ca2363e52))
    (fp_line (start 0 -3.25) (end -0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp a3bf5c49-022b-4c37-b318-98d8a3489ddc))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 4845588e-3de2-4483-94c3-c6e49b44e38c))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 89ad07fa-bdbe-4ea7-bfc3-e635047b4b5e))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp a6d97fa1-711f-4d62-9d9e-5a2433a7f730))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 17 "/OUT_230V_2") (pintype "passive") (tstamp a8b3b6eb-f8c6-42be-9e75-53f32178179e))
    (pad "2" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(JP2-Pad2)") (pintype "passive") (tstamp ade75e16-0e2b-431a-a0c7-31b3c938521e))
    (pad "3" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(JP2-Pad3)") (pintype "passive") (tstamp e6556225-867a-43ec-a2b5-ab36c9d4f0a0))
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 6fea6b6a-91ec-44ae-a7a2-825e33e9023f)
    (at 93.65 69.95)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006113f020")
    (attr through_hole)
    (fp_text reference "R27" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 12af7de5-438f-40b3-8901-cff6df39fa84)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 08b7940f-f26d-497d-b60d-79a567019209)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 342813ef-9fb7-4163-8f84-b6b8818b913c))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 8ffd1771-d738-4946-aeb9-88b9409c2df0))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9d59f936-fe46-4830-b29c-7972584685a9))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(Q14-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c83ce120-b600-4b8b-9f2b-864a7266d561))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 7025dc31-a912-4e64-959a-cd89555d3dee)
    (at 135.85 26.35)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b562")
    (attr through_hole)
    (fp_text reference "C12" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 4ef8d3fe-c75e-4c37-a565-e2b29d9ba7cd)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d5f3db18-892c-42d3-9b7d-1af17c519898)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 4e04ebe6-744b-4c06-b11d-f8b1bc9665a3))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 8da1d4bd-a3bc-4940-a88a-ca9ebfe2b9d3))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f30e502c-22e9-4e4a-8b5f-e8d8a49f7036))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 18ce0592-422f-4ec5-b380-6f8b23a995b0))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp 7210e877-1ecb-4bfc-baec-694cbee7dba5)
    (at 108.5 52.85)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b50a")
    (attr through_hole)
    (fp_text reference "C16" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 7930b116-3a41-49a3-812a-a738151841b6)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 1f12dbf2-0aae-4ba4-9155-f7e42bc7ef2c)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 4ac506a4-53d2-4a60-b2a6-d806782feca5))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 632eac14-fee9-48a6-a916-0defdf5ec3ee))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9192dadd-443f-424f-b74d-5127c48428e5))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/boot0") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3e11db27-d640-483b-ba9f-cdf9fee0dacc))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SOD-123" (layer "F.Cu")
    (tedit 61B9B30C) (tstamp 754e4b9f-d9ba-4983-9ac1-4afb924c94d5)
    (at 53.02 78.385)
    (property "Partkeepr" "1300")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1c6")
    (attr through_hole)
    (fp_text reference "D3" (at 0 1.6) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp c76bbc47-43b1-4125-9463-347bf071d35a)
    )
    (fp_text value "1N4148W" (at 0 -0.0127) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
      (tstamp b240ab55-767c-4054-be79-50b69f8671d4)
    )
    (fp_line (start 1.08 -0.8) (end 1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 18f3a9e7-3348-4872-9bec-a1ce69d4706c))
    (fp_line (start -1.08 -0.8) (end -1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 28d05dd7-f941-4ad3-9108-97aba1198b8d))
    (fp_line (start 1.905 -0.762) (end 2.159 -0.762) (layer "F.SilkS") (width 0.17) (tstamp 5f024212-9d31-4f38-be6a-09f7e4bee71d))
    (fp_line (start -2.6 -1) (end -2.6 -0.6) (layer "F.SilkS") (width 0.12) (tstamp af81938e-8a13-4137-a26c-db9087f8a9e7))
    (fp_line (start -2.8 -0.8) (end -2.4 -0.8) (layer "F.SilkS") (width 0.12) (tstamp d8bf9871-ac1a-41c3-be74-776823ae2c45))
    (pad "1" smd rect locked (at -1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "K") (pintype "passive") (tstamp e52aca4f-e8af-49cc-ade6-4976ef326821))
    (pad "2" smd rect locked (at 1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 73ef6609-1f38-493c-8fc9-3f3e30aee277))
    (model "${MY_PATH}/3D/D.3dshapes/SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 759fb291-21c3-4d58-9a25-6bfe82b052c9)
    (at 133.35 30.06)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182afa3")
    (attr through_hole)
    (fp_text reference "R3" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp f96c446f-ba54-4324-898e-1e2d961ca90d)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 6059efc4-d9e6-446c-830c-9be93f9676e3)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3dfe2705-9e86-472c-8a0f-3f37d0a5e098))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 4bbec282-43ea-44d1-a0bf-e60824c40729))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(Q1-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 591d96c1-229d-426e-880a-9de1ac70c26e))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/12V_1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d76d1056-2c94-4457-8cd4-ea0396a0ef43))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Module:ESP-12F" (layer "F.Cu")
    (tedit 61B9BC79) (tstamp 795bf2ff-c0bd-44ae-8dc8-b9a5a3a4e223)
    (at 52.26 37.6)
    (property "Partkeepr" "2800")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/c61e59c2-2aa1-45dd-b3c5-7ee4fb2fb345")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -13) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11bf3717-0ad4-4f2e-b06c-98aa8d961b12)
    )
    (fp_text value "ESP-12F" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed2224ac-c62e-488e-a8d9-c7bfe5b3a87c)
    )
    (fp_line (start -6.5 10.5) (end -6.5 -12) (layer "F.SilkS") (width 0.15) (tstamp 1e034db0-86ba-449a-b4e9-a533d3e521a9))
    (fp_line (start 6.5 10.5) (end -6.5 10.5) (layer "F.SilkS") (width 0.15) (tstamp 4c19f20b-c39b-462c-a2f6-602b5733057b))
    (fp_line (start 6.5 -12) (end 6.5 10.5) (layer "F.SilkS") (width 0.15) (tstamp 87e8c42f-37ee-4bf5-8e01-da6cabfc5321))
    (fp_line (start -6.5 -12) (end 6.5 -12) (layer "F.SilkS") (width 0.15) (tstamp ac0a73fc-3e20-4442-8bde-354920ac9fce))
    (pad "1" smd rect locked (at -7.6 -3.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/RST") (pinfunction "RST") (pintype "input") (tstamp f1335666-6a14-4b5f-86e3-10d1aefa6db0))
    (pad "2" smd rect locked (at -7.6 -1.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "unconnected-(U1-Pad2)") (pinfunction "ADC") (pintype "input+no_connect") (tstamp 2a5809f6-890f-4ae2-a6a6-f0737123808a))
    (pad "3" smd rect locked (at -7.6 0.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R1-Pad2)") (pinfunction "EN") (pintype "input") (tstamp 9131aea5-ceeb-4140-bf9b-ace4037e6746))
    (pad "4" smd rect locked (at -7.6 2.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "unconnected-(U1-Pad4)") (pinfunction "GPIO16") (pintype "input+no_connect") (tstamp 9eea7d74-11ba-4aa0-9ada-b6d04726030d))
    (pad "5" smd rect locked (at -7.6 4.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "unconnected-(U1-Pad5)") (pinfunction "GPIO14") (pintype "input+no_connect") (tstamp a4d128e3-4187-43a4-a717-9a74d95f53b0))
    (pad "6" smd rect locked (at -7.6 6.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "unconnected-(U1-Pad6)") (pinfunction "GPIO12") (pintype "input+no_connect") (tstamp 55b0917a-8f98-440a-818b-26a2375aed5d))
    (pad "7" smd rect locked (at -7.6 8.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(U1-Pad7)") (pinfunction "GPIO13") (pintype "input+no_connect") (tstamp 436a47ee-5d71-447f-86bd-abc9773bc082))
    (pad "8" smd rect locked (at -7.6 10.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "VCC") (pintype "input") (tstamp ea5cd121-c3d7-45e1-aa4d-e2bee89b54fc))
    (pad "9" smd rect locked (at -5 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U1-Pad9)") (pinfunction "CS0") (pintype "input+no_connect") (tstamp 59c1aae6-31a0-40d0-902a-558cf908d541))
    (pad "10" smd rect locked (at -3 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(U1-Pad10)") (pinfunction "MISO") (pintype "input+no_connect") (tstamp 856c2d03-4a87-40c4-a743-fdc6701f7d42))
    (pad "11" smd rect locked (at -1 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "unconnected-(U1-Pad11)") (pinfunction "GPIO9") (pintype "input+no_connect") (tstamp 994b24c0-fd30-48a7-8756-0678ed1e8c66))
    (pad "12" smd rect locked (at 1 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U1-Pad12)") (pinfunction "GPIO10") (pintype "input+no_connect") (tstamp 48449591-c82e-4e16-be40-341d7648e3d4))
    (pad "13" smd rect locked (at 3 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(U1-Pad13)") (pinfunction "MOSI") (pintype "input+no_connect") (tstamp ee94609b-49e1-45be-85a0-cd17fcd9c7f6))
    (pad "14" smd rect locked (at 5 11.5) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "unconnected-(U1-Pad14)") (pinfunction "SCLK") (pintype "input+no_connect") (tstamp 5af123a1-3a3b-4c18-83e9-69e1e355265a))
    (pad "15" smd rect locked (at 7.6 10.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "GND") (pintype "input") (tstamp 70fa0348-0bb9-4654-b6ab-01d9f13047b4))
    (pad "16" smd rect locked (at 7.6 8.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "GPIO15") (pintype "input") (tstamp 232c4951-2f37-400b-ae60-bc534e0c70ca))
    (pad "17" smd rect locked (at 7.6 6.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(R6-Pad2)") (pinfunction "GPIO2") (pintype "input") (tstamp d8c3149f-0a6c-4987-be91-ff1ad1f4b443))
    (pad "18" smd rect locked (at 7.6 4.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/GPIO0") (pinfunction "GPIO0") (pintype "input") (tstamp 833aa0ca-f929-40bb-ac00-22558baf520f))
    (pad "19" smd rect locked (at 7.6 2.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U1-Pad19)") (pinfunction "GPIO4") (pintype "input+no_connect") (tstamp d44bf05b-0d0a-4650-a34d-aa3401970b42))
    (pad "20" smd rect locked (at 7.6 0.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U1-Pad20)") (pinfunction "GPIO5") (pintype "input+no_connect") (tstamp 48838095-3e4a-4e1e-ad8e-b60f43732469))
    (pad "21" smd rect locked (at 7.6 -1.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/RX") (pinfunction "RXD") (pintype "input") (tstamp c305ae4d-12e0-4d69-9390-9a73bbb3915c))
    (pad "22" smd rect locked (at 7.6 -3.5) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/TX") (pinfunction "TXD") (pintype "input") (tstamp 3387e7aa-db8c-44b0-8e80-601c632b2fdc))
    (model "${MY_PATH}/3D/Module.3dshapes/ESP-12F.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 79e849c8-d34a-4a2e-b644-2255ee5ab6cc)
    (at 103.37 63.6)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006125010e")
    (attr through_hole)
    (fp_text reference "R22" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp f64b988d-c3f6-4d1f-b5ee-5276b39082c3)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 869e42ab-688d-4aca-bc6a-486483007a7a)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 15d66eae-7435-4c1f-9d78-b5f4488bce1a))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 79549ffb-0079-44e6-bf5d-85d5f68700ca))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/Flo_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 9a2b0c84-e0d2-4258-a6f2-fa0b4119a5dd))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(Q11-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 38b32e6e-1f9a-4365-8a3f-2d042726eab3))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 7b8937ce-1a4c-406f-8be4-d73f4aab643e)
    (at 104.9 52.86)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa77")
    (attr through_hole)
    (fp_text reference "R14" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp be1da735-ead3-40e3-a31b-b63eee10bb84)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp ee6ae239-fe27-4134-a776-17bd4ef5bb6f)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 98ed3162-990b-4e04-b1f2-026e060ed3d4))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp f14e603f-6ca0-4209-afd4-81cfdd4ef94e))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(Q10-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8f9ced1a-afdc-414e-85a1-e95d936e8d0c))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/230V_4_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 710c2f48-ba25-4512-989f-797671d69427))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0603" (layer "F.Cu")
    (tedit 61B9ACFA) (tstamp 7dfca857-0c1e-4096-bba2-d2e31cdac26f)
    (at 97 69.69)
    (property "Partkeepr" "0600")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b548")
    (attr through_hole)
    (fp_text reference "C3" (at 0 1.3 180) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 4fcc727c-a0fc-49a4-bd05-03fce6380e59)
    )
    (fp_text value "22pF" (at -0.7 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 357b9c67-a45a-464a-bd6f-cd35118534a8)
    )
    (fp_line (start -0.2 -0.49) (end 0.2 -0.49) (layer "F.SilkS") (width 0.17) (tstamp 34b3abd2-bbf8-460c-a0b5-28d2c777c32f))
    (fp_line (start 0.2 0.5) (end -0.2 0.5) (layer "F.SilkS") (width 0.17) (tstamp 76b0261e-d802-400b-b241-a41a47bb41cd))
    (pad "1" smd rect (at 0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 99a3e9ee-06d1-45b8-b79a-6365dcb64051))
    (pad "2" smd rect (at -0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1985b035-0364-43c2-a0b1-e6f13ee684de))
    (model "${MY_PATH}/3D/C.3dshapes/0603.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:Jumper3X250V" (layer "F.Cu")
    (tedit 616418B8) (tstamp 88c16b63-d060-4522-ac6c-c23d49adda5f)
    (at 107.05 36.075)
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006177bd08")
    (attr through_hole)
    (fp_text reference "JP1" (at 4.5 0 90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dfa73398-fe5b-4e19-9415-596507cdcc01)
    )
    (fp_text value "Jumper3" (at 0 4.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 72ee4641-80be-4e6c-a8a4-e1cd6d85b470)
    )
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1.75 0.75)
        (xy 1.75 -0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
        (xy 3.5 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 577cb776-88f5-47c5-a62f-f635641d9d2f))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 83832288-b3f5-44b1-a1ee-0a3af8aee09a))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp cff32f11-6a85-41f8-9a1e-1aa3adaa89dc))
    (fp_line (start 0 -3.25) (end -0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 5a8759d6-22d2-440d-8d1b-06c5feb36613))
    (fp_line (start 0 -3.25) (end 0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp d4770a44-b20f-41f1-ad6d-2de99065e10c))
    (fp_line (start 1 3.25) (end -0.75 3.25) (layer "F.SilkS") (width 0.12) (tstamp d7bb0657-4cba-47eb-af7e-c2f79eedea38))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 6ea93336-dc95-440c-bf96-53c617d1d74d))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 9a47d23b-7f4d-4f63-9001-5757e88ac04c))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp e275ab62-c79a-4b8f-9959-d3811c3e7054))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 14 "/OUT_230V_1") (pintype "passive") (tstamp 7eab3388-f1f6-421e-bdcb-15a21cf3c55c))
    (pad "2" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(JP1-Pad2)") (pintype "passive") (tstamp da70ef60-0873-4370-bb98-2239d97ec550))
    (pad "3" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 13 "Net-(JP1-Pad3)") (pintype "passive") (tstamp cccaf0ce-b166-4b96-bbcb-71d3eef3fdcc))
  )

  (footprint "PinHeader:PinHeader2.54_1X5" (layer "F.Cu")
    (tedit 61B9B7E6) (tstamp 8b5b9b38-c0fd-47fb-a325-5a15da1a3186)
    (at 50.058 74.475)
    (property "Partkeepr" "0100")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/b8a200f3-5c6c-4080-b75e-46947944eca5")
    (attr through_hole)
    (fp_text reference "P1" (at 0 2.032) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfa00454-7ebc-46f1-ba03-07ba5132b283)
    )
    (fp_text value "CONN_01X05" (at 0 -1.905) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 360e2eab-8ab7-40cf-8961-9435df6a4e2f)
    )
    (fp_line (start 6.35 1.143) (end 6.35 -1.143) (layer "F.SilkS") (width 0.15) (tstamp 1c7fdc5c-e9a5-4cd0-9f77-bdd2911c39fe))
    (fp_line (start -5.207 1.778) (end -5.334 1.524) (layer "F.SilkS") (width 0.15) (tstamp 3b88a686-3770-4bba-8b6e-cdb2a62c0c0d))
    (fp_line (start -5.461 -1.905) (end -4.953 -1.905) (layer "F.SilkS") (width 0.15) (tstamp 4059ea71-802b-4e4b-bd73-236e1223253d))
    (fp_line (start -5.207 -1.524) (end -5.461 -1.905) (layer "F.SilkS") (width 0.15) (tstamp 414f2d76-9a61-441e-84d5-20473ee1c845))
    (fp_line (start -5.08 -1.778) (end -5.334 -1.778) (layer "F.SilkS") (width 0.15) (tstamp 51ad7619-d3cf-4c1b-b760-bf7b0c57c244))
    (fp_line (start 6.35 -1.143) (end -6.223 -1.143) (layer "F.SilkS") (width 0.15) (tstamp 594d7df9-8619-4578-8722-ed7cefb8b950))
    (fp_line (start -6.223 1.143) (end 6.35 1.143) (layer "F.SilkS") (width 0.15) (tstamp 5d5c46a7-c83d-4146-9e21-1b42ad29505a))
    (fp_line (start -4.953 -1.905) (end -5.207 -1.524) (layer "F.SilkS") (width 0.15) (tstamp 94af8f03-c9c7-4e28-9f57-1fa64b2860fd))
    (fp_line (start -6.223 -1.143) (end -6.223 1.143) (layer "F.SilkS") (width 0.15) (tstamp a446bb36-d9d0-4fa9-bd76-bf0c0d296f96))
    (fp_line (start -5.207 -1.651) (end -5.08 -1.778) (layer "F.SilkS") (width 0.15) (tstamp a9646f1d-ab42-496b-9424-0029e4179345))
    (fp_line (start -5.334 1.524) (end -5.334 1.651) (layer "F.SilkS") (width 0.15) (tstamp c0ab5aaa-d6cb-42f2-80fc-3a191796601a))
    (fp_line (start -5.207 -1.778) (end -5.207 -1.651) (layer "F.SilkS") (width 0.15) (tstamp c9252769-392f-42a2-a5be-5ff8a8bcdd93))
    (fp_line (start -5.461 1.778) (end -5.207 1.778) (layer "F.SilkS") (width 0.15) (tstamp ed26bc52-fac3-4bf6-af7a-949dcc505c01))
    (fp_line (start -5.334 1.524) (end -5.461 1.778) (layer "F.SilkS") (width 0.15) (tstamp f0cc2eda-8b8b-4e6b-8d0c-4b52000407e8))
    (pad "1" thru_hole circle locked (at -5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 25 "/TX") (pinfunction "P1") (pintype "passive") (tstamp 49029a7b-c8c0-4226-9f37-898aea8fe250))
    (pad "2" thru_hole circle locked (at -2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "/RX") (pinfunction "P2") (pintype "passive") (tstamp f44f0b38-6cc7-4137-b7c9-228db49d3c2b))
    (pad "3" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "/GPIO0") (pinfunction "P3") (pintype "passive") (tstamp 30e0695c-6d7f-4c41-bd92-46441470ce02))
    (pad "4" thru_hole circle locked (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "/RST") (pinfunction "P4") (pintype "passive") (tstamp 88d7e066-1ed7-4bd4-9530-2718c42015e6))
    (pad "5" thru_hole circle locked (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "/GND") (pinfunction "P5") (pintype "passive") (tstamp 739ee6ae-1371-4da6-81fc-1c362f4658c9))
    (model "${MY_PATH}/3D/PinHeader.3dshapes/PinHeader2.54_1X5.step"
      (offset (xyz 1 11.5 -5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 8e766716-8269-490f-8067-bf7061a791f0)
    (at 103.37 60.93)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061154d7b")
    (attr through_hole)
    (fp_text reference "R30" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 37f032e4-0bd3-401c-9596-cff8d6ae71f7)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 6ffe00bd-fbe6-4527-9963-e7901a56ac53)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 0cf942dc-53b0-4759-8dff-4910cb2a6e95))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 23e725a3-099c-455e-9e25-ea0e3813adcb))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/Flo_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ec272dce-64cc-4be9-ae59-36437b7aa708))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(Q14-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 322b4143-279c-4b92-b4a4-9f57e4f5dd65))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT-223" (layer "F.Cu")
    (tedit 61B9BBA8) (tstamp 92dbbc1e-bf46-4d83-ad73-e1decce21c13)
    (at 114.81 37.245)
    (property "Partkeepr" "2004")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d995062a-4b0a-430d-b42a-28233eb04ccc")
    (attr through_hole)
    (fp_text reference "Q4" (at 4.5 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89fcaaba-4399-4a5d-899f-2a61c80a833e)
    )
    (fp_text value "IRLL2705" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp aaf20351-a05b-4bf7-be2f-8acba2a996c4)
    )
    (fp_line (start 3.15 -1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 091defb4-ce68-4310-9a6a-21b5c2c8350b))
    (fp_line (start -3.15 -1.75) (end -3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 720cb75f-8ed0-4965-9ad4-43ecf29ae9c0))
    (fp_line (start -3.15 -1.75) (end 3.15 -1.75) (layer "F.SilkS") (width 0.12) (tstamp d80485f4-12e5-4c82-9d75-d23381f4394b))
    (fp_line (start -3.15 1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp f9b33ba2-8e2d-4c16-8e16-2caff8cbe514))
    (pad "1" smd rect locked (at -2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(Q4-Pad1)") (pinfunction "G") (pintype "input") (tstamp 56c00ac8-4f97-4a90-89b7-3b98b3d51477))
    (pad "2" smd rect locked (at 0 -3.25) (size 4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/OUT_12V_4") (pinfunction "D") (pintype "input") (tstamp 3aeefcb7-437e-4bbe-8325-40aa8cb3cebc))
    (pad "2" smd rect locked (at 0 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/OUT_12V_4") (pinfunction "D") (pintype "input") (tstamp e64b7f92-c546-4dfa-b58e-94daa667535e))
    (pad "3" smd rect locked (at 2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "S") (pintype "input") (tstamp 78874d21-4c8e-4003-b312-b2a995826780))
    (model "${MY_PATH}/3D/U.3dshapes/SOT-223.step"
      (offset (xyz -0.35 -11.5 -8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 945954f2-5a45-465e-a1f2-3f04f1bb52eb)
    (at 118.47 45.83)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/6b0bebb7-cee2-45da-8bc7-fb070cf9bc8c")
    (attr through_hole)
    (fp_text reference "R5" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp fc0acc51-6044-407f-9f8d-ffa582e0ad14)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp f9b686ba-abaa-4154-a207-269b40967058)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 65d83845-fee0-4318-8851-cbbe06334de7))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp dc050144-08a2-478e-9a43-a0ad9b17dd9d))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8fe28619-9fa7-4ae8-a4e1-82371757e60f))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/GPIO0") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 13618bdd-87df-4dad-be87-63945ada8853))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Jumper:Jumper3X250V" (layer "F.Cu")
    (tedit 616418B8) (tstamp 96d135d4-4bbe-4b7e-8fdb-d579387959c4)
    (at 119.88 28.835)
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1d4")
    (attr through_hole)
    (fp_text reference "JP3" (at 4.5 0 90) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 40352355-0080-4b73-9076-1da92a71a720)
    )
    (fp_text value "Jumper3" (at 0 4.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b1206d25-ad18-4bb2-b508-eb44fe17833b)
    )
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 0c1b447c-23dc-4ce8-8c4c-6b59426e75f8))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp 3b139347-3082-4a21-abb6-49417a08e8fd))
    (fp_poly (pts
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1.75 0.75)
        (xy 1.75 -0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
        (xy 3.5 -3.25)
      ) (layer "F.Cu") (width 0.1) (fill solid) (tstamp a3d75311-9e3c-4616-8a77-97e14840247b))
    (fp_line (start 1 3.25) (end -0.75 3.25) (layer "F.SilkS") (width 0.12) (tstamp 134dde94-4361-453c-9b36-2b0605df0156))
    (fp_line (start 0 -3.25) (end -0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 4ac18931-6a47-4158-8b8c-2f3465de6c54))
    (fp_line (start 0 -3.25) (end 0.75 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 9f3ad782-9479-4993-af0b-ad5cdd3a4bd5))
    (fp_poly (pts
        (xy -1.75 2)
        (xy -0.75 3.25)
        (xy -3.5 3.25)
        (xy -3.5 0.75)
        (xy -0.75 0.75)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp 9cf56269-698e-431b-a955-799e17f2db89))
    (fp_poly (pts
        (xy -1.75 -2)
        (xy -0.75 -0.75)
        (xy -3.5 -0.75)
        (xy -3.5 -3.25)
        (xy -0.75 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp d34f0533-9d93-43ff-aae3-c1394e108f97))
    (fp_poly (pts
        (xy 3.5 -3.25)
        (xy 3.5 3.25)
        (xy 1 3.25)
        (xy 0 2)
        (xy 1 0.75)
        (xy 1 -0.75)
        (xy 0 -2)
        (xy 1 -3.25)
      ) (layer "F.Mask") (width 0.1) (fill solid) (tstamp f2c512bb-6f68-458b-b85d-cfebe6b2c0bc))
    (pad "1" smd rect locked (at 2.25 0) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 20 "/OUT_230V_3") (pintype "passive") (tstamp 60776020-d6ed-40fc-b1f3-f98e8f4119d7))
    (pad "2" smd circle locked (at -3.5 -2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(JP3-Pad2)") (pintype "passive") (tstamp 3329d14f-0373-43ab-bd22-6f00e6036479))
    (pad "3" smd circle locked (at -3.5 2) (size 2.5 2.5) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(JP3-Pad3)") (pintype "passive") (tstamp 59d0d8b5-a681-4a55-a9ec-6065d69216f6))
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 97d750b0-4d15-49c5-9591-9f7315832ea8)
    (at 86.45 70.79)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250122")
    (attr through_hole)
    (fp_text reference "R23" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 5a2ae3a9-d192-42d1-9439-ade331a0324d)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 0f49cd40-b3ef-4747-8fc0-f4ab85a78262)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 62d60640-1525-4a3e-8d1b-25502c6abca4))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp d5adf31b-2284-41c6-8c5c-d1124b4b9a6f))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/Full_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f2ee187a-abdb-439c-b787-4a3102c4fe77))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(Q12-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 27bb713a-b65d-4a32-9db4-cf39549c8713))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SOD-123" (layer "F.Cu")
    (tedit 61B9B30C) (tstamp 99a64fb7-a20c-4d01-bdbf-c0e7fa12cc25)
    (at 107.41 41.445)
    (property "Partkeepr" "1300")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa92")
    (attr through_hole)
    (fp_text reference "D4" (at 0 1.6) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 7857b0a4-039e-4e18-b2ac-784890caaeb4)
    )
    (fp_text value "1N4148W" (at 0 -0.0127) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
      (tstamp ea0cd23f-c7c3-4288-af42-06a370617522)
    )
    (fp_line (start 1.08 -0.8) (end 1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 42eec751-06e3-43e6-8707-77940fc144d9))
    (fp_line (start -1.08 -0.8) (end -1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 81894bc0-59e3-4e8b-b675-0c1220d852a7))
    (fp_line (start -2.6 -1) (end -2.6 -0.6) (layer "F.SilkS") (width 0.12) (tstamp bdd3b49f-67b5-41dc-a441-8968f9d48fee))
    (fp_line (start 1.905 -0.762) (end 2.159 -0.762) (layer "F.SilkS") (width 0.17) (tstamp d6343cee-4a12-4425-840d-b56aae821403))
    (fp_line (start -2.8 -0.8) (end -2.4 -0.8) (layer "F.SilkS") (width 0.12) (tstamp e0f4b472-44d7-4511-8053-0659d33b08a6))
    (pad "1" smd rect locked (at -1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "K") (pintype "passive") (tstamp 45a1fac9-43cd-47ba-9b1e-6738325923c0))
    (pad "2" smd rect locked (at 1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 6e496941-2f93-441f-8a57-43c0db1f3267))
    (model "${MY_PATH}/3D/D.3dshapes/SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp 9a5ef001-f568-4d62-a8e1-e5f2aaf69ffe)
    (at 120.53 38.195)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608ae")
    (attr through_hole)
    (fp_text reference "Q15" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp efd65811-ff21-41aa-8186-21a3fecf72e4)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb698743-0c44-46d9-b38f-6f6d0e6d62d4)
    )
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 037e6efb-dca3-4309-95d0-0cf33fd54883))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 22908e7c-0d0f-4838-ba91-669b478148ec))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 967954a0-6a9d-4563-ae8b-04bc868cfecb))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp dd8ef232-39cc-4496-b734-1cbb1ea8c50c))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(Q15-Pad1)") (pintype "input") (tstamp 280a258e-9b67-48ab-bce3-80e17cc4c410))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/Full_BAS") (pintype "input") (tstamp a5f9249a-637d-49d9-8616-773ca4220f84))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(Q15-Pad3)") (pintype "input") (tstamp 2e16a7e7-2f7c-4ef7-975e-7969c6136dc4))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "PinHeader:PinHeader2.54_1X5" (layer "F.Cu")
    (tedit 61B9B7E6) (tstamp 9dbe4839-935f-40ab-a25f-5bb51bbea63e)
    (at 50.058 69.645)
    (property "Partkeepr" "")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b58c")
    (attr through_hole)
    (fp_text reference "P16" (at 0 2.032) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 57514e3b-0320-4491-80b0-d74f185abbad)
    )
    (fp_text value "Debug µC" (at 0 -1.905) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06f5c95c-bc3b-43f1-9835-6102143494b7)
    )
    (fp_line (start -5.207 -1.524) (end -5.461 -1.905) (layer "F.SilkS") (width 0.15) (tstamp 14591e7e-8487-4f26-a8a5-658a0c3e9f0f))
    (fp_line (start -6.223 -1.143) (end -6.223 1.143) (layer "F.SilkS") (width 0.15) (tstamp 1bb538d5-5373-4237-bb9c-ceaaa7447bf9))
    (fp_line (start -5.08 -1.778) (end -5.334 -1.778) (layer "F.SilkS") (width 0.15) (tstamp 1d5bbb5a-90e0-4a85-982b-026bf0054cee))
    (fp_line (start -5.461 -1.905) (end -4.953 -1.905) (layer "F.SilkS") (width 0.15) (tstamp 26beb1d4-d5b0-4f8e-9f14-9b8d4441a24e))
    (fp_line (start -4.953 -1.905) (end -5.207 -1.524) (layer "F.SilkS") (width 0.15) (tstamp 29642e48-2fac-4310-bb01-83e7c0a1644d))
    (fp_line (start -5.334 1.524) (end -5.334 1.651) (layer "F.SilkS") (width 0.15) (tstamp 2a3064cc-b725-4b1f-9383-6638da4ea1ce))
    (fp_line (start 6.35 1.143) (end 6.35 -1.143) (layer "F.SilkS") (width 0.15) (tstamp 3b746f2a-edd4-4c28-8b5e-c4f8b3dc1dda))
    (fp_line (start -6.223 1.143) (end 6.35 1.143) (layer "F.SilkS") (width 0.15) (tstamp 3ba53f33-622b-4c19-9cf9-712477dfddf1))
    (fp_line (start -5.207 -1.778) (end -5.207 -1.651) (layer "F.SilkS") (width 0.15) (tstamp 8657d79a-942a-42d6-b4e1-578bdfdc1f89))
    (fp_line (start -5.207 -1.651) (end -5.08 -1.778) (layer "F.SilkS") (width 0.15) (tstamp 88548b24-d284-40c0-9e01-74eea955bff4))
    (fp_line (start -5.461 1.778) (end -5.207 1.778) (layer "F.SilkS") (width 0.15) (tstamp 92f90196-f4b1-496e-897b-3db9ed6096c3))
    (fp_line (start 6.35 -1.143) (end -6.223 -1.143) (layer "F.SilkS") (width 0.15) (tstamp 9ae744d1-2ba0-4aa8-98c6-5e0945a602bc))
    (fp_line (start -5.207 1.778) (end -5.334 1.524) (layer "F.SilkS") (width 0.15) (tstamp d2b0e40c-6851-44e1-b915-c82df6fcdb60))
    (fp_line (start -5.334 1.524) (end -5.461 1.778) (layer "F.SilkS") (width 0.15) (tstamp f19d81e9-4dac-409c-b970-2328584a4beb))
    (pad "1" thru_hole circle locked (at -5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "/3.3V") (pinfunction "P1") (pintype "passive") (tstamp fbb48271-bd15-41e5-864c-cb81a024115b))
    (pad "2" thru_hole circle locked (at -2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 33 "/swclk") (pinfunction "P2") (pintype "passive") (tstamp 49c6068f-fddd-44d2-ae5b-e0576edc819f))
    (pad "3" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "/GND") (pinfunction "P3") (pintype "passive") (tstamp 8c6ff26f-3d37-4af4-bd94-19578e711324))
    (pad "4" thru_hole circle locked (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 34 "/swdio") (pinfunction "P4") (pintype "passive") (tstamp b133fa16-7d6f-4d8c-ad38-729bef4ae4f4))
    (pad "5" thru_hole circle locked (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask "F.SilkS")
      (net 6 "/nrst") (pinfunction "P5") (pintype "passive") (tstamp 1ff27306-5705-4f0f-ac1a-8aa8a0907c88))
    (model "${MY_PATH}/3D/PinHeader.3dshapes/PinHeader2.54_1X5.step"
      (offset (xyz 1 11.5 -5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp 9ec115e2-fd1b-47b4-9cba-c7953d3bc640)
    (at 95.95 64.63)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182abc5")
    (attr through_hole)
    (fp_text reference "R7" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp fced2022-6d18-4149-8a39-565de9f0c674)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 170484db-f905-45e4-8a6c-5733398eaf66)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 01202a75-c23a-40eb-bb89-444d94db66a0))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp c2e332d1-9e6d-4b59-a402-fa7e958474fd))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(Q3-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 202d0463-5015-4bab-9753-f2cc3d0262b8))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/12V_3_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c053cd74-aaf5-4d1d-814c-20d13fd93c4d))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SO8N" (layer "F.Cu")
    (tedit 57E93E6D) (tstamp a1906991-fc7e-4163-828a-954c74119aec)
    (at 71.825 75.915)
    (property "Partkeepr" "1507")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/cac6055c-4eb4-4fc3-88e2-0f95b47ffaec")
    (attr through_hole)
    (fp_text reference "U3" (at 3.5 0.05 270) (layer "F.SilkS")
      (effects (font (size 0.75 0.75) (thickness 0.15)))
      (tstamp 36680146-4c2b-4b94-92b7-09d20bb2107b)
    )
    (fp_text value "P82B715" (at 3.45 0 270) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b389f51-2617-4d89-b9c4-0aef34a3000e)
    )
    (fp_line (start -2.5 1.75) (end -2.5 -1.75) (layer "F.SilkS") (width 0.15) (tstamp 0fcf8bbd-a2d2-4586-96e8-eecb60769acb))
    (fp_line (start 2.5 1.75) (end -2.5 1.75) (layer "F.SilkS") (width 0.15) (tstamp 4206ba97-7681-4450-afd7-099ee1323f7b))
    (fp_line (start 2.5 -1.75) (end 2.5 1.75) (layer "F.SilkS") (width 0.15) (tstamp 43086112-50f6-4921-bec2-8c3993946674))
    (fp_line (start -2.5 -1.75) (end 2.5 -1.75) (layer "F.SilkS") (width 0.15) (tstamp 537d89e2-c5fc-4252-bd36-70100da63ce9))
    (fp_line (start -2.5 -1.75) (end 2.5 -1.75) (layer "F.SilkS") (width 0.15) (tstamp 80d5c74c-c294-4413-bfff-dcdc531c38fe))
    (fp_circle (center -1.95 1.35) (end -1.95 1.55) (layer "F.SilkS") (width 0.15) (fill none) (tstamp 34fc8d00-a6e5-4ce7-92be-6539f7be03e5))
    (pad "1" smd rect (at -1.905 2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "unconnected-(U3-Pad1)") (pinfunction "NC") (pintype "no_connect") (tstamp 32f9a2f6-7a19-49c1-9606-b454bc183dc3))
    (pad "2" smd rect (at -0.7 2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/LDA") (pinfunction "Lx") (pintype "bidirectional") (tstamp aa43fc84-d470-4162-aaa9-f5eccf202c96))
    (pad "3" smd rect (at 0.635 2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/sda") (pinfunction "Sx") (pintype "bidirectional") (tstamp 1f3a486d-9c4c-4e7e-9629-da731a5a1e29))
    (pad "4" smd rect (at 1.905 2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "GND") (pintype "power_out") (tstamp 325fad30-87c5-4874-9d5b-a5b759f9b8c8))
    (pad "5" smd rect (at 1.905 -2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(U3-Pad5)") (pinfunction "NC") (pintype "open_collector") (tstamp d0b6cb1c-8647-47cc-902f-f92f84a47c4a))
    (pad "6" smd rect (at 0.635 -2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/sdl") (pinfunction "Sy") (pintype "bidirectional") (tstamp b386f0c2-0fec-4cfe-90fc-7b9599cfffd4))
    (pad "7" smd rect (at -0.635 -2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/LDL") (pinfunction "Ly") (pintype "bidirectional") (tstamp 66a550d5-02a9-4293-9e22-21ad5d63334c))
    (pad "8" smd rect (at -1.905 -2.65) (size 0.6 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "Vcc") (pintype "power_in") (tstamp e1c407d8-33ce-4f8b-be1a-2bd1085b113e))
    (model "${MY_PATH}/3D/U.3dshapes/SO8S.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp a1f56346-88f6-4273-91cb-238453d4a402)
    (at 122.07 44.66)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611b737b")
    (attr through_hole)
    (fp_text reference "R9" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 85986571-d5e5-45d1-ac66-8ba2113e907c)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 8135c964-fba9-49e7-8ec7-1122ccd35626)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 4e3dfc0d-d9de-466e-b8d5-c83a594486f4))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp b1c26d58-cca2-4e9e-afd6-312ee9cba16c))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(Q5-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 72d2dbc5-a16d-4e03-8d7a-f7335c628c50))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/Vent1_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 403b29a7-6ddb-4f79-bda4-a55c3610966d))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp a4c85cbd-1b76-449a-bb32-432f0fadfbfc)
    (at 107.39 58.18)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611608bb")
    (attr through_hole)
    (fp_text reference "R31" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 33864088-9722-413a-95fe-70ed693e5e20)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 4bc49831-8a9b-47d4-8324-2e649e671a93)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3c95f4a2-c9d1-4e18-9525-9a1f26893830))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 5a4f5349-0ed0-475c-b7fc-44eb37ca5359))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/Full_BAS_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp f95413da-0c38-4467-9955-d8c4cdd61320))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(Q15-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 064f400a-6eef-4ae1-b8fd-879c235f28f8))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp a7882f45-c0ff-41c9-bb3d-6ce551fd47bd)
    (at 131.54 32.73)
    (property "Champ4" "0931")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/a151b0ce-7d72-482b-b53f-bf4b1081e17a")
    (attr through_hole)
    (fp_text reference "R18" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 6017a9b1-3df9-43ca-bc55-ca98b7696b04)
    )
    (fp_text value "4.7K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp d82054ef-cd28-4c0e-b97f-2a6a946766c1)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 37d8a727-9a62-4417-9ed9-ac4f4f98be19))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 7e421f8c-1365-4f47-b457-dfe91ee20e2c))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp ec92b7b6-241f-46c6-af8c-878e652e57fd))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/LDL") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 13565e32-9748-4097-8381-745152a57b4e))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp a91188f0-ce71-4eb7-a91a-d3eb439e941d)
    (at 99.55 66.23)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654e3")
    (attr through_hole)
    (fp_text reference "R29" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 1196142f-d00f-490d-919b-18aefed4b5d5)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 5e905353-9ed4-49df-8ef1-e0579f6b7ada)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 3536fea0-2af9-4e74-a43b-845eea98c446))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp ad1e9208-5f24-4cbb-a25a-737b5b1f9b64))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3e6cb554-b22a-4dd8-8546-e28e70bb3cc0))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(Q16-Pad3)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp fc771a8e-52b3-42e4-b5a6-a96287772ccc))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT-223" (layer "F.Cu")
    (tedit 61B9BBA8) (tstamp a917dca0-48bb-4bcd-85a4-a21a3c769b03)
    (at 90.24 61.155)
    (property "Partkeepr" "2004")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/372c1b8e-3b7d-4a68-be87-3ce9640b5f57")
    (attr through_hole)
    (fp_text reference "Q3" (at 4.5 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp df476e6f-2755-4da9-9469-bc9dd7a9df98)
    )
    (fp_text value "IRLL2705" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 9ed61060-1e9a-4f51-a038-46b48913a3da)
    )
    (fp_line (start -3.15 1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 63582672-d42c-44d8-b6ee-a127c96a5d6d))
    (fp_line (start -3.15 -1.75) (end 3.15 -1.75) (layer "F.SilkS") (width 0.12) (tstamp 64af8c89-1100-4d19-87e6-058c06df79b9))
    (fp_line (start 3.15 -1.75) (end 3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp 80ba080a-8964-431c-b673-5fc27b98993e))
    (fp_line (start -3.15 -1.75) (end -3.15 1.75) (layer "F.SilkS") (width 0.12) (tstamp fd91fb6c-305f-47bb-8f11-1c5e9d7cffdd))
    (pad "1" smd rect locked (at -2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(Q3-Pad1)") (pinfunction "G") (pintype "input") (tstamp c0a21c49-26a1-4900-a410-f577ae616ee5))
    (pad "2" smd rect locked (at 0 -3.25) (size 4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(Q3-Pad2)") (pinfunction "D") (pintype "input") (tstamp 92bacd6b-5d92-48d8-a5d2-0827205f5f95))
    (pad "2" smd rect locked (at 0 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(Q3-Pad2)") (pinfunction "D") (pintype "input") (tstamp f31b80eb-66c6-48a7-b986-a583828da73c))
    (pad "3" smd rect locked (at 2.3 3.25) (size 1.4 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(Q3-Pad3)") (pinfunction "S") (pintype "input") (tstamp 4650d9b4-32bc-4c82-9182-e7a6ea3bd730))
    (model "${MY_PATH}/3D/U.3dshapes/SOT-223.step"
      (offset (xyz -0.35 -11.5 -8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp aa104dab-213e-4064-b04c-c842429167ea)
    (at 106.06 49.675)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061127f03")
    (attr through_hole)
    (fp_text reference "Q14" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp befcc9d7-09ce-409a-80b5-6edf74c83f9f)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1daaee6-ecc3-4ba6-aea4-821f5d0861ee)
    )
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 3efa0975-a611-4e86-83b6-178cf9beec6c))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 97283c44-3cd8-4ac6-adff-2e8af5a9f576))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp b7318ab4-f12d-458f-8435-61b23da565e7))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp d7e27dda-31f2-465a-9db4-fe4a6fdd9944))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(Q14-Pad1)") (pintype "input") (tstamp 3805a62c-bb3a-4cf0-a961-5b247ccd9c34))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/Flo_BAS") (pintype "input") (tstamp 2ebc0d7a-3039-42ca-b1d6-963d16d648ae))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(Q14-Pad3)") (pintype "input") (tstamp 44bf90f3-63f7-41f2-8b5d-410a606c7236))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp ad667f14-8a85-4c6f-804e-44ef55a18a14)
    (at 95.6 53.395)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/d7c047b2-dcd3-4c84-bce0-f88914740f32")
    (attr through_hole)
    (fp_text reference "P8" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 37bd82bb-839a-4c3f-93a6-d5a68c79d6d0)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp db33ea26-6bef-4cbc-86db-bd5c21af9d14)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp bcaf731d-2ff4-4181-a39c-ddac459d33d1))
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp b09151db-6573-4202-ac2d-88eaed352bd2)
    (at 88.54 67.605)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000611654dd")
    (attr through_hole)
    (fp_text reference "Q16" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 26c8371f-c321-4263-ba11-5519c9921673)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d12b4ea1-ce0c-4c36-89d0-ac3beef7a622)
    )
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 37a0dfd5-2742-4e80-83f8-d947c25f1be2))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 60ad4d9d-cfad-46b9-bf1a-74a38833ec09))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp b5b6c8fc-f8ab-49ae-84c2-bb62bd5d46d3))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp e4a5c716-c3cb-4eeb-9ce5-198f5651080a))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(Q16-Pad1)") (pintype "input") (tstamp cd4a0a06-8538-4725-8d48-22af47385de8))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/Cro_BAS") (pintype "input") (tstamp c786cd34-1a93-4ba6-b989-e31b08dca182))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(Q16-Pad3)") (pintype "input") (tstamp 7c54f6b5-4389-4663-ad84-680d7b8845fc))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp b2f2a913-d3f8-4f37-97e3-9f870b10b7ad)
    (at 114.87 43.18)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061250136")
    (attr through_hole)
    (fp_text reference "R24" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 6a98b26c-2d88-4a26-86f7-baf5e313f17b)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp eec8e350-17cf-4cff-b5bc-6c42ffd394ec)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 10dd9b28-0d0a-48f6-8ff8-fd76a592a560))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp f99a885b-2ed1-4782-849e-e144fb7f20a1))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/Cro_HAUT_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 3216a875-4f9d-4877-9866-ff427a8490ad))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(Q13-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 8cf103a4-e96c-4391-a7a7-332a06b35888))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp b355f603-ef82-4c09-9847-373eff8fc858)
    (at 120.53 34.495)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/97510556-b979-4c8e-b357-f1c993b52101")
    (attr through_hole)
    (fp_text reference "Q6" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 1b7040c2-f711-4d6a-b8a8-7ed733b1e60c)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a277d064-ff43-4806-a2bf-8d41350e25d7)
    )
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 14ec098c-8d39-4469-9f34-96dc8ce5acfd))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 472c220d-0a19-4223-aa3d-71d45cc31264))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp c4f17039-7857-481c-a95b-ebb4d97b1c60))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp fa40f392-03c1-4703-b1a7-b5530f1cfafd))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(Q6-Pad1)") (pintype "input") (tstamp 69f878e2-6b57-4b56-afb2-28314d5361c9))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "input") (tstamp 8bb5e468-f1c0-4a60-8b95-ebc3794d2d66))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/Vent2") (pintype "input") (tstamp 663a4928-7227-47d0-b50c-4617541c8aa9))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp b5341834-4d7e-4b40-89ba-faf79f0764f2)
    (at 103.79 58.18)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/1730e9d9-36f1-49d1-bbf1-e1f74510417e")
    (attr through_hole)
    (fp_text reference "R2" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 675b33d9-5877-4349-9857-33e794c124cd)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp ecbac94a-b63c-463b-ae8a-eaee8b37a8d3)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 37ec81b1-4be0-414e-897e-ed8336061671))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp a5f836f3-0dea-4cfc-80ce-eba0524f90ca))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c1d9b46c-7650-477d-8b14-1c52ba340079))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/RST") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 01e76237-763e-4e7f-9a94-796b775fb5d2))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp bc543c7c-ecec-497e-8f9b-43d03302d06b)
    (at 90.05 73.45)
    (property "Partkeepr" "0607")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b5a2")
    (attr through_hole)
    (fp_text reference "C8" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 22cec2a3-bd07-4aaf-a0de-20291a7083cc)
    )
    (fp_text value "4.7µF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 3dde6147-099c-4b2d-a678-dba151ab8ad1)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 2930533e-c6b5-41f2-b368-547d52d77638))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 52a18a93-b0b2-45f5-a5cd-c592d1922e34))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp e78de33f-ef78-4da0-aaf3-2b2526dcde66))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 7177c4cb-2388-4363-aa5d-a4c51a1fcc96))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Y:5032" (layer "F.Cu")
    (tedit 61B9BBFE) (tstamp bcf686af-bf54-430b-b891-3f30940ec426)
    (at 46.46 78.66)
    (property "Partkeepr" "1650")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b53a")
    (attr through_hole)
    (fp_text reference "Y1" (at 0 2.2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9770c81d-e93f-478b-ace3-e98d8795e39d)
    )
    (fp_text value "25Mhz" (at 0 -2.15) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9fda9c77-43d9-4b85-aadf-ca44cfcc6423)
    )
    (fp_line (start -0.75 -1.25) (end 0.75 -1.25) (layer "F.SilkS") (width 0.17) (tstamp 68de6408-f63b-42d1-a3ed-fecd3e3faa5a))
    (fp_line (start -0.75 1.25) (end 0.75 1.25) (layer "F.SilkS") (width 0.17) (tstamp bf296e16-c22a-4300-bc39-8951c2acc807))
    (pad "1" smd rect locked (at -1.85 0) (size 1.7 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 201096f8-3131-4eb5-8525-f58be9a1ef52))
    (pad "2" smd rect locked (at 1.85 0) (size 1.7 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C4-Pad1)") (pinfunction "2") (pintype "passive") (tstamp a433a0f3-ddf0-4c4d-8fbd-c2c959db46c3))
    (model "${MY_PATH}/3D/Y.3dshapes/5032.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp bd6aa9ed-5080-4124-9951-97be88893ee4)
    (at 89.32 76.12)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/bfd26f61-39c9-4461-be5d-dcc8900f2a8a")
    (attr through_hole)
    (fp_text reference "C2" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 485c9751-8aa6-46ce-843e-e3b38aec1c83)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp bec314c6-8c55-4e99-936d-317079ce945b)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 3f20cb66-38a1-4fd5-aa6e-e358c0622e56))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp bfb2992f-7fa8-48dd-8e24-b1ce6da518f6))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 968dd469-d5bf-4940-b824-76f3536084b1))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp c46b3742-e79a-4fd2-8898-c5a8421ac6c2))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MH:MH3mm5" (layer "F.Cu")
    (tedit 5CE7D089) (tstamp bdba7610-0415-4993-913c-de2aef5184a6)
    (at 100.6 53.395)
    (descr "module Non Plated Through Hole")
    (tags "DEV")
    (property "Partkeepr" "NA")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/4fc7d59e-2928-4cf2-8aff-3697086090ef")
    (attr through_hole)
    (fp_text reference "P7" (at -3.81 2.54) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp 4e9dd392-ebe0-46ff-ad48-df4dd6f00c5f)
    )
    (fp_text value "MH1" (at 0 0) (layer "Cmts.User") hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
      (tstamp a73f2daa-f636-474d-970b-bc9b391dddcc)
    )
    (pad "" np_thru_hole circle locked (at 0 0) (size 4 4) (drill 3.6) (layers *.Cu *.Mask) (tstamp 5a8c6202-1f35-4490-94b5-130e62407a90))
  )

  (footprint "Bornier:Bornier5_1x2" (layer "F.Cu")
    (tedit 5B362772) (tstamp be35e975-feee-47a3-b125-998ae6c40d67)
    (at 90.09 44.81)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061474a30")
    (attr through_hole)
    (fp_text reference "P6" (at 0.381 4.572) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp db4b2fc3-17f4-49ec-aa32-5cbdbdb04f49)
    )
    (fp_text value "IN_230V" (at 0.381 -3.556) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d225be94-f09e-4ba8-a716-04d233acc442)
    )
    (fp_line (start 5.969 -2.54) (end 5.969 3.556) (layer "F.SilkS") (width 0.15) (tstamp 94ff9f06-f95b-45e0-a71e-b5ef9fb12327))
    (fp_line (start 5.969 2.54) (end -5.715 2.54) (layer "F.SilkS") (width 0.15) (tstamp adb1d0e5-a730-467c-9961-fd59bbec440b))
    (fp_line (start -5.715 3.556) (end 5.969 3.556) (layer "F.SilkS") (width 0.15) (tstamp b5eae7f3-2cd7-4f0f-97cc-87b27f713549))
    (fp_line (start -5.667 -2.5) (end -5.667 3.5) (layer "F.SilkS") (width 0.15) (tstamp f6b1d67e-3472-4066-b9ff-b358d1036470))
    (fp_line (start -5.715 -2.54) (end 5.969 -2.54) (layer "F.SilkS") (width 0.15) (tstamp f8a4705a-bda0-49f1-ba6c-ba2437f4ec39))
    (pad "1" thru_hole rect locked (at -2.667 0) (size 4 4) (drill 1.1) (layers *.Cu *.Mask "F.SilkS")
      (net 24 "/230V") (pinfunction "P1") (pintype "passive") (tstamp 3e0e49d1-ba06-4cba-a8bc-e3d8054af0e2))
    (pad "2" thru_hole circle locked (at 2.413 0) (size 4 4) (drill 1.1) (layers *.Cu *.Mask "F.SilkS")
      (net 30 "/Neutre") (pinfunction "P2") (pintype "passive") (tstamp 15cfbe41-3b94-479f-a852-a10223923710))
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp be4ca92a-4550-49c8-9129-8a2d68227d22)
    (at 81.91 77.035)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/14a26789-33a4-4b2d-ad64-2339c90d97f7")
    (attr through_hole)
    (fp_text reference "Q7" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp 0b7907dc-d57d-4dbf-9540-b595b6a7094e)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 83138aa8-0b69-45ab-adba-2beaab82e0f4)
    )
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 18753467-df7c-4c7f-ab5c-a79c3dc893f6))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 60db04dd-7c0c-410e-80f3-28122140546e))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 621f39d5-e336-4dd5-a884-a773745674ea))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp b0971e86-ebfc-4336-acbc-c6b3eeb40df9))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(Q7-Pad1)") (pintype "input") (tstamp 429a4fae-4338-4953-835c-2337efec04ac))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp a53a4415-27b1-4b3f-a4c5-e5968cf004d0))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D1-Pad2)") (pintype "input") (tstamp 5b3e8d97-031b-4be7-9fa4-3f14496b383c))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp be659624-1a86-4883-b7a5-a48eba4cab04)
    (at 132.04 26.875)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006176c1b4")
    (attr through_hole)
    (fp_text reference "Q9" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp bef88720-f8dd-482c-86d3-8febc665abdf)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2ded20e1-7656-40bb-a81b-9ec1b325c898)
    )
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 665704b6-8373-40c8-9e65-4e6e356b6da6))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 86d2649d-303f-4c97-8b31-69e5e5a1b27c))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp a5c0ba8f-2d16-4814-b766-2055bf9d6a65))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp ba71ad91-db0d-4da7-a56d-4ef96eca379d))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(Q9-Pad1)") (pintype "input") (tstamp 50052b7d-dfec-42b4-a05f-a7f53da9bb33))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp 8edbe203-2758-40e3-9c25-d0320861e4c5))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad2)") (pintype "input") (tstamp d727421e-a6e0-492b-b098-e28d1ef03ab5))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0603" (layer "F.Cu")
    (tedit 61B9ACFA) (tstamp c5fe7f60-31ad-4169-9bf7-335d380e40e8)
    (at 106.72 60.59)
    (property "Partkeepr" "0600")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b541")
    (attr through_hole)
    (fp_text reference "C4" (at 0 1.3 180) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp 8df407e1-9aae-44d5-b685-5a52edde0e13)
    )
    (fp_text value "22pF" (at -0.7 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 10bbca11-e8fc-4a33-8804-b4c1efa86f22)
    )
    (fp_line (start 0.2 0.5) (end -0.2 0.5) (layer "F.SilkS") (width 0.17) (tstamp 7c38aae0-6ee2-45f0-a256-a4b1a62427a8))
    (fp_line (start -0.2 -0.49) (end 0.2 -0.49) (layer "F.SilkS") (width 0.17) (tstamp d6b23f09-ea95-413f-b099-4bf267ed9da9))
    (pad "1" smd rect (at 0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C4-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6441fea3-67cc-4bea-a1f6-6eada30d3ae5))
    (pad "2" smd rect (at -0.7 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d36f0854-c190-4311-b3b9-c85cb211caba))
    (model "${MY_PATH}/3D/C.3dshapes/0603.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp d3943950-a977-49bc-9f95-b1cefe3819e5)
    (at 129.75 30.05)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b4f8")
    (attr through_hole)
    (fp_text reference "C15" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 84ccee49-52ac-4af2-93c6-4173f14cec70)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp fb330e31-1105-4ade-8ead-80156583fb69)
    )
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp 53a88e15-f761-4e8e-8937-fb440b988783))
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp ac0bd238-c122-4698-a68a-87d521401884))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d719e131-e77e-485f-a34b-4c1ec9d176b1))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/nrst") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp a7310354-2185-42b8-8bb5-4e2862d00f34))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp d56effe6-0b67-4a10-92f6-926afe90c2b9)
    (at 90.05 70.79)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d46")
    (attr through_hole)
    (fp_text reference "R12" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 5234c975-3be0-4a00-a1f4-3f7973d29c73)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp 9c134d1c-017e-49b2-bc0f-88d3ffc087db)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 07789fb9-b22b-4b32-826f-d081f0eb9dd6))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 6f21b260-d52e-41ef-9f5e-9e7bb9b8c1d7))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(Q8-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp aabf668a-880c-4363-b513-7fa109fa304b))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/230V_2_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 1e69ccea-8127-4a51-8711-03214331a177))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp e20fba59-4ac9-4c6f-bf95-daa101e0dc4c)
    (at 139.45 26.36)
    (property "Partkeepr" "0910")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/337f1538-9f0d-4286-a918-99960bd9148c")
    (attr through_hole)
    (fp_text reference "R21" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 0738bd9d-9b16-48ed-a2b0-81ef90fa0698)
    )
    (fp_text value "10K" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp df773e1c-fe54-47b9-a120-f523c9f2ebaa)
    )
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 0a5e77e5-3824-41e8-8dc8-de534428cefd))
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 363314aa-0095-4289-8248-7773756e1b24))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 6b56afaf-68f7-4e1c-bb9b-34745fc9c6ba))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/sdl") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp cc8ac10a-0223-4128-8eaf-5d45ffc6de02))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "D:SOD-123" (layer "F.Cu")
    (tedit 61B9B30C) (tstamp f670bdfe-33c3-44cc-aece-970db0638046)
    (at 127.29 26.585)
    (property "Partkeepr" "1300")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d5f")
    (attr through_hole)
    (fp_text reference "D2" (at 0 1.6) (layer "F.SilkS")
      (effects (font (size 0.9 0.7) (thickness 0.17)))
      (tstamp e2d28ec2-5d38-4f52-a460-3c028e66618d)
    )
    (fp_text value "1N4148W" (at 0 -0.0127) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
      (tstamp 289b3bd5-0d82-4c1b-bc25-849697b6afdd)
    )
    (fp_line (start -1.08 -0.8) (end -1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 4c6b61ec-9cb5-4c44-b58e-643eeacf170b))
    (fp_line (start 1.905 -0.762) (end 2.159 -0.762) (layer "F.SilkS") (width 0.17) (tstamp 5c98226c-1412-408d-b38d-578176d99d0d))
    (fp_line (start 1.08 -0.8) (end 1.08 0.8) (layer "F.SilkS") (width 0.17) (tstamp 6c1d013d-af9e-4d37-9d31-f9051468282a))
    (fp_line (start -2.6 -1) (end -2.6 -0.6) (layer "F.SilkS") (width 0.12) (tstamp 96768ad9-fff5-46bc-b2ea-5a2da344d591))
    (fp_line (start -2.8 -0.8) (end -2.4 -0.8) (layer "F.SilkS") (width 0.12) (tstamp 9791cc58-be59-4243-9ee6-e652ec8112cf))
    (pad "1" smd rect locked (at -1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pinfunction "K") (pintype "passive") (tstamp 97b4baa5-81e1-478a-b8b3-af8defed0fc7))
    (pad "2" smd rect locked (at 1.64 0) (size 0.91 1.22) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp e5cbcb8d-bdd7-4d0e-a86b-ba1dec300ba4))
    (model "${MY_PATH}/3D/D.3dshapes/SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "R:0805" (layer "F.Cu")
    (tedit 61B891DF) (tstamp f68b2d11-8363-4660-92bb-676cb38c0574)
    (at 85.72 76.52)
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006182a897")
    (attr through_hole)
    (fp_text reference "R8" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp 937a01a0-3649-4c5e-ac90-5526f4275a82)
    )
    (fp_text value "R" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp ce681be8-3f89-4eaa-8f1b-f282cb09c3e2)
    )
    (fp_line (start -0.25 -0.75) (end 0.25 -0.75) (layer "F.SilkS") (width 0.17) (tstamp 0482bbae-a4e4-4a4a-998a-196c5fc8bfa5))
    (fp_line (start -0.25 0.75) (end 0.25 0.75) (layer "F.SilkS") (width 0.17) (tstamp 810fc2c6-816c-4a09-99e2-4259fb4b26e1))
    (pad "1" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(Q4-Pad1)") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp d13466e0-71da-4aa0-a22f-40f7a9b030d1))
    (pad "2" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/12V_4_IN") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 4907dda2-9743-40a3-b95f-5e5b0267d2a9))
    (model "${MY_PATH}/3D/R.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "C:0805" (layer "F.Cu")
    (tedit 60D1E9D4) (tstamp fa6a567b-9542-4c0c-878c-c9a1e894e7c2)
    (at 118.47 43.17)
    (property "Partkeepr" "0605")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006104b551")
    (attr through_hole)
    (fp_text reference "C13" (at 0 1.4 180) (layer "F.SilkS")
      (effects (font (size 0.7 0.66) (thickness 0.16)))
      (tstamp c23707a1-c334-4096-ac11-dc8949aa7f69)
    )
    (fp_text value "100nF" (at -0.875 0 90) (layer "F.Fab")
      (effects (font (size 0.3 0.2) (thickness 0.05)))
      (tstamp ef1b1d40-4ccd-4995-81c1-007577e0393d)
    )
    (fp_line (start 0.3 -0.74) (end -0.3 -0.74) (layer "F.SilkS") (width 0.17) (tstamp 03620659-b3b7-4e8a-bfbe-855d33a397bf))
    (fp_line (start 0.3 0.74) (end -0.3 0.74) (layer "F.SilkS") (width 0.17) (tstamp d4b730f1-f24a-42b8-ae21-2f541bcd7c61))
    (pad "1" smd rect (at 0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/3.3V") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 31d5d251-2654-4aef-a479-13369fa20917))
    (pad "2" smd rect (at -0.875 0) (size 0.85 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "passive") (solder_mask_margin 0.07) (solder_paste_margin -0.05) (tstamp 41f33ee8-65b0-4cea-9af9-4d83b3104c97))
    (model "${MY_PATH}/3D/C.3dshapes/0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp fc7cf0f9-846a-4a98-b693-0a1096c98a3e)
    (at 95.96 61.445)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00006171fa7e")
    (attr through_hole)
    (fp_text reference "Q10" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp c8fe25ad-97f8-4351-95ad-eebdde7ddb8a)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f73e11a-25fd-40df-bbbd-49f0052860dd)
    )
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 33a1689a-8bd5-41d6-8c71-0e551d55df8e))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 38b08e0d-04b3-4464-b569-c6fd2d2cc0c7))
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 73b795ba-5c45-4eb8-afb1-f880ebfe1c0d))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 9d50b27f-2920-4656-8fee-9cba8ffac7d1))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(Q10-Pad1)") (pintype "input") (tstamp 1f751859-8cd6-4571-a886-d69e62053d08))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp d178550a-c013-418a-a430-d0ec09485fe5))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D4-Pad2)") (pintype "input") (tstamp 351d11d9-fdb0-4bb8-8555-c1521117360c))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "U:SOT23-3" (layer "F.Cu")
    (tedit 61B89090) (tstamp fc8ac205-d097-47c7-aca5-0c9632c3cbe6)
    (at 111.06 48.375)
    (property "Partkeepr" "2550")
    (property "Sheetfile" "ProcCult.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000061773d4d")
    (attr through_hole)
    (fp_text reference "Q8" (at 2 0 90) (layer "F.SilkS")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
      (tstamp c49b1532-05ea-4971-91e9-dac73f02cd05)
    )
    (fp_text value "NPN_2222A" (at 0 2.31) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3fabb85-91a2-4f17-bb05-ee63be0774e7)
    )
    (fp_line (start -1.45 -0.5) (end 1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 31441e30-1d54-46bf-a918-93282e28c764))
    (fp_line (start 1.45 0.5) (end -1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp 57e989ea-77a5-4cbb-a367-25fdeaf8aec1))
    (fp_line (start -1.45 0.5) (end -1.45 -0.5) (layer "F.SilkS") (width 0.12) (tstamp 8175cdfb-9b9b-4ebe-9796-a22c2b722064))
    (fp_line (start 1.45 -0.5) (end 1.45 0.5) (layer "F.SilkS") (width 0.12) (tstamp a79d404e-b68d-4c93-836b-433d0c5ee16d))
    (pad "1" smd rect (at -0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(Q8-Pad1)") (pintype "input") (tstamp 6adab893-2116-493f-8655-dc835680a076))
    (pad "2" smd rect (at 0.95 1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pintype "input") (tstamp faac7634-4bee-4e44-9fcb-517c11567cd4))
    (pad "3" smd rect (at 0 -1) (size 0.6 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D2-Pad2)") (pintype "input") (tstamp 5edc49e0-8caf-4b5d-b292-2940da6d68a4))
    (model "${MY_PATH}/3D/U.3dshapes/SOT23-3.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
