{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["IO","Alim"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"IO","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Nom","Type","PIN","Com","Couleurs"]
["RougeHaut","O",2]
["RougeBas","O",3]
["BleuHaut","O",4]
["BleuBas","O",5]
["TousHaut","O",6]
["TousBas","O",7]
["Dehumidificateur","O",8]
["VentilHaut","O",9]
["VentilBas",null,10]
["Extraction","O",11]
["Arro","O",12]
["Evacuation","O",13]
["interType","I",22,"Flo/Cro","Bleu"]
["interLum","I",24,"Extinxtion Lumiere","Blanc"]
["interONExt","I",26,"Extraction Auto/ON","Gris rose"]
["interONVentil","I",28,"Ventilation Auto/ON","Rouge bleu"]
["interOFFExt","I",30,"Extraction ventilation Off","violet"]
["interONAro","I",32,"Arrosage Auto/On","rose"]
["interONVid","I",34,"Vidange Auto/On","jaune"]
["interOFFAro","I",36,"Arrosage Vidange Off","marron"]
["Inter9","I",38,null,"Vert"]
["Inter10","I",40,null,"Gris"]
["HumidSolCroi","I",16]
["HumidSolFlo","I",17]
["RTC","I2C","20/21"]
["Temp","Onewire",14]
["Humi","Autres",15]

{"sheet":"Alim","index":1,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Relais rouge"]
["Relais bleu"]
["Relais Ventilation"]
["Relais arrosage"]
["Inter","Avec pull up"]
["HumidSolCroi"]
["HumidFloFlo"]
["RTC"]
["Temp"]
["Humi"]