{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["IO","Alim"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"IO","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Nom","Type","PIN","Com","Couleurs"]
["Haut","O",2]
["Bas","O",3]
["Ventil","O",4]
["Arro","O",5]
["interLumBas","I",6,"Lumiere bas ON/OFF"]
["interLumOff","I",7,"Lumiere OFF"]
["interVentAuto","I",8,"Ventilation ON/Auto"]
["interVentOff","I",9,"Ventilation OFF"]
["interArroAuto","I",10,"Arro ON/Auto"]
["interArroOff","I",11,"Arro OFF"]
["Inter7","I",12]
["RTC","I2C"]

{"sheet":"Alim","index":1,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Relais rouge"]
["Relais bleu"]
["Relais Ventilation"]
["Relais arrosage"]
["Inter","Avec pull up"]
["HumidSolCroi"]
["HumidFloFlo"]
["RTC"]
["Temp"]
["Humi"]