{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["IO","Alim"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"IO","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Nom","Type","PIN","Com","Couleurs"]
["Rouge1","O",3]
["Rouge2","O",4]
["Bleu1","O",5]
["Bleu2","O",6]
["Bleu3","O",7]
["Dehumidificateur","O",8]
["Ventilation","O",9]
["Extraction","O",10]
["ArrosageFlo","O",11]
["ArrosageCro","O",12]
["Evacuation","O",13]
["Inter1","I",22,"Extinxtion Lumiere","Bleu"]
["Inter2","I",24,"Marche forcé Extraction","Blanc"]
["Inter3","I",26,"60%/70 %","Gris rose"]
["Inter4","I",28,"Lum Mere","Rouge bleu"]
["Inter5","I",30,null,"violet"]
["Inter6","I",32,"Alum ArrossageFlo","rose"]
["Inter7","I",34,"Alum ArrosageCro","jaune"]
["Inter8","I",36,"Pompe vidange","marron"]
["Inter9","I",38,"ArrosageFlo Auto","Vert"]
["Inter10","I",40,"ArrosageCro Auto","Gris"]
["HumidSolCroi","I",46]
["HumidSolFlo","I",48]
["RTC","I2C","20/21"]
["Temp","Onewire",14]
["Humi","Onewire",15]

{"sheet":"Alim","index":1,"n_rows":10,"n_cols":2,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Relais rouge"]
["Relais bleu"]
["Relais Ventilation"]
["Relais arrosage"]
["Inter","Avec pull up"]
["HumidSolCroi"]
["HumidFloFlo"]
["RTC"]
["Temp"]
["Humi"]