(module NEO-7 (layer F.Cu) (tedit 60DDE4A9)
  (fp_text reference REF** (at 4 9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NEO-7 (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.1 8) (end 6.1 8) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.1 8) (end 6.1 -8) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.1 -8) (end -6.1 -8) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.1 -8) (end -6.1 8) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at 6 7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 6 5.9) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 6 4.8) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 6 3.7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 6 2.6) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 6 1.5) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 6 0.4) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 6 -2.6) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 6 -3.7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 6 -4.8) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 6 -5.9) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 6 -7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -6 1.5) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -6 -4.8) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -6 3.7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at -6 4.8) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -6 2.6) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -6 -5.9) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -6 -7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -6 -0.7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -6 -3.7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at -6 7) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at -6 5.9) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -6 0.4) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask))
  (model ${MY_PATH}/3D/module.3dshapes/NEO-7.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
