(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)

  (general
    (thickness 1.6)
    (drawings 45)
    (tracks 0)
    (zones 0)
    (modules 9)
    (nets 38)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 12.192 197.866)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /Terre)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J2-Pad5)")
  (net 9 "Net-(J2-Pad6)")
  (net 10 "Net-(J2-Pad7)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad9)")
  (net 13 "Net-(J2-Pad10)")
  (net 14 "Net-(P1-Pad4)")
  (net 15 "Net-(P1-Pad2)")
  (net 16 "Net-(P1-Pad3)")
  (net 17 "Net-(P1-Pad1)")
  (net 18 "Net-(P2-Pad4)")
  (net 19 "Net-(P2-Pad2)")
  (net 20 "Net-(P2-Pad3)")
  (net 21 "Net-(P2-Pad1)")
  (net 22 "Net-(P3-Pad4)")
  (net 23 "Net-(P3-Pad2)")
  (net 24 "Net-(P3-Pad3)")
  (net 25 "Net-(P3-Pad1)")
  (net 26 "Net-(P4-Pad1)")
  (net 27 "Net-(P4-Pad2)")
  (net 28 "Net-(P4-Pad3)")
  (net 29 "Net-(P4-Pad4)")
  (net 30 "Net-(P5-Pad1)")
  (net 31 "Net-(P5-Pad2)")
  (net 32 "Net-(P5-Pad3)")
  (net 33 "Net-(P5-Pad4)")
  (net 34 "Net-(P6-Pad1)")
  (net 35 "Net-(P6-Pad2)")
  (net 36 "Net-(P6-Pad3)")
  (net 37 "Net-(P6-Pad4)")

  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Terre)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1R_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1ECD) (tstamp 5FC12438)
    (at 177.9 78.9)
    (descr "MSTBO 2,5 G1R 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1R")
    (path /5FC14CD7)
    (fp_text reference P6 (at 0 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.Fab) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 34 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 35 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 36 "Net-(P6-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 37 "Net-(P6-Pad4)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1R_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1R_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1ECD) (tstamp 5FC12415)
    (at 170.8 62.5)
    (descr "MSTBO 2,5 G1R 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1R")
    (path /5FC156CD)
    (fp_text reference P5 (at 0 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.Fab) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 30 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 31 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 32 "Net-(P5-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 33 "Net-(P5-Pad4)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1R_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1R_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1ECD) (tstamp 5FC123F2)
    (at 163.7 46.1)
    (descr "MSTBO 2,5 G1R 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1R")
    (path /5FC15BB9)
    (fp_text reference P4 (at 0 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.Fab) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start 3.6 1.15) (end 3.6 2.35) (angle 90) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.5 -9.2) (end 2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 2.4 -9.2) (end 2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 3.6 2.35) (end 11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 2.35) (end 11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 11.7 6.1) (end 3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 6.1) (end 3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start 3.8 9.1) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -1.5 -9.2) (end -1.5 9.1) (layer F.Fab) (width 0.15))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 26 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 28 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 29 "Net-(P4-Pad4)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1R_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1L_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1F19) (tstamp 5FC123CF)
    (at 136.3 46.1)
    (descr "MSTBO 2,5 G1L 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1L")
    (path /5FC118BC)
    (fp_text reference P3 (at -0.508 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.CrtYd) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.SilkS) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 "Net-(P3-Pad4)"))
    (pad 2 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 23 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad3)"))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad1)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1L_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1L_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1F19) (tstamp 5FC123AC)
    (at 129.2 62.5)
    (descr "MSTBO 2,5 G1L 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1L")
    (path /5FC121C3)
    (fp_text reference P2 (at -0.508 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.CrtYd) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.SilkS) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad4)"))
    (pad 2 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad3)"))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad1)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1L_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Phoenix:PhoenixContact_MSTBO_2,5_4-G1L_1x4_p5.00mm (layer F.Cu) (tedit 5B3A1F19) (tstamp 5FC12389)
    (at 122.1 78.9)
    (descr "MSTBO 2,5 G1L 1x4 p5.00mm")
    (tags "Connector Phoenix Contact MSTBO G1L")
    (path /5FC12A34)
    (fp_text reference P1 (at -0.508 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X04 (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.CrtYd) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.SilkS) (width 0.15))
    (fp_arc (start -3.6 1.15) (end -3.6 2.35) (angle -90) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.Fab) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.Fab) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.Fab) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.5 -9.2) (end -2.4 -9.2) (layer F.CrtYd) (width 0.15))
    (fp_line (start -2.4 -9.2) (end -2.4 1.15) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.6 2.35) (end -11.7 2.35) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 2.35) (end -11.7 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -11.7 6.1) (end -3.8 6.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 6.1) (end -3.8 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start -3.8 9.1) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (fp_line (start 1.5 -9.2) (end 1.5 9.1) (layer F.CrtYd) (width 0.15))
    (pad 4 thru_hole circle (at 0 7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad4)"))
    (pad 2 thru_hole circle (at 0 2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -7.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad3)"))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad1)"))
    (model ${KIPRJMOD}/Connector_Phoenix_MSTBO.3Dshapes/PhoenixContact_MSTBO_2,5_4-G1L_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PCBEdge:PCBEdge_1x1_6x3mm (layer F.Cu) (tedit 5B3A358F) (tstamp 5B4436A2)
    (at 170.05 146)
    (path /5B39F362)
    (fp_text reference J3 (at 0 -4.826) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value EARTH (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.032 4.064) (end -2.032 -4.064) (layer F.CrtYd) (width 0.15))
    (fp_line (start 2.032 4.064) (end -2.032 4.064) (layer F.CrtYd) (width 0.15))
    (fp_line (start 2.032 -4.064) (end 2.032 4.064) (layer F.CrtYd) (width 0.15))
    (fp_line (start -2.032 -4.064) (end 2.032 -4.064) (layer F.CrtYd) (width 0.15))
    (fp_line (start -2.032 4.064) (end -2.032 -4.064) (layer B.CrtYd) (width 0.15))
    (fp_line (start 2.032 4.064) (end -2.032 4.064) (layer B.CrtYd) (width 0.15))
    (fp_line (start 2.032 -4.064) (end 2.032 4.064) (layer B.CrtYd) (width 0.15))
    (fp_line (start -2.032 -4.064) (end 2.032 -4.064) (layer B.CrtYd) (width 0.15))
    (pad 1 smd rect (at 0 0) (size 3 6) (layers F.Cu F.Paste F.Mask)
      (net 1 /Terre))
    (pad 1 smd rect (at 0 0) (size 3 6) (layers B.Cu B.Paste B.Mask)
      (net 1 /Terre))
  )

  (module PCBEdge:PCBEdge_1x10_5.7x2.21mm_p3.81mm (layer F.Cu) (tedit 5B3A35E0) (tstamp 5B44369C)
    (at 146.95 135.9)
    (path /5B39F28C)
    (fp_text reference J2 (at 0 -4.572) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DATA (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 19.05 -3.556) (end 19.05 3.556) (layer F.CrtYd) (width 0.15))
    (fp_line (start -19.05 3.556) (end -19.05 -3.556) (layer F.CrtYd) (width 0.15))
    (fp_line (start -19.05 3.556) (end 19.05 3.556) (layer F.CrtYd) (width 0.15))
    (fp_line (start 19.05 -3.556) (end -19.05 -3.556) (layer F.CrtYd) (width 0.15))
    (fp_line (start 19.05 -3.556) (end -19.05 -3.556) (layer B.CrtYd) (width 0.15))
    (fp_line (start 19.05 3.556) (end 19.05 -3.556) (layer B.CrtYd) (width 0.15))
    (fp_line (start -19.05 3.556) (end 19.05 3.556) (layer B.CrtYd) (width 0.15))
    (fp_line (start -19.05 -3.556) (end -19.05 3.556) (layer B.CrtYd) (width 0.15))
    (pad 1 smd rect (at -17.145 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -13.335 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -9.525 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -5.715 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -1.905 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at 1.905 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 5.715 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at 9.525 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at 13.335 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad9)"))
    (pad 10 smd rect (at 17.145 0) (size 2.21 5.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 1 smd rect (at -17.145 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -13.335 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -9.525 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -5.715 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -1.905 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at 1.905 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 5.715 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at 9.525 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at 13.335 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad9)"))
    (pad 10 smd rect (at 17.145 0) (size 2.21 5.7) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad10)"))
  )

  (module PCBEdge:PCBEdge_1x4_7.6x1.5mm_p1.9mm_2pins (layer F.Cu) (tedit 5B3A3610) (tstamp 5B443684)
    (at 120.24 134.95)
    (path /5B39F329)
    (fp_text reference J1 (at 0 -5.08) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PWR (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.064 -4.318) (end -4.064 4.318) (layer F.CrtYd) (width 0.15))
    (fp_line (start 4.064 -4.318) (end -4.064 -4.318) (layer F.CrtYd) (width 0.15))
    (fp_line (start 4.064 4.318) (end 4.064 -4.318) (layer F.CrtYd) (width 0.15))
    (fp_line (start -4.064 4.318) (end 4.064 4.318) (layer F.CrtYd) (width 0.15))
    (fp_line (start -4.064 -4.318) (end -4.064 4.318) (layer B.CrtYd) (width 0.15))
    (fp_line (start 4.064 -4.318) (end -4.064 -4.318) (layer B.CrtYd) (width 0.15))
    (fp_line (start 4.064 4.318) (end 4.064 -4.318) (layer B.CrtYd) (width 0.15))
    (fp_line (start -4.064 4.318) (end 4.064 4.318) (layer B.CrtYd) (width 0.15))
    (pad 1 smd rect (at -2.85 0) (size 1.5 7.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 1.5 7.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.5 7.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 2.85 0) (size 1.5 7.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2.85 0) (size 1.5 7.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 1.5 7.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.5 7.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 2.85 0) (size 1.5 7.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )

  (gr_arc (start 174.4 66.6) (end 173.2 66.6) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.3 51.4) (end 173.2 51.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.7 51.4) (end 126.8 51.4) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.7 50.2) (end 132.7 51.4) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 167.3 50.2) (end 166.1 50.2) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.6 67.8) (end 119.7 67.8) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 125.6 66.6) (end 125.6 67.8) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174.4 67.8) (end 180.3 67.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.1 50.2) (end 166.1 36.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.9 50.2) (end 133.9 36.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.3 67.8) (end 180.3 68.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.8 66.6) (end 126.8 53.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.8 51.4) (end 126.8 52.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.2 51.4) (end 173.2 52.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.2 66.6) (end 173.2 53.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.7 67.8) (end 119.7 68.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.75 139.25) (end 110 139.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.3 149.30718) (end 168.7 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.3 83) (end 180.3 69.7) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 181.5 83) (end 180.3 83) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.5 84.2) (end 188.72549 84.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190 86.7) (end 188.72549 84.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190 148) (end 190 86.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 188.845299 150) (end 190 148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 139.25) (end 110 138.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.27451 84.2) (end 110 86.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.5 84.2) (end 111.27451 84.2) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 118.5 83) (end 118.5 84.2) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.7 83) (end 119.7 69.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 86.7) (end 110 138.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.3 149.30718) (end 167.95 148.700962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.95 140.45) (end 167.95 148.700962) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.75 140.45) (end 167.95 140.45) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2 138.75) (end 111.2 85.1) (layer Cmts.User) (width 0.1))
  (gr_line (start 119.7 68.7) (end 119.7 69.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.8 52.3) (end 126.8 53.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.9 36.4) (end 133.9 36.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.1 36.4) (end 133.9 36.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.1 36.9) (end 166.1 36.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.2 53.3) (end 173.2 52.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.3 69.7) (end 180.3 68.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 188.8 85.1) (end 188.8 150) (layer Cmts.User) (width 0.1))
  (gr_line (start 188.8 150) (end 188.845299 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.7 150) (end 171.8 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.8 150) (end 188.8 150) (layer Edge.Cuts) (width 0.1))

)
