(module Micro-USB (layer F.Cu) (tedit 5B3625F1)
  (fp_text reference REF** (at 6.6 -1.7 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Micro-USB (at 0 4.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "A Supp" (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.675 -2.75) (end -3.675 1.75) (layer F.Fab) (width 0.15))
  (fp_line (start 3.675 -2.75) (end 3.675 1.75) (layer F.Fab) (width 0.15))
  (fp_line (start -3.675 -2.75) (end 3.675 -2.75) (layer F.Fab) (width 0.15))
  (fp_text user "PCB edge" (at 0 3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd rect (at -1.3 -3.825) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 -3.825) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -3.825) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.65 -3.825) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.3 -3.825) (size 0.4 1.05) (layers F.Cu F.Paste F.Mask))
  (pad 0 thru_hole oval (at -4.85 -3.3) (size 1.4 2.3) (drill oval 0.8 1.7) (layers *.Cu *.Mask))
  (pad 0 thru_hole oval (at -4.85 0) (size 1.4 2.3) (drill oval 0.8 1.7) (layers *.Cu *.Mask))
  (pad 0 thru_hole oval (at 4.85 0) (size 1.4 2.3) (drill oval 0.8 1.7) (layers *.Cu *.Mask))
  (pad 0 thru_hole oval (at 4.85 -3.3) (size 1.4 2.3) (drill oval 0.8 1.7) (layers *.Cu *.Mask))
)
