{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","Projet","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":16,"n_cols":11,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Nom","Commentaire","Version","Test","Proc","Drivers","Ordinateur","Fille","Ventilateur","Peristatique","GPS_MOTO"]
["EEPROM",null,"V2",null,"V1",null,"V1",null,null,"V1","V1"]
["Entre12V","Entrée securiser","V1","Nok","V1",null,"V1",null,"V1"]
["ESP12F",null,"V1",null,"V1",null,"V1",null,null,"V1"]
["LM317",null,"V1",null,"V1",null,"V1",null,null,"V1"]
["RTC",null,"V1",null,"V1",null,"V1",null,null,"V1"]
["STM32F0",null,"V1",{"$nulls":6},"V1"]
["STM32F4",null,"V1",null,"V1",null,"V1"]
["USB","USB pour stm32","V1",null,"V1",null,"V1",null,null,null,"V1"]
["HD44780","Driver LCD","V1",null,null,null,"V1",null,null,"V1"]
["MT-008A","Joystique","V1",null,null,null,"V1",null,null,"V1"]
["STM32L4","STM32 low energie","V1",{"$nulls":7},"V1"]
["GPS",null,"V1"]
["7 segment",null,"V1",{"$nulls":7},"V1"]
["STC4054","Chargeur Baterie","V1",{"$nulls":7},"V1"]
["STM32L476",null,"V1",{"$nulls":7},"V1"]

{"sheet":"Projet","index":1,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Nom","ID","Descrition"]
["Proc",1,"Carte de gestion des led d'aquarium"]
["Drivers",2,"Carte des drivers des led aquarium"]
["Ordinateur",3,"Carte de gestion du recifal"]
["Fille",4,"Carte fille des relais du recifal"]
["Ventilateur",5,"carte de gestion d'un ventilateur"]
["GPS_moto",6,"Carte gps pour moto"]

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}