{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["résolution PT1000 sans AOP"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"résolution PT1000 sans AOP","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,0,0,2],[5,0,5,3],[14,0,14,3]]}
[]
["tension de ref","nb bit","résolution volt","tension alim pt1000","résistance série PT1000 ",null,"mini résitance serie","maxi résitance série"]
[3.3,12,{"$f":"A3/POWER(2,B3)","v":8.0566406249999996E-4},3.3,43000,null,{"$f":"(D3/0.0001)-1000","v":32000},{"$f":"(D3/0.00001)-1000","v":328999.99999999994}]
[]
[]
[]
[null,null,null,"résolution max",null,null,"auto echauffement","K*R*I2"]
[{"$f":"D20+C3","v":8.2921575921049151E-2},{"$f":"A8*(E3/(D3-D20))","v":1108.0659423828124},{"$f":"B8-1097.3","v":10.765942382812455},{"$f":"1/(3.9/C8)","v":2.7604980468749885}]
{"$rows_empty":7}
["résolution voulue","résolution ohmique (PT1000)"]
[0.01,{"$f":"3.9*A17","v":3.9E-2}]
[]
[null,null,null,"mV"]
[null,null,1097.3,{"$f":"(D3*C20)/(E3+C20)","v":8.2115911858549148E-2}]
[null,null,{"$f":"C20+B17","v":1097.3389999999999},{"$f":"(D3*C21)/(E3+C21)","v":8.2118757778105372E-2}]
[null,null,"diff",{"$f":"D21-D20","v":2.8459195562241524E-6}]
[null,null,"doit etre sup a 1",{"$f":"D22/C3","v":3.5323898491800391E-3}]