{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Feuille1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuille1","index":0,"n_rows":4,"n_cols":6,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Endroit","Type","Iportance","Utilité","Réaction"]
["Cuve","Niveau Haut","Indispensable","Detecte si complication désente de l’eau","Stop Pompe de remonté Arrte Ecumage arret osmolation"]
["Technique","Niveau inter","Indispensable",null,"Demarre pompe osmolateur"]
["Reserve eau","Niveau Bas","Indispensable","Detecte niveau trop bas pour la cuve d’eau osmosé","Arrete la pompe d’eau osmosé","Peu etre remplacé par un timeout sur la technique inter"]