(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)

  (general
    (thickness 1.6)
    (drawings 87)
    (tracks 162)
    (zones 0)
    (modules 63)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.3)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.8 2.8)
    (pad_drill 2.8)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 47 34)
    (grid_origin 47 34)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Driver/"))
  )

  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(Q1-Pad1)")
  (net 5 "Net-(Q1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3BB9)
    (at 129.125 119 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3BB5)
    (at 117 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3BA8)
    (at 122 117.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3BA4)
    (at 142 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E3B8B)
    (at 137.1 117.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E3B7C)
    (at 130 101 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3B73)
    (at 129.125 116 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E3AFC)
    (at 104.1 117.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3AF0)
    (at 89 117.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3AE7)
    (at 96.125 116 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E3ACE)
    (at 97 101 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3AC6)
    (at 96.125 119 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3AC0)
    (at 109 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3AB9)
    (at 84 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3A54)
    (at 56 117.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3A50)
    (at 76 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3A46)
    (at 63.125 116 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3A42)
    (at 51 109)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3A3B)
    (at 63.125 119 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E3A24)
    (at 64 101 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E3A0C)
    (at 71.1 117.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E399C)
    (at 137.1 87.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E3992)
    (at 130 71 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3986)
    (at 122 87.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E397C)
    (at 117 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E396A)
    (at 129.125 89 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3962)
    (at 129.125 86 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E395D)
    (at 142 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E38FA)
    (at 96.125 89 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E38F6)
    (at 84 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E38ED)
    (at 97 71 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E38DA)
    (at 104.1 87.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E38D2)
    (at 96.125 86 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E38BF)
    (at 109 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E38A9)
    (at 89 87.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3849)
    (at 51 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E383E)
    (at 56 87.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3836)
    (at 63.125 86 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E382F)
    (at 63.125 89 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E381C)
    (at 71.1 87.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E37FD)
    (at 64 71 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E37F9)
    (at 76 79)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3799)
    (at 129.125 56 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3790)
    (at 142 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E3789)
    (at 129.125 59 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E3785)
    (at 117 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E3779)
    (at 130 41 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3766)
    (at 122 57.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E3754)
    (at 137.1 57.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E36ED)
    (at 109 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 602E36E8)
    (at 84 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E36E0)
    (at 96.125 56 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E36D5)
    (at 89 57.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E36C3)
    (at 104.1 57.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E36B9)
    (at 96.125 59 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E36B0)
    (at 97 41 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 5BB86C47)
    (at 76 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 602E2C0F) (tstamp 5BB86C3B)
    (at 51 49)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 602E34BD)
    (at 71.1 57.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 602E33D4)
    (at 64 41 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 602E3495)
    (at 56 57.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E347C)
    (at 63.125 56 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 602E34F1)
    (at 63.125 59 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text GND (at 126 122) (layer F.SilkS) (tstamp 602E3BB4)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 129.6 108.6 180) (layer B.SilkS) (tstamp 602E3B9D)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 120.5 122.5) (end 121.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3B87))
  (gr_line (start 122.5 121.5) (end 122.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3B86))
  (gr_line (start 121.5 122.5) (end 121.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3B85))
  (gr_text LED (at 118 122) (layer F.SilkS) (tstamp 602E3B7B)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 9 (at 144 122) (layer F.SilkS) (tstamp 602E3B72)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 121.5 121.5) (end 122.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3B6D))
  (gr_line (start 88.5 122.5) (end 88.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3B0E))
  (gr_line (start 89.5 121.5) (end 89.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3AE1))
  (gr_line (start 87.5 122.5) (end 88.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3AE0))
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 96.6 108.6 180) (layer B.SilkS) (tstamp 602E3ADE)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 93 122) (layer F.SilkS) (tstamp 602E3ADB)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 8 (at 111 122) (layer F.SilkS) (tstamp 602E3ACD)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 122) (layer F.SilkS) (tstamp 602E3AC4)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 88.5 121.5) (end 89.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3ABF))
  (gr_line (start 54.5 122.5) (end 55.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3A60))
  (gr_line (start 55.5 121.5) (end 56.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3A3A))
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 63.6 108.6 180) (layer B.SilkS) (tstamp 602E3A37)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 55.5 122.5) (end 55.5 121.5) (layer F.SilkS) (width 0.2) (tstamp 602E3A34))
  (gr_text 7 (at 78 122) (layer F.SilkS) (tstamp 602E3A33)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 52 122) (layer F.SilkS) (tstamp 602E3A2F)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text GND (at 60 122) (layer F.SilkS) (tstamp 602E3A2D)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 56.5 121.5) (end 56.5 122.5) (layer F.SilkS) (width 0.2) (tstamp 602E3A1E))
  (gr_line (start 121.5 91.5) (end 122.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E3991))
  (gr_text LED (at 118 92) (layer F.SilkS) (tstamp 602E3984)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 122.5 91.5) (end 122.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E3980))
  (gr_line (start 121.5 92.5) (end 121.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E397A))
  (gr_text 6 (at 144 92) (layer F.SilkS) (tstamp 602E3979)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 120.5 92.5) (end 121.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E3977))
  (gr_text GND (at 126 92) (layer F.SilkS) (tstamp 602E395C)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 129.6 78.6 180) (layer B.SilkS) (tstamp 602E395B)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 87.5 92.5) (end 88.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E38CF))
  (gr_text GND (at 93 92) (layer F.SilkS) (tstamp 602E38C8)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 88.5 91.5) (end 89.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E38C4))
  (gr_line (start 89.5 91.5) (end 89.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E38C3))
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 96.6 78.6 180) (layer B.SilkS) (tstamp 602E38BD)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text 5 (at 111 92) (layer F.SilkS) (tstamp 602E38B7)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 92) (layer F.SilkS) (tstamp 602E38B5)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 88.5 92.5) (end 88.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E38B4))
  (gr_text 4 (at 78 92) (layer F.SilkS) (tstamp 602E3850)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 54.5 92.5) (end 55.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E383D))
  (gr_line (start 55.5 92.5) (end 55.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E381A))
  (gr_line (start 55.5 91.5) (end 56.5 91.5) (layer F.SilkS) (width 0.2) (tstamp 602E3817))
  (gr_text GND (at 60 92) (layer F.SilkS) (tstamp 602E3816)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 63.6 78.6 180) (layer B.SilkS) (tstamp 602E380F)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 56.5 91.5) (end 56.5 92.5) (layer F.SilkS) (width 0.2) (tstamp 602E380D))
  (gr_text LED (at 52 92) (layer F.SilkS) (tstamp 602E3808)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 121.5 62.5) (end 121.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E3798))
  (gr_line (start 121.5 61.5) (end 122.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E3782))
  (gr_line (start 120.5 62.5) (end 121.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E3777))
  (dimension 33 (width 0.3) (layer Dwgs.User) (tstamp 602E3774)
    (gr_text "33,000 mm" (at 129.5 27.9) (layer Dwgs.User) (tstamp 602E3775)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 146 34) (xy 146 29.413579)))
    (feature2 (pts (xy 113 34) (xy 113 29.413579)))
    (crossbar (pts (xy 113 30) (xy 146 30)))
    (arrow1a (pts (xy 146 30) (xy 144.873496 30.586421)))
    (arrow1b (pts (xy 146 30) (xy 144.873496 29.413579)))
    (arrow2a (pts (xy 113 30) (xy 114.126504 30.586421)))
    (arrow2b (pts (xy 113 30) (xy 114.126504 29.413579)))
  )
  (gr_text GND (at 126 62) (layer F.SilkS) (tstamp 602E3753)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 122.5 61.5) (end 122.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E3752))
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 129.6 48.6 180) (layer B.SilkS) (tstamp 602E374D)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text 3 (at 144 62) (layer F.SilkS) (tstamp 602E374B)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 118 62) (layer F.SilkS) (tstamp 602E3749)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 88.5 62.5) (end 88.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E36AC))
  (gr_line (start 88.5 61.5) (end 89.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E36AB))
  (gr_line (start 89.5 61.5) (end 89.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E36AA))
  (gr_text GND (at 93 62) (layer F.SilkS) (tstamp 602E36A9)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 96.6 48.6 180) (layer B.SilkS) (tstamp 602E36A8)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (dimension 33 (width 0.3) (layer Dwgs.User) (tstamp 602E36A6)
    (gr_text "33,000 mm" (at 96.5 27.9) (layer Dwgs.User) (tstamp 602E36A7)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 113 34) (xy 113 29.413579)))
    (feature2 (pts (xy 80 34) (xy 80 29.413579)))
    (crossbar (pts (xy 80 30) (xy 113 30)))
    (arrow1a (pts (xy 113 30) (xy 111.873496 30.586421)))
    (arrow1b (pts (xy 113 30) (xy 111.873496 29.413579)))
    (arrow2a (pts (xy 80 30) (xy 81.126504 30.586421)))
    (arrow2b (pts (xy 80 30) (xy 81.126504 29.413579)))
  )
  (gr_text 2 (at 111 62) (layer F.SilkS) (tstamp 602E36A5)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 62) (layer F.SilkS) (tstamp 602E36A4)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 87.5 62.5) (end 88.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E36A3))
  (gr_line (start 113 34) (end 113 124) (layer F.SilkS) (width 0.15))
  (gr_line (start 47 94) (end 146 94) (layer F.SilkS) (width 0.15))
  (gr_line (start 47 64) (end 146 64) (layer F.SilkS) (width 0.15))
  (gr_line (start 80 34) (end 80 84) (layer F.SilkS) (width 0.15))
  (gr_line (start 80 84) (end 80 124) (layer F.SilkS) (width 0.15) (tstamp 5E428B70))
  (gr_line (start 47 124) (end 146 124) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE4813))
  (gr_text GND (at 60 62) (layer F.SilkS) (tstamp 602E3512)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 56.5 61.5) (end 56.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E350F))
  (gr_line (start 55.5 61.5) (end 56.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E350C))
  (gr_line (start 55.5 62.5) (end 55.5 61.5) (layer F.SilkS) (width 0.2) (tstamp 602E3509))
  (gr_line (start 54.5 62.5) (end 55.5 62.5) (layer F.SilkS) (width 0.2) (tstamp 602E3515))
  (gr_text LED (at 52 62) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (dimension 90 (width 0.3) (layer Eco2.User)
    (gr_text "90,000 mm" (at 35.900001 79 270) (layer Eco2.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 47 124) (xy 37.41358 124)))
    (feature2 (pts (xy 47 34) (xy 37.41358 34)))
    (crossbar (pts (xy 38.000001 34) (xy 38.000001 124)))
    (arrow1a (pts (xy 38.000001 124) (xy 37.41358 122.873496)))
    (arrow1b (pts (xy 38.000001 124) (xy 38.586422 122.873496)))
    (arrow2a (pts (xy 38.000001 34) (xy 37.41358 35.126504)))
    (arrow2b (pts (xy 38.000001 34) (xy 38.586422 35.126504)))
  )
  (dimension 99 (width 0.3) (layer Eco2.User)
    (gr_text "99,000 mm" (at 96.5 21.9) (layer Eco2.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 146 34) (xy 146 23.413579)))
    (feature2 (pts (xy 47 34) (xy 47 23.413579)))
    (crossbar (pts (xy 47 24) (xy 146 24)))
    (arrow1a (pts (xy 146 24) (xy 144.873496 24.586421)))
    (arrow1b (pts (xy 146 24) (xy 144.873496 23.413579)))
    (arrow2a (pts (xy 47 24) (xy 48.126504 24.586421)))
    (arrow2b (pts (xy 47 24) (xy 48.126504 23.413579)))
  )
  (gr_text 1 (at 78 62) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 47 34) (end 47 124) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE480A))
  (gr_line (start 146 34) (end 146 124) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE4754))
  (gr_line (start 47 34) (end 146 34) (layer Edge.Cuts) (width 0.15))
  (dimension 33 (width 0.3) (layer Dwgs.User)
    (gr_text "33,000 mm" (at 63.5 27.9) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 80 34) (xy 80 29.413579)))
    (feature2 (pts (xy 47 34) (xy 47 29.413579)))
    (crossbar (pts (xy 47 30) (xy 80 30)))
    (arrow1a (pts (xy 80 30) (xy 78.873496 30.586421)))
    (arrow1b (pts (xy 80 30) (xy 78.873496 29.413579)))
    (arrow2a (pts (xy 47 30) (xy 48.126504 30.586421)))
    (arrow2b (pts (xy 47 30) (xy 48.126504 29.413579)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30,000 mm" (at 40.9 49 270) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 47 64) (xy 42.413579 64)))
    (feature2 (pts (xy 47 34) (xy 42.413579 34)))
    (crossbar (pts (xy 43 34) (xy 43 64)))
    (arrow1a (pts (xy 43 64) (xy 42.413579 62.873496)))
    (arrow1b (pts (xy 43 64) (xy 43.586421 62.873496)))
    (arrow2a (pts (xy 43 34) (xy 42.413579 35.126504)))
    (arrow2b (pts (xy 43 34) (xy 43.586421 35.126504)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2021" (at 63.6 48.6 180) (layer B.SilkS) (tstamp 5BB86BF9)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )

  (segment (start 53.46 44.46) (end 50 41) (width 0.8) (layer F.Cu) (net 1))
  (segment (start 53.46 57.48) (end 53.46 44.46) (width 0.8) (layer F.Cu) (net 1))
  (segment (start 86.46 44.46) (end 83 41) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E36AD))
  (segment (start 86.46 57.48) (end 86.46 44.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E36EC))
  (segment (start 119.46 57.48) (end 119.46 44.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3778))
  (segment (start 119.46 44.46) (end 116 41) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E37A0))
  (segment (start 53.46 74.46) (end 50 71) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3809))
  (segment (start 53.46 87.48) (end 53.46 74.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E380B))
  (segment (start 86.46 74.46) (end 83 71) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E38B6))
  (segment (start 86.46 87.48) (end 86.46 74.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E38C9))
  (segment (start 119.46 74.46) (end 116 71) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E397B))
  (segment (start 119.46 87.48) (end 119.46 74.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E39AF))
  (segment (start 53.46 104.46) (end 50 101) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3A20))
  (segment (start 53.46 117.48) (end 53.46 104.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3A31))
  (segment (start 86.46 117.48) (end 86.46 104.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3ABE))
  (segment (start 86.46 104.46) (end 83 101) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3AC5))
  (segment (start 119.46 117.48) (end 119.46 104.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3B6A))
  (segment (start 119.46 104.46) (end 116 101) (width 0.8) (layer F.Cu) (net 1) (tstamp 602E3B71))
  (segment (start 57.48 56) (end 56 57.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3503) (status 20))
  (segment (start 62.25 56) (end 57.48 56) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3500) (status 10))
  (segment (start 90.48 56) (end 89 57.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E36AE) (status 20))
  (segment (start 95.25 56) (end 90.48 56) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E36AF) (status 10))
  (segment (start 128.25 56) (end 123.48 56) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E374E) (status 10))
  (segment (start 123.48 56) (end 122 57.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E374F) (status 20))
  (segment (start 62.25 86) (end 57.48 86) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E380C) (status 10))
  (segment (start 57.48 86) (end 56 87.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E384E) (status 20))
  (segment (start 95.25 86) (end 90.48 86) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E38BE) (status 10))
  (segment (start 90.48 86) (end 89 87.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E38D0) (status 20))
  (segment (start 128.25 86) (end 123.48 86) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3969) (status 10))
  (segment (start 123.48 86) (end 122 87.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3973) (status 20))
  (segment (start 57.48 116) (end 56 117.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3A0B) (status 20))
  (segment (start 62.25 116) (end 57.48 116) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3A22) (status 10))
  (segment (start 95.25 116) (end 90.48 116) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3ADC) (status 10))
  (segment (start 90.48 116) (end 89 117.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3ADF) (status 20))
  (segment (start 123.48 116) (end 122 117.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3B6F) (status 20))
  (segment (start 128.25 116) (end 123.48 116) (width 0.8) (layer F.Cu) (net 2) (tstamp 602E3BA1) (status 10))
  (segment (start 60.73 57.48) (end 62.25 59) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E352A) (status 20))
  (segment (start 58.54 57.48) (end 60.73 57.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3527) (status 10))
  (segment (start 66.72 60.28) (end 67.85 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3524) (status 20))
  (segment (start 66 61) (end 66.72 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3521))
  (segment (start 63 61) (end 66 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E351E))
  (segment (start 62.25 59) (end 62.25 60.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E351B) (status 10))
  (segment (start 62.25 60.25) (end 63 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3518))
  (segment (start 93.73 57.48) (end 95.25 59) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E369C) (status 20))
  (segment (start 91.54 57.48) (end 93.73 57.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E369D) (status 10))
  (segment (start 99.72 60.28) (end 100.85 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E369E) (status 20))
  (segment (start 99 61) (end 99.72 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E369F))
  (segment (start 96 61) (end 99 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E36A0))
  (segment (start 95.25 59) (end 95.25 60.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E36A1) (status 10))
  (segment (start 95.25 60.25) (end 96 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E36A2))
  (segment (start 132.72 60.28) (end 133.85 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3750) (status 20))
  (segment (start 124.54 57.48) (end 126.73 57.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3751) (status 10))
  (segment (start 132 61) (end 132.72 60.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3771))
  (segment (start 129 61) (end 132 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3773))
  (segment (start 128.25 60.25) (end 129 61) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3783))
  (segment (start 128.25 59) (end 128.25 60.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3794) (status 10))
  (segment (start 126.73 57.48) (end 128.25 59) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3796) (status 20))
  (segment (start 62.25 90.25) (end 63 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E380A))
  (segment (start 58.54 87.48) (end 60.73 87.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E380E) (status 10))
  (segment (start 66 91) (end 66.72 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3812))
  (segment (start 62.25 89) (end 62.25 90.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3814) (status 10))
  (segment (start 66.72 90.28) (end 67.85 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3815) (status 20))
  (segment (start 60.73 87.48) (end 62.25 89) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E382E) (status 20))
  (segment (start 63 91) (end 66 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E384D))
  (segment (start 99 91) (end 99.72 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38B8))
  (segment (start 95.25 90.25) (end 96 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38BC))
  (segment (start 91.54 87.48) (end 93.73 87.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38C6) (status 10))
  (segment (start 96 91) (end 99 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38C7))
  (segment (start 99.72 90.28) (end 100.85 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38CB) (status 20))
  (segment (start 93.73 87.48) (end 95.25 89) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38D1) (status 20))
  (segment (start 95.25 89) (end 95.25 90.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E38D9) (status 10))
  (segment (start 129 91) (end 132 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3959))
  (segment (start 126.73 87.48) (end 128.25 89) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3961) (status 20))
  (segment (start 124.54 87.48) (end 126.73 87.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3971) (status 10))
  (segment (start 128.25 90.25) (end 129 91) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3974))
  (segment (start 128.25 89) (end 128.25 90.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3976) (status 10))
  (segment (start 132.72 90.28) (end 133.85 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3978) (status 20))
  (segment (start 132 91) (end 132.72 90.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E39B0))
  (segment (start 66.72 120.28) (end 67.85 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A09) (status 20))
  (segment (start 62.25 119) (end 62.25 120.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A1F) (status 10))
  (segment (start 58.54 117.48) (end 60.73 117.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A2E) (status 10))
  (segment (start 60.73 117.48) (end 62.25 119) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A38) (status 20))
  (segment (start 62.25 120.25) (end 63 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A39))
  (segment (start 63 121) (end 66 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A4D))
  (segment (start 66 121) (end 66.72 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3A4E))
  (segment (start 95.25 119) (end 95.25 120.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3ABD) (status 10))
  (segment (start 96 121) (end 99 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3AD8))
  (segment (start 99 121) (end 99.72 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3ADA))
  (segment (start 95.25 120.25) (end 96 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3ADD))
  (segment (start 99.72 120.28) (end 100.85 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3AE4) (status 20))
  (segment (start 93.73 117.48) (end 95.25 119) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3AE6) (status 20))
  (segment (start 91.54 117.48) (end 93.73 117.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3AEE) (status 10))
  (segment (start 132.72 120.28) (end 133.85 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3B69) (status 20))
  (segment (start 129 121) (end 132 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3B6B))
  (segment (start 124.54 117.48) (end 126.73 117.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3B6E) (status 10))
  (segment (start 132 121) (end 132.72 120.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3B89))
  (segment (start 128.25 120.25) (end 129 121) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3BA2))
  (segment (start 126.73 117.48) (end 128.25 119) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3BB3) (status 20))
  (segment (start 128.25 119) (end 128.25 120.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 602E3BC0) (status 10))
  (segment (start 64 59) (end 64 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E34E8) (status 30))
  (segment (start 64.32 55.68) (end 64 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E34E5) (status 30))
  (segment (start 67.85 55.68) (end 64.32 55.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E34E2) (status 30))
  (segment (start 97 59) (end 97 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E36C0) (status 30))
  (segment (start 97.32 55.68) (end 97 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E36C1) (status 30))
  (segment (start 100.85 55.68) (end 97.32 55.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E36C2) (status 30))
  (segment (start 133.85 55.68) (end 130.32 55.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E374C) (status 30))
  (segment (start 130.32 55.68) (end 130 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3784) (status 30))
  (segment (start 130 59) (end 130 56) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3795) (status 30))
  (segment (start 64.32 85.68) (end 64 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3807) (status 30))
  (segment (start 67.85 85.68) (end 64.32 85.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3813) (status 30))
  (segment (start 64 89) (end 64 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E381B) (status 30))
  (segment (start 97.32 85.68) (end 97 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E38B9) (status 30))
  (segment (start 100.85 85.68) (end 97.32 85.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E38BA) (status 30))
  (segment (start 97 89) (end 97 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E38C5) (status 30))
  (segment (start 130 89) (end 130 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3975) (status 30))
  (segment (start 133.85 85.68) (end 130.32 85.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E399B) (status 30))
  (segment (start 130.32 85.68) (end 130 86) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E39AE) (status 30))
  (segment (start 64.32 115.68) (end 64 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3A32) (status 30))
  (segment (start 67.85 115.68) (end 64.32 115.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3A4F) (status 30))
  (segment (start 64 119) (end 64 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3A5F) (status 30))
  (segment (start 97 119) (end 97 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3AD7) (status 30))
  (segment (start 97.32 115.68) (end 97 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3AD9) (status 30))
  (segment (start 100.85 115.68) (end 97.32 115.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3AEF) (status 30))
  (segment (start 130 119) (end 130 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3B6C) (status 30))
  (segment (start 133.85 115.68) (end 130.32 115.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3B7A) (status 30))
  (segment (start 130.32 115.68) (end 130 116) (width 0.8) (layer F.Cu) (net 4) (tstamp 602E3BA0) (status 30))
  (segment (start 76 57.98) (end 74.35 57.98) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 78.849999 55.130001) (end 76 57.98) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 78.849999 41.849999) (end 78.849999 55.130001) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 78 41) (end 78.849999 41.849999) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 111.849999 41.849999) (end 111.849999 55.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3699))
  (segment (start 111 41) (end 111.849999 41.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E369A))
  (segment (start 111.849999 55.130001) (end 109 57.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E369B))
  (segment (start 109 57.98) (end 107.35 57.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E36E7))
  (segment (start 142 57.98) (end 140.35 57.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E374A))
  (segment (start 144 41) (end 144.849999 41.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3772))
  (segment (start 144.849999 41.849999) (end 144.849999 55.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3776))
  (segment (start 144.849999 55.130001) (end 142 57.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3797))
  (segment (start 76 87.98) (end 74.35 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3806))
  (segment (start 78 71) (end 78.849999 71.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3818))
  (segment (start 78.849999 71.849999) (end 78.849999 85.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3819))
  (segment (start 78.849999 85.130001) (end 76 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E384F))
  (segment (start 109 87.98) (end 107.35 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E38BB))
  (segment (start 111 71) (end 111.849999 71.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E38CA))
  (segment (start 111.849999 85.130001) (end 109 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E38CE))
  (segment (start 111.849999 71.849999) (end 111.849999 85.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E38EC))
  (segment (start 144.849999 71.849999) (end 144.849999 85.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E395A))
  (segment (start 144.849999 85.130001) (end 142 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3972))
  (segment (start 142 87.98) (end 140.35 87.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3983))
  (segment (start 144 71) (end 144.849999 71.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3985))
  (segment (start 78.849999 101.849999) (end 78.849999 115.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3A0A))
  (segment (start 76 117.98) (end 74.35 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3A21))
  (segment (start 78.849999 115.130001) (end 76 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3A23))
  (segment (start 78 101) (end 78.849999 101.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3A30))
  (segment (start 111.849999 101.849999) (end 111.849999 115.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3AE5))
  (segment (start 109 117.98) (end 107.35 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3AFB))
  (segment (start 111.849999 115.130001) (end 109 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3B0F))
  (segment (start 111 101) (end 111.849999 101.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3B10))
  (segment (start 144.849999 101.849999) (end 144.849999 115.130001) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3B70))
  (segment (start 144.849999 115.130001) (end 142 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3B88))
  (segment (start 142 117.98) (end 140.35 117.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3B8A))
  (segment (start 144 101) (end 144.849999 101.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 602E3BA3))

)
