{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Feuil1","TEST","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Tache",null,"Date mini","Importance",null,"Obligatoire","La rampes a led e peu pas fonctionné sans "]
["RTC","Oscillator fail",null,"Erreur",null,"Erreur","La rampes a led peu fonctionné sans mais pas de détection d'erreur"]
[null,"interuption Low power",null,"Erreur",null,"Confort","Confort d'utilisation de la rampes a led"]
["PWM","Test PWM sur la rampe a led","2019-01-18","Obligatoire",null,"Surplus"]
["Eeprom","faire .c",null,"Erreur"]
["Général","Serveurs interuption (Bouton, RTC)",null,"Erreur"]
[null,"Gestion des led d'indication","2019-01-25","Erreur"]
["I2C Externe",null,null,"Surplus"]
["USB",null,null,"Erreur"]
["Wifi",null,null,"Confort"]
["Initialisation","Initialisation RTC","2019-01-25","Obligatoire"]
[null,"Calibration RTC"," ","Obligatoire"]

{"sheet":"TEST","index":1,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["File","Name","Resultat","Documentation"]
["PWM","void PWMSetDutyCycle(uint32_t sortie, uint16_t value);"]
["PWM","void PWMSetZero(uint32_t sortie);"]
["PWM","void PWMSetMAX(uint32_t sortie);"]
["PWM","void PWMStart(uint8_t sortie);"]
["PWM","uint16_t PWMvalue(uint8_t heure);"]
[]
["Freertos","void TimerTask(void const * argument);"]
["Freertos","void init();"]
["Freertos","uint16_t minimum(uint16_t a,uint16_t b);"]
[]
["Tab","uint8_t readCase(uint8_t sortie, uint8_t heure);"]
[]
["RTC","void readRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","void writeRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","uint8_t readMinute();"]
["RTC","uint8_t readHeure();"]
["RTC","void readDate(Date *date);"]
["RTC","void redemareRTC();"]
[]
["EEPROM","void readEeprom(int add, uint8_t *tab, int len);"]
["EEPROM","void writeEeprom(int add, uint8_t *tab, int len);"]
["EEPROM","void readTab(uint8_t *tab);"]
["EEPROM","uint16_t readPointer();"]
["EEPROM","void writePointer(uint16_t p);"]
["EEPROM","void writeError(uint8_t *tab, int len);"]
["EEPROM","void readError(uint8_t *tab);"]

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}