{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Tache","Interruption","TEST","Port Blynk","Protocole UART","Led erreur","AddEEPROM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tache","index":0,"n_rows":4,"n_cols":7,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Tache",null,null,"Importance",null,"Obligatoire","La rampes a led e peu pas fonctionné sans "]
[{"$nulls":5},"Erreur","La rampes a led peu fonctionné sans mais pas de détection d'erreur"]
[{"$nulls":5},"Confort","Confort d'utilisation de la rampes a led"]
[{"$nulls":5},"Surplus"]

{"sheet":"Interruption","index":1,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Type","Ligne","Corespondence","Prio","Reaction"]
["IO",0,"Aquit"]
["IO",1]
["IO",2,"MFP"]
["IO",3]
["IO",4]
["IO",5]
["IO",6]
["IO",7]
["IO",8]
["IO",9]
["IO",10]
["IO",11]
["IO",12]
["IO",13]
["IO",14]
["IO",15]
["TIM4"]

{"sheet":"TEST","index":2,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["File","Name","Resultat","Documentation"]
["PWM","void PWMSetDutyCycle(uint32_t sortie, uint16_t value);"]
["PWM","void PWMSetZero(uint32_t sortie);"]
["PWM","void PWMSetMAX(uint32_t sortie);"]
["PWM","void PWMStart(uint8_t sortie);"]
["PWM","uint16_t PWMvalue(uint8_t heure);"]
[]
["Freertos","void TimerTask(void const * argument);"]
["Freertos","void init();"]
["Freertos","uint16_t minimum(uint16_t a,uint16_t b);"]
[]
["Tab","uint8_t readCase(uint8_t sortie, uint8_t heure);"]
[]
["RTC","void readRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","void writeRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","uint8_t readMinute();"]
["RTC","uint8_t readHeure();"]
["RTC","void readDate(Date *date);"]
["RTC","void redemareRTC();"]

{"sheet":"Port Blynk","index":3,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,4,0,8],[4,4,4,8]]}
[null,"Port","Type",null,"TYPE du tableau"]
["Eteint","V6","ON/OFF",null,null,"Max","Pente","Demmarage","Arret"]
["essai","V7","ON/OFF",null,"Type","Value Imput","Value Imput","Time input","Time input"]
[]
[{"$nulls":4},"Port du tableau"]
[{"$nulls":5},"Max","Pente","Demmarage","Arret","Essai"]
[{"$nulls":4},"Blanc","V8","V9","V10","V11","V1"]
[{"$nulls":4},"Chaud","V12","V13","V14","V15","V2"]
[{"$nulls":4},"Bleu","V16","V17","V18","V19","V3"]
[{"$nulls":4},"UV","V20","V21","V22","V23","V4"]

{"sheet":"Protocole UART","index":4,"n_rows":29,"n_cols":27,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,1,0,8],[0,10,0,17]]}
[null,"ESP",{"$nulls":8},"STM",{"$nulls":8},"Hex","Action",null,"Abreviation ","Nom",null,"Type","ID"]
["Write Tab Heure",0,0,0,1,"D/E","ID","ID","ID",null,0,0,0,1,"D/E","ID","ID","ID",null,"0x0X","Write Tab Heure",null,"V1","Ventilateur",null,"Blanc Max","0x01"]
[null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"0x1X","Write Tab Value",null,"LED","Type de led",null,"Chaud Max","0x02"]
[null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"0x2X",null,null,"PM","Puissance",null,"Bleu Max","0x03"]
[{"$nulls":19},"0x3X","Read Ventilation",null,"D/E","Demmarage = 0 ou extinction",null,"Rouge Max","0x04"]
["Write Tab Value",0,0,1,0,"M/P","ID","ID","ID",null,0,0,1,0,"M/P","ID","ID","ID",null,"0x4X","Write Ventilation",null,"M/P","Max = 0 ou Pente = 1",null,"UV Max","0x05"]
[null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"0x5X",{"$nulls":5},"Vert Max","0x06"]
[{"$nulls":19},"0x6X","WriteValue essai",{"$nulls":4},"Blanc Pente","0x08"]
["Read Ventilation",0,0,1,1,"X","X","X","X",null,0,0,1,1,"V1","V1","V1","V1",null,"0x7X","Stop",{"$nulls":4},"Chaud Pente","0x09"]
[{"$nulls":19},"0x8X","essai",null,"ID","LED",null,"Bleu Pente","0x0A"]
["Write Ventilation",0,1,0,0,"V1","V1","V1","V1",null,0,1,0,0,"V1","V1","V1","V1",null,"0x9X","sync RTC",null,0,"Blanc",null,"Rouge Pente","0X0B"]
[{"$nulls":19},"0xAX",null,null,1,"Chaud",null,"UV Pente","0x0C"]
["WriteValueEssai",0,1,1,0,"X","ID","ID","ID",null,0,1,1,0,"ID","ID","ID","ID",null,"0xBX",null,null,2,"Bleu",null,"Vert Pente","0x0D"]
[null,"PM","PM","PM","PM","PM","PM","PM","PM",null,"PM","PM","PM","PM","PM","PM","PM","PM",null,"0xCX",null,null,3,"UV",null,"Blanc Demmarage","0x01"]
[{"$nulls":19},"0xDX",null,null,4,null,null,"Chaud Demmarage","0x02"]
["Stop",0,1,1,1,"X","X","X","On",null,0,1,1,1,"X","X","X","X",null,"0xEX",null,null,5,null,null,"Bleu Demmarage","0x03"]
[{"$nulls":19},"0xFX","StartSync",null,6,null,null,"Rouge Demmarage","0x04"]
["essai",1,0,0,0,"X","X","X","On",null,1,0,0,0,"X","X","X","X",{"$nulls":4},7,null,null,"UV Demmarage","0x05"]
[{"$nulls":25},"Vert Demmarage","0x06"]
["sync RTC",1,0,0,0,"X","X","X","X",{"$nulls":16},"Blanc Arret","0x08"]
[null,"Y","Y","Y","Y","Y","Y","Y","Y",{"$nulls":16},"Chaud Arret","0x09"]
[null,"M","M","M","M","M","M","M","M",{"$nulls":16},"Bleu Arret","0x0A"]
[null,"J","J","J","J","J","J","J","J",{"$nulls":16},"Rouge Arret","0X0B"]
[null,"Day","Day","Day","Day","Day","Day","Day","Day",{"$nulls":16},"UV Arret","0x0C"]
[null,"H","H","H","H","H","H","H","H",{"$nulls":16},"Vert Arret","0x0D"]
[null,"M","M","M","M","M","M","M","M"]
[null,"S","S","S","S","S","S","S","S"]
[]
["StartSync",{"$nulls":8},1,1,1,1,"X","X","X","X"]

{"sheet":"Led erreur","index":5,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[null,null,"Vert","Orange","Rouge"]
["Erreur","RAS",1,0,0]
[null,"Batterie RTC",1,0,1]
[null,"Oscillator fail",0,0,1]

{"sheet":"AddEEPROM","index":6,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Nom","address Eeprpm"]
["Blanc Max","0x0000"]
["Chaud Max","0x0002"]
["Bleu Max","0x0004"]
["Rouge Max","0x0006"]
["UV Max","0x0008"]
["Vert Max","0x000A"]
["Blanc Pente","0x000C"]
["Chaud Pente","0x000E"]
["Bleu Pente","0x0010"]
["Rouge Pente","0x0012"]
["UV Pente","0x0014"]
["Vert Pente","0x0016"]
["Blanc Demmarage","0x0018"]
["Chaud Demmarage","0x001A"]
["Bleu Demmarage","0x001C"]
["Rouge Demmarage","0x001E"]
["UV Demmarage","0x0020"]
["Vert Demmarage","0x0022"]
["Blanc Arret","0x0024"]
["Chaud Arret","0x0028"]
["Bleu Arret","0x002A"]
["Rouge Arret","0x002C"]
["UV Arret","0x002E"]
["Vert Arret","0x0030"]