(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")

  (general
    (thickness 1.6)
    (drawings 77)
    (tracks 160)
    (zones 0)
    (modules 56)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.3)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.8 2.8)
    (pad_drill 2.8)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 47 34)
    (grid_origin 47 34)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Driver/"))
  )

  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(Q1-Pad1)")
  (net 5 "Net-(Q1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428CB7)
    (at 63.125 104 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428CB0)
    (at 63.125 101 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E428CA5)
    (at 56 102.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428C9C)
    (at 63 89 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E428C98)
    (at 74 96.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428C94)
    (at 52 96)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428C82)
    (at 71.1 102.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E428C43)
    (at 89 127.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428C3A)
    (at 96 114 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E428C36)
    (at 107 121.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428C32)
    (at 85 121)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428C20)
    (at 104.1 127.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428C19)
    (at 96.125 104 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428C12)
    (at 96.125 101 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E428C07)
    (at 89 102.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428BFE)
    (at 96 89 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E428BFA)
    (at 107 96.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428BF6)
    (at 85 96)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428BE4)
    (at 104.1 102.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E428BCA)
    (at 56 127.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428BC1)
    (at 63 114 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E428BBD)
    (at 74 121.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428BB9)
    (at 52 121)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428BA7)
    (at 71.1 127.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428BA0)
    (at 63.125 129 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428B99)
    (at 63.125 126 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428B92)
    (at 96.125 129 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428B8B)
    (at 96.125 126 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E428AAA)
    (at 56 77.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428AA1)
    (at 63 64 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E428A9D)
    (at 74 71.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428A99)
    (at 52 71)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428A87)
    (at 71.1 77.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428A80)
    (at 63.125 79 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428A79)
    (at 63.125 76 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E4289FF)
    (at 96.125 79 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E4289F8)
    (at 96.125 76 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E4289ED)
    (at 89 77.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E4289E4)
    (at 96 64 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E4289E0)
    (at 107 71.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E4289DC)
    (at 85 71)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E4289CA)
    (at 104.1 77.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E42895C)
    (at 96.125 54 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5E428955)
    (at 96.125 51 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5E42894A)
    (at 89 52.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5E428941)
    (at 96 39 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5E42893D)
    (at 107 46.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5E428939)
    (at 85 46)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5E428927)
    (at 104.1 52.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module U:SOT-223 (layer F.Cu) (tedit 58121019) (tstamp 5BB86C10)
    (at 71.1 52.98 270)
    (path /5CB86B6B)
    (fp_text reference Q1 (at 3.429 -4.064) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value N_MOSFET (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    )
    (fp_line (start 1.9685 -2.032) (end -1.9685 -2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.0955) (end 1.9685 -2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start 1.9685 -2.2225) (end -1.9685 -2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -1.9685 -2.3495) (end 1.9685 -2.3495) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.286) (end 0.6985 2.286) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.159) (end -0.6985 2.159) (layer F.Cu) (width 0.15))
    (fp_line (start 0.6985 2.032) (end -0.6985 2.032) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.0955) (end 0.6985 2.0955) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.2225) (end 0.6985 2.2225) (layer F.Cu) (width 0.15))
    (fp_line (start -0.6985 2.3495) (end 0.6985 2.3495) (layer F.Cu) (width 0.15))
    (pad 2 smd rect (at 0 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -2.3 3.25 270) (size 1.4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -3.25 270) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad2)"))
    (pad "" connect rect (at 0 0 270) (size 6 4) (layers F.Cu F.Adhes F.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288D8) (tstamp 5BB86C3B)
    (at 52 46)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704C456)
    (fp_text reference P3 (at 0.43 -0.14) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at -1 0.5) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module MH:MH2mm8 (layer F.Cu) (tedit 5E4288E4) (tstamp 5BB86C47)
    (at 74 46.5)
    (descr "module Non Plated Through Hole")
    (tags DEV)
    (path /5704BD0C)
    (fp_text reference P2 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (fp_text value CONN_01X01 (at 0 0) (layer Cmts.User) hide
      (effects (font (size 0.75 0.7) (thickness 0.17)))
    )
    (pad "" thru_hole circle (at 2 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
  )

  (module R:ciment (layer F.Cu) (tedit 5A775490) (tstamp 5BB86C76)
    (at 63 39 180)
    (path /57EB844A)
    (fp_text reference R1 (at 12.432 -4.087001 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -11 -4.75) (end -11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 4.75) (end 11 4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -4.75) (end 11 -4.75) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at 14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -14 0 180) (size 1.7 1.7) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad2)"))
  )

  (module Connector:Bornier2.54_1x3 (layer F.Cu) (tedit 5B3CCA80) (tstamp 5BB86C93)
    (at 56 52.48)
    (path /56BF4595)
    (fp_text reference P1 (at -4.826 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at -0.762 -3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.04 3.35) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.064 2.54) (end -4.016 2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end 4.04 -2.95) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.04 -2.95) (end -4.04 3.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.04 -2.95) (end 4.04 3.35) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5CCC48BD)
    (at 63.125 51 180)
    (path /5CCC457C)
    (fp_text reference R2 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 120 (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module R:0805 (layer F.Cu) (tedit 5703B877) (tstamp 5CCC48A8)
    (at 63.125 54 180)
    (path /5CCC442E)
    (fp_text reference R3 (at 0.05 0 270) (layer F.SilkS)
      (effects (font (size 0.7 0.66) (thickness 0.16)))
    )
    (fp_text value 10k (at -0.875 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.2) (thickness 0.05)))
    )
    (fp_line (start -0.4 0.75) (end 0.4 0.75) (layer F.SilkS) (width 0.17))
    (fp_line (start -0.4 -0.75) (end 0.4 -0.75) (layer F.SilkS) (width 0.17))
    (pad 1 smd rect (at -0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at 0.875 0 180) (size 0.85 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (model ${KIPRJMOD}/../packages3d/None-R0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 47 84) (end 113 84) (layer F.SilkS) (width 0.2))
  (gr_line (start 54.5 132.5) (end 55.5 132.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CCC))
  (gr_line (start 55.5 132.5) (end 55.5 131.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CCB))
  (gr_line (start 55.5 131.5) (end 56.5 131.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CCA))
  (gr_line (start 56.5 131.5) (end 56.5 132.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC9))
  (gr_line (start 87.5 132.5) (end 88.5 132.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC8))
  (gr_line (start 88.5 132.5) (end 88.5 131.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC7))
  (gr_line (start 88.5 131.5) (end 89.5 131.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC6))
  (gr_line (start 89.5 131.5) (end 89.5 132.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC5))
  (gr_line (start 87.5 107.5) (end 88.5 107.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC4))
  (gr_line (start 88.5 107.5) (end 88.5 106.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC3))
  (gr_line (start 88.5 106.5) (end 89.5 106.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC2))
  (gr_line (start 89.5 106.5) (end 89.5 107.5) (layer F.SilkS) (width 0.2) (tstamp 5E428CC1))
  (gr_text 5 (at 78 107) (layer F.SilkS) (tstamp 5E428CC0)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 52 107) (layer F.SilkS) (tstamp 5E428CBF)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text GND (at 60 107) (layer F.SilkS) (tstamp 5E428CBE)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 96 116 180) (layer B.SilkS) (tstamp 5E428C78)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 93 132) (layer F.SilkS) (tstamp 5E428C77)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 132) (layer F.SilkS) (tstamp 5E428C76)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 8 (at 111 132) (layer F.SilkS) (tstamp 5E428C75)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 63 116 180) (layer B.SilkS) (tstamp 5E428BE3)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 60 132) (layer F.SilkS) (tstamp 5E428BE2)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 52 132) (layer F.SilkS) (tstamp 5E428BE1)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 7 (at 78 132) (layer F.SilkS) (tstamp 5E428BE0)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 96 91 180) (layer B.SilkS) (tstamp 5E428B85)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 93 107) (layer F.SilkS) (tstamp 5E428B84)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 107) (layer F.SilkS) (tstamp 5E428B83)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 6 (at 111 107) (layer F.SilkS) (tstamp 5E428B74)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 63 91 180) (layer B.SilkS) (tstamp 5E428B73)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 47 109) (end 113 109) (layer F.SilkS) (width 0.15) (tstamp 5E428B71))
  (gr_line (start 80 84) (end 80 134) (layer F.SilkS) (width 0.15) (tstamp 5E428B70))
  (gr_line (start 54.5 107.5) (end 55.5 107.5) (layer F.SilkS) (width 0.2) (tstamp 5E428B6F))
  (gr_line (start 55.5 107.5) (end 55.5 106.5) (layer F.SilkS) (width 0.2) (tstamp 5E428B6E))
  (gr_line (start 55.5 106.5) (end 56.5 106.5) (layer F.SilkS) (width 0.2) (tstamp 5E428B6D))
  (gr_line (start 56.5 106.5) (end 56.5 107.5) (layer F.SilkS) (width 0.2) (tstamp 5E428B6C))
  (gr_line (start 47 134) (end 113 134) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE4813))
  (gr_line (start 54.5 82.5) (end 55.5 82.5) (layer F.SilkS) (width 0.2) (tstamp 5E428ACD))
  (gr_line (start 55.5 82.5) (end 55.5 81.5) (layer F.SilkS) (width 0.2) (tstamp 5E428ACC))
  (gr_line (start 55.5 81.5) (end 56.5 81.5) (layer F.SilkS) (width 0.2) (tstamp 5E428ACB))
  (gr_line (start 56.5 81.5) (end 56.5 82.5) (layer F.SilkS) (width 0.2) (tstamp 5E428ACA))
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 63 66 180) (layer B.SilkS) (tstamp 5E428AC9)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 60 82) (layer F.SilkS) (tstamp 5E428AC8)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 52 82) (layer F.SilkS) (tstamp 5E428AC7)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 3 (at 78 82) (layer F.SilkS) (tstamp 5E428AC6)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 87.5 82.5) (end 88.5 82.5) (layer F.SilkS) (width 0.2) (tstamp 5E428A19))
  (gr_line (start 88.5 82.5) (end 88.5 81.5) (layer F.SilkS) (width 0.2) (tstamp 5E428A18))
  (gr_line (start 88.5 81.5) (end 89.5 81.5) (layer F.SilkS) (width 0.2) (tstamp 5E428A17))
  (gr_line (start 89.5 81.5) (end 89.5 82.5) (layer F.SilkS) (width 0.2) (tstamp 5E428A16))
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 96 66 180) (layer B.SilkS) (tstamp 5E4289C6)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text GND (at 93 82) (layer F.SilkS) (tstamp 5E4289C5)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 82) (layer F.SilkS) (tstamp 5E4289C4)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 4 (at 111 82) (layer F.SilkS) (tstamp 5E4289C3)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text 2 (at 111 57) (layer F.SilkS) (tstamp 5E428965)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text LED (at 85 57) (layer F.SilkS) (tstamp 5E428964)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text GND (at 93 57) (layer F.SilkS) (tstamp 5E428963)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 96 41 180) (layer B.SilkS) (tstamp 5E428913)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 87.5 57.5) (end 88.5 57.5) (layer F.SilkS) (width 0.2) (tstamp 5E428911))
  (gr_line (start 88.5 57.5) (end 88.5 56.5) (layer F.SilkS) (width 0.2) (tstamp 5E428910))
  (gr_line (start 88.5 56.5) (end 89.5 56.5) (layer F.SilkS) (width 0.2) (tstamp 5E42890F))
  (gr_line (start 89.5 56.5) (end 89.5 57.5) (layer F.SilkS) (width 0.2) (tstamp 5E42890E))
  (gr_text GND (at 60 57) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 56.5 56.5) (end 56.5 57.5) (layer F.SilkS) (width 0.2))
  (gr_line (start 55.5 56.5) (end 56.5 56.5) (layer F.SilkS) (width 0.2))
  (gr_line (start 55.5 57.5) (end 55.5 56.5) (layer F.SilkS) (width 0.2))
  (gr_line (start 54.5 57.5) (end 55.5 57.5) (layer F.SilkS) (width 0.2))
  (gr_text LED (at 52 57) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (dimension 100 (width 0.3) (layer Eco2.User)
    (gr_text "100,000 mm" (at 35.900001 84 270) (layer Eco2.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 47 134) (xy 37.41358 134)))
    (feature2 (pts (xy 47 34) (xy 37.41358 34)))
    (crossbar (pts (xy 38.000001 34) (xy 38.000001 134)))
    (arrow1a (pts (xy 38.000001 134) (xy 37.41358 132.873496)))
    (arrow1b (pts (xy 38.000001 134) (xy 38.586422 132.873496)))
    (arrow2a (pts (xy 38.000001 34) (xy 37.41358 35.126504)))
    (arrow2b (pts (xy 38.000001 34) (xy 38.586422 35.126504)))
  )
  (dimension 66 (width 0.3) (layer Eco2.User)
    (gr_text "66,000 mm" (at 80 21.9) (layer Eco2.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 113 34) (xy 113 23.413579)))
    (feature2 (pts (xy 47 34) (xy 47 23.413579)))
    (crossbar (pts (xy 47 24) (xy 113 24)))
    (arrow1a (pts (xy 113 24) (xy 111.873496 24.586421)))
    (arrow1b (pts (xy 113 24) (xy 111.873496 23.413579)))
    (arrow2a (pts (xy 47 24) (xy 48.126504 24.586421)))
    (arrow2b (pts (xy 47 24) (xy 48.126504 23.413579)))
  )
  (gr_text 1 (at 78 57) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 80 34) (end 80 84) (layer F.SilkS) (width 0.15))
  (gr_line (start 47 59) (end 113 59) (layer F.SilkS) (width 0.15))
  (gr_line (start 47 134) (end 47 34) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE480A))
  (gr_line (start 113 34) (end 113 134) (layer Edge.Cuts) (width 0.15) (tstamp 5CEE4754))
  (gr_line (start 47 34) (end 113 34) (layer Edge.Cuts) (width 0.15))
  (dimension 33 (width 0.3) (layer Dwgs.User)
    (gr_text "33,000 mm" (at 63.5 27.9) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 80 34) (xy 80 29.413579)))
    (feature2 (pts (xy 47 34) (xy 47 29.413579)))
    (crossbar (pts (xy 47 30) (xy 80 30)))
    (arrow1a (pts (xy 80 30) (xy 78.873496 30.586421)))
    (arrow1b (pts (xy 80 30) (xy 78.873496 29.413579)))
    (arrow2a (pts (xy 47 30) (xy 48.126504 30.586421)))
    (arrow2b (pts (xy 47 30) (xy 48.126504 29.413579)))
  )
  (dimension 25 (width 0.3) (layer Dwgs.User)
    (gr_text "25,000 mm" (at 40.9 46.5 270) (layer Dwgs.User)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (feature1 (pts (xy 47 59) (xy 42.413579 59)))
    (feature2 (pts (xy 47 34) (xy 42.413579 34)))
    (crossbar (pts (xy 43 34) (xy 43 59)))
    (arrow1a (pts (xy 43 59) (xy 42.413579 57.873496)))
    (arrow1b (pts (xy 43 59) (xy 43.586421 57.873496)))
    (arrow2a (pts (xy 43 34) (xy 42.413579 35.126504)))
    (arrow2b (pts (xy 43 34) (xy 43.586421 35.126504)))
  )
  (gr_text "Drivers LED V 3.2\nR.C 02/2020" (at 63 41 180) (layer B.SilkS) (tstamp 5BB86BF9)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )

  (segment (start 53.46 43.46) (end 53.46 52.48) (width 0.8) (layer F.Cu) (net 1))
  (segment (start 49 39) (end 53.46 43.46) (width 0.8) (layer F.Cu) (net 1))
  (segment (start 82 39) (end 86.46 43.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428918))
  (segment (start 86.46 43.46) (end 86.46 52.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E42891E))
  (segment (start 82 64) (end 86.46 68.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428A06))
  (segment (start 86.46 68.46) (end 86.46 77.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428A0C))
  (segment (start 49 64) (end 53.46 68.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428AB6))
  (segment (start 53.46 68.46) (end 53.46 77.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428ABC))
  (segment (start 53.46 118.46) (end 53.46 127.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428B7E))
  (segment (start 49 89) (end 53.46 93.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428BD5))
  (segment (start 53.46 93.46) (end 53.46 102.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428BDB))
  (segment (start 82 89) (end 86.46 93.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428C4E))
  (segment (start 86.46 93.46) (end 86.46 102.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428C54))
  (segment (start 82 114) (end 86.46 118.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428C5E))
  (segment (start 86.46 118.46) (end 86.46 127.48) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428C64))
  (segment (start 49 114) (end 53.46 118.46) (width 0.8) (layer F.Cu) (net 1) (tstamp 5E428C72))
  (segment (start 57.48 51) (end 56 52.48) (width 0.8) (layer F.Cu) (net 2))
  (segment (start 62.25 51) (end 57.48 51) (width 0.8) (layer F.Cu) (net 2))
  (segment (start 90.48 51) (end 89 52.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E42891F))
  (segment (start 95.25 51) (end 90.48 51) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428920))
  (segment (start 90.48 76) (end 89 77.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428A0D))
  (segment (start 95.25 76) (end 90.48 76) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428A0E))
  (segment (start 57.48 76) (end 56 77.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428ABD))
  (segment (start 62.25 76) (end 57.48 76) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428ABE))
  (segment (start 62.25 126) (end 57.48 126) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428B7B))
  (segment (start 57.48 126) (end 56 127.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428B81))
  (segment (start 90.48 101) (end 89 102.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C55))
  (segment (start 95.25 101) (end 90.48 101) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C56))
  (segment (start 90.48 126) (end 89 127.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C65))
  (segment (start 95.25 126) (end 90.48 126) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C66))
  (segment (start 57.48 101) (end 56 102.48) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C79))
  (segment (start 62.25 101) (end 57.48 101) (width 0.8) (layer F.Cu) (net 2) (tstamp 5E428C7B))
  (segment (start 60.73 52.48) (end 62.25 54) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 58.54 52.48) (end 60.73 52.48) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 66.72 55.28) (end 67.85 55.28) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 66 56) (end 66.72 55.28) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 63 56) (end 66 56) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 62.25 54) (end 62.25 55.25) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 62.25 55.25) (end 63 56) (width 0.8) (layer F.Cu) (net 3))
  (segment (start 95.25 55.25) (end 96 56) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428912))
  (segment (start 99.72 55.28) (end 100.85 55.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428921))
  (segment (start 91.54 52.48) (end 93.73 52.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428922))
  (segment (start 93.73 52.48) (end 95.25 54) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428923))
  (segment (start 96 56) (end 99 56) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428924))
  (segment (start 95.25 54) (end 95.25 55.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428925))
  (segment (start 99 56) (end 99.72 55.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428926))
  (segment (start 95.25 80.25) (end 96 81) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E4289C8))
  (segment (start 99.72 80.28) (end 100.85 80.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A0F))
  (segment (start 91.54 77.48) (end 93.73 77.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A10))
  (segment (start 93.73 77.48) (end 95.25 79) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A11))
  (segment (start 96 81) (end 99 81) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A12))
  (segment (start 95.25 79) (end 95.25 80.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A13))
  (segment (start 99 81) (end 99.72 80.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A14))
  (segment (start 62.25 80.25) (end 63 81) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428A77))
  (segment (start 66.72 80.28) (end 67.85 80.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428ABF))
  (segment (start 58.54 77.48) (end 60.73 77.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428AC0))
  (segment (start 60.73 77.48) (end 62.25 79) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428AC1))
  (segment (start 63 81) (end 66 81) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428AC2))
  (segment (start 62.25 79) (end 62.25 80.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428AC3))
  (segment (start 66 81) (end 66.72 80.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428AC4))
  (segment (start 62.25 105.25) (end 63 106) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B72))
  (segment (start 95.25 130.25) (end 96 131) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B7C))
  (segment (start 66.72 130.28) (end 67.85 130.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B7F))
  (segment (start 60.73 127.48) (end 62.25 129) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B86))
  (segment (start 63 131) (end 66 131) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B87))
  (segment (start 62.25 129) (end 62.25 130.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B88))
  (segment (start 66 131) (end 66.72 130.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428B89))
  (segment (start 58.54 127.48) (end 60.73 127.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428BDD))
  (segment (start 95.25 105.25) (end 96 106) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428BDE))
  (segment (start 99.72 105.28) (end 100.85 105.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C57))
  (segment (start 91.54 102.48) (end 93.73 102.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C58))
  (segment (start 93.73 102.48) (end 95.25 104) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C59))
  (segment (start 96 106) (end 99 106) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C5A))
  (segment (start 95.25 104) (end 95.25 105.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C5B))
  (segment (start 99 106) (end 99.72 105.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C5C))
  (segment (start 99.72 130.28) (end 100.85 130.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C67))
  (segment (start 91.54 127.48) (end 93.73 127.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C68))
  (segment (start 93.73 127.48) (end 95.25 129) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C69))
  (segment (start 96 131) (end 99 131) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C6A))
  (segment (start 95.25 129) (end 95.25 130.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C6B))
  (segment (start 99 131) (end 99.72 130.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C6C))
  (segment (start 62.25 130.25) (end 63 131) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C6F))
  (segment (start 66.72 105.28) (end 67.85 105.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C7C))
  (segment (start 58.54 102.48) (end 60.73 102.48) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C7D))
  (segment (start 60.73 102.48) (end 62.25 104) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C7E))
  (segment (start 63 106) (end 66 106) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C7F))
  (segment (start 62.25 104) (end 62.25 105.25) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C80))
  (segment (start 66 106) (end 66.72 105.28) (width 0.8) (layer F.Cu) (net 3) (tstamp 5E428C81))
  (segment (start 64 54) (end 64 51) (width 0.8) (layer F.Cu) (net 4))
  (segment (start 64.32 50.68) (end 64 51) (width 0.8) (layer F.Cu) (net 4))
  (segment (start 67.85 50.68) (end 64.32 50.68) (width 0.8) (layer F.Cu) (net 4))
  (segment (start 97 54) (end 97 51) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428914))
  (segment (start 97.32 50.68) (end 97 51) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428915))
  (segment (start 100.85 50.68) (end 97.32 50.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428916))
  (segment (start 97.32 75.68) (end 97 76) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E4289C7))
  (segment (start 97 79) (end 97 76) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E4289C9))
  (segment (start 100.85 75.68) (end 97.32 75.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428A15))
  (segment (start 64.32 75.68) (end 64 76) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428A76))
  (segment (start 64 79) (end 64 76) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428AB5))
  (segment (start 67.85 75.68) (end 64.32 75.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428AC5))
  (segment (start 64 104) (end 64 101) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428B75))
  (segment (start 64.32 100.68) (end 64 101) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428B76))
  (segment (start 67.85 100.68) (end 64.32 100.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428B77))
  (segment (start 97.32 125.68) (end 97 126) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428B79))
  (segment (start 67.85 125.68) (end 64.32 125.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428B8A))
  (segment (start 97.32 100.68) (end 97 101) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428BDC))
  (segment (start 97 104) (end 97 101) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428BDF))
  (segment (start 97 129) (end 97 126) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428C5D))
  (segment (start 100.85 125.68) (end 97.32 125.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428C6D))
  (segment (start 64.32 125.68) (end 64 126) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428C6E))
  (segment (start 64 129) (end 64 126) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428C71))
  (segment (start 100.85 100.68) (end 97.32 100.68) (width 0.8) (layer F.Cu) (net 4) (tstamp 5E428C7A))
  (segment (start 67.35 52.48) (end 67.85 52.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5BB86C59))
  (segment (start 76.150001 39.849999) (end 77 39) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 73.899999 42.100001) (end 76.150001 39.849999) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 73.899999 49.729999) (end 73.899999 42.100001) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 74.35 50.18) (end 73.899999 49.729999) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 74.35 52.98) (end 74.35 50.18) (width 0.8) (layer F.Cu) (net 5))
  (segment (start 100.35 52.48) (end 100.85 52.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428917))
  (segment (start 107.35 52.98) (end 107.35 50.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428919))
  (segment (start 107.35 50.18) (end 106.899999 49.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E42891A))
  (segment (start 106.899999 49.729999) (end 106.899999 42.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E42891B))
  (segment (start 106.899999 42.100001) (end 109.150001 39.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E42891C))
  (segment (start 109.150001 39.849999) (end 110 39) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E42891D))
  (segment (start 100.35 77.48) (end 100.85 77.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E4289C2))
  (segment (start 107.35 77.98) (end 107.35 75.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A07))
  (segment (start 107.35 75.18) (end 106.899999 74.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A08))
  (segment (start 106.899999 74.729999) (end 106.899999 67.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A09))
  (segment (start 106.899999 67.100001) (end 109.150001 64.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A0A))
  (segment (start 109.150001 64.849999) (end 110 64) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A0B))
  (segment (start 67.35 77.48) (end 67.85 77.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428A78))
  (segment (start 74.35 77.98) (end 74.35 75.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428AB7))
  (segment (start 74.35 75.18) (end 73.899999 74.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428AB8))
  (segment (start 73.899999 74.729999) (end 73.899999 67.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428AB9))
  (segment (start 73.899999 67.100001) (end 76.150001 64.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428ABA))
  (segment (start 76.150001 64.849999) (end 77 64) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428ABB))
  (segment (start 100.35 102.48) (end 100.85 102.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B6B))
  (segment (start 67.35 102.48) (end 67.85 102.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B78))
  (segment (start 76.150001 114.849999) (end 77 114) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B7A))
  (segment (start 73.899999 117.100001) (end 76.150001 114.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B7D))
  (segment (start 73.899999 124.729999) (end 73.899999 117.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B80))
  (segment (start 100.35 127.48) (end 100.85 127.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428B82))
  (segment (start 74.35 102.98) (end 74.35 100.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428BD6))
  (segment (start 74.35 100.18) (end 73.899999 99.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428BD7))
  (segment (start 73.899999 99.729999) (end 73.899999 92.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428BD8))
  (segment (start 73.899999 92.100001) (end 76.150001 89.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428BD9))
  (segment (start 76.150001 89.849999) (end 77 89) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428BDA))
  (segment (start 107.35 102.98) (end 107.35 100.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C4F))
  (segment (start 107.35 100.18) (end 106.899999 99.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C50))
  (segment (start 106.899999 99.729999) (end 106.899999 92.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C51))
  (segment (start 106.899999 92.100001) (end 109.150001 89.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C52))
  (segment (start 109.150001 89.849999) (end 110 89) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C53))
  (segment (start 107.35 127.98) (end 107.35 125.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C5F))
  (segment (start 107.35 125.18) (end 106.899999 124.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C60))
  (segment (start 106.899999 124.729999) (end 106.899999 117.100001) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C61))
  (segment (start 106.899999 117.100001) (end 109.150001 114.849999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C62))
  (segment (start 109.150001 114.849999) (end 110 114) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C63))
  (segment (start 67.35 127.48) (end 67.85 127.98) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C70))
  (segment (start 74.35 127.98) (end 74.35 125.18) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C73))
  (segment (start 74.35 125.18) (end 73.899999 124.729999) (width 0.8) (layer F.Cu) (net 5) (tstamp 5E428C74))

)
