{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Tache","Interruption","TEST","Port Blynk","Protocole UART","Status","AddEEPROM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tache","index":0,"n_rows":4,"n_cols":7,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Tache",null,null,"Importance",null,"Obligatoire","La rampes a led e peu pas fonctionné sans "]
[{"$nulls":5},"Erreur","La rampes a led peu fonctionné sans mais pas de détection d'erreur"]
[{"$nulls":5},"Confort","Confort d'utilisation de la rampes a led"]
[{"$nulls":5},"Surplus"]

{"sheet":"Interruption","index":1,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Type","Ligne","Corespondence","Prio","Reaction"]
["IO",0,"Aquit"]
["IO",1]
["IO",2,"MFP"]
["IO",3]
["IO",4]
["IO",5]
["IO",6]
["IO",7]
["IO",8]
["IO",9]
["IO",10]
["IO",11]
["IO",12]
["IO",13]
["IO",14]
["IO",15]
["TIM4"]

{"sheet":"TEST","index":2,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["File","Name","Resultat","Documentation"]
["PWM","void PWMSetDutyCycle(uint32_t sortie, uint16_t value);"]
["PWM","void PWMSetZero(uint32_t sortie);"]
["PWM","void PWMSetMAX(uint32_t sortie);"]
["PWM","void PWMStart(uint8_t sortie);"]
["PWM","uint16_t PWMvalue(uint8_t heure);"]
[]
["Freertos","void TimerTask(void const * argument);"]
["Freertos","void init();"]
["Freertos","uint16_t minimum(uint16_t a,uint16_t b);"]
[]
["Tab","uint8_t readCase(uint8_t sortie, uint8_t heure);"]
[]
["RTC","void readRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","void writeRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","uint8_t readMinute();"]
["RTC","uint8_t readHeure();"]
["RTC","void readDate(Date *date);"]
["RTC","void redemareRTC();"]

{"sheet":"Port Blynk","index":3,"n_rows":16,"n_cols":13,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,4,0,8],[4,4,4,8]]}
[null,"Port","Type",null,"TYPE du tableau",{"$nulls":6},"Terminal","V60"]
["Eteint","V6","ON/OFF",null,null,"Max","Pente","Demmarage","Arret","Essai"]
["essai","V7","ON/OFF",null,"Type","Value Imput","Value Imput","Time input","Time input"]
[]
[{"$nulls":4},"Port du tableau"]
[{"$nulls":5},"Max","Pente","Demmarage","Arret","Essai"]
[{"$nulls":4},"S1","V10","V20","V30","V40","V50"]
[{"$nulls":4},"S2","V11","V21","V31","V41","V51"]
[{"$nulls":4},"S3","V12","V22","V32","V42","V52"]
[{"$nulls":4},"S4","V13","V23","V33","V43","V53"]
[{"$nulls":4},"S5","V14","V24","V34","V44","V54"]
[{"$nulls":4},"S6","V15","V25","V35","V45","V55"]
[{"$nulls":4},"S7","V16","V26","V36","V46","V56"]
[{"$nulls":4},"S8","V17","V27","V37","V47","V57"]
[{"$nulls":4},"S9","V18","V28","V38","V48","V58"]
[{"$nulls":4},"S10","V19","V29","V39","V49","V59"]

{"sheet":"Protocole UART","index":4,"n_rows":46,"n_cols":28,"rows_kept":46,"cut":false,"hidden":false,"merged":[[0,1,0,8],[0,10,0,17]]}
[null,"ESP",{"$nulls":8},"STM",{"$nulls":8},"Hex","Action",null,"Abreviation ","Nom",null,"ID","LED"]
["Write Tab Heure",0,0,0,0,"X","X","X","X",null,0,0,0,0,"X","x","x","x",null,"0x0X","Write Tab Heure",null,"V1","Ventilateur",null,0,"S1"]
[null,"D/E",null,null,null,"ID","ID","ID","ID",null,"D/E",null,null,null,"ID","ID","ID","ID",null,"0x1X","Read Tab Heure",null,"LED","Type de led",null,1,"S2"]
[null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"0x2X","Write Tab Value",null,"D/E","Demmarage = 0 ou extinction",null,2,"S3"]
[null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"0x3X","Read Tac Value",null,"M/P","Max = 0 ou Pente = 1",null,3,"S4"]
[{"$nulls":19},"0x4X","Read Ventilation",null,"Pente","temps en minute",null,4,"S5"]
["Read Tab Heure",0,0,0,1,"X","X","X","X",null,0,0,0,1,"X","x","x","x",null,"0x5X","Write Ventilation",{"$nulls":4},5,"S6"]
[null,"D/E",null,null,null,"ID","ID","ID","ID",null,"D/E",null,null,null,"ID","ID","ID","ID",null,"0x6X","WriteValue essai",{"$nulls":4},6,"S7"]
[{"$nulls":10},"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"0x7X","Stop",{"$nulls":4},7,"S8"]
[{"$nulls":10},"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"0x8X","essai",{"$nulls":4},8,"S9"]
[{"$nulls":19},"0x9X","sync RTC",{"$nulls":4},9,"S10"]
["Write Tab Value",0,0,1,0,"X","X","X","X",null,0,0,1,0,"X","X","X","X",null,"0xAX","Status"]
[null,"M/P",null,null,null,"ID","ID","ID","ID",null,"M/P",null,null,null,"ID","ID","ID","ID",null,"0xBX"]
[null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"0xCX"]
[{"$nulls":19},"0xDX"]
["Write Tab Value",0,0,1,1,"X","X","X","X",null,0,0,1,1,"X","X","X","X",null,"0xEX"]
[null,"M/P",null,null,null,"ID","ID","ID","ID",null,"M/P",null,null,null,"ID","ID","ID","ID",null,"0xFX"]
[{"$nulls":10},"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL"]
[]
["Read Ventilation",0,1,0,0,"X","X","X","X",null,0,1,0,0,"X","X","X","X"]
[null,"V1","V1","V1","V1","V1","V1","V1","V1",null,"V1","V1","V1","V1","V1","V1","V1","V1"]
[]
["Write Ventilation",0,1,0,1,"X","X","X","X",null,0,1,0,1,"X","X","X","X"]
[null,"V1","V1","V1","V1","V1","V1","V1","V1",null,"V1","V1","V1","V1","V1","V1","V1","V1"]
[{"$nulls":25},100,9.4,{"$f":"AA25/Z25","v":0.094}]
["WriteValueEssai",0,1,1,0,"X","X","X","X",null,0,1,1,0,"X","X","X","X",{"$nulls":7},250,9.9,{"$f":"AA26/Z26","v":0.0396}]
[{"$nulls":5},"ID","ID","ID","ID",{"$nulls":5},"ID","ID","ID","ID",{"$nulls":7},500,15.9,{"$f":"AA27/Z27","v":0.0318}]
[null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",{"$nulls":7},1000,27.9,{"$f":"AA28/Z28","v":0.0279}]
[{"$nulls":25},2000,49.9,{"$f":"AA29/Z29","v":0.02495}]
["Stop",0,1,1,0,"X","X","X","X",null,0,1,1,0,"X","X","X","X"]
[{"$nulls":8},"On",{"$nulls":8},"ON"]
[]
["essai",1,0,0,0,"X","X","X","X",null,1,0,0,0,"X","X","X","X"]
[{"$nulls":8},"On",{"$nulls":8},"On"]
[]
["sync RTC",1,0,0,1,"X","X","X","X",null,1,0,0,1,"X","X","X","X"]
[null,"Y","Y","Y","Y","Y","Y","Y","Y",null,"Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"M","M","M","M","M","M","M","M",null,"M","M","M","M","M","M","M","M"]
[null,"J","J","J","J","J","J","J","J",null,"J","J","J","J","J","J","J","J"]
[null,"Day","Day","Day","Day","Day","Day","Day","Day",null,"Day","Day","Day","Day","Day","Day","Day","Day"]
[null,"H","H","H","H","H","H","H","H",null,"H","H","H","H","H","H","H","H"]
[null,"M","M","M","M","M","M","M","M",null,"M","M","M","M","M","M","M","M"]
[null,"S","S","S","S","S","S","S","S",null,"S","S","S","S","S","S","S","S"]
[]
["Status",1,0,1,0,"X","X","X","X",null,1,0,1,0,"X","X","X","X"]
[{"$nulls":10},"E","R","R","E","U","R",null,1]

{"sheet":"Status","index":5,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Code erreur","Type","Action"]
[0,"Tous est ok","ne rien faire"]
[1,"Perte de Syncro","Blynk.syncAll(); + syncro RTC"]

{"sheet":"AddEEPROM","index":6,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Nom","address Eeprpm","nbByte"]
["TabSortie[0].Extinxtion; ","0x0000",2]
["TabSortie[0].Demmarage; ","0x0002",2]
["TabSortie[0].PuissanceMax; ","0x0003",1]
["TabSortie[0].Pente; ","0x0004",1]
[]
["TabSortie[1].Extinxtion; ","0x0005"]
["TabSortie[1].Demmarage; ","0x0007"]
["TabSortie[1].PuissanceMax; ","0x0008"]
["TabSortie[1].Pente; "]
[]
[","]
[","]
[","]
["TabSortie[9].Extinxtion; "]
["TabSortie[9].Demmarage; "]
["TabSortie[9].PuissanceMax; "]
["TabSortie[9].Pente; "]