(export (version D)
  (design
    (source /home/remy/Projet/Cult/eda/LED/LED.sch)
    (date "lun. 18 janv. 2021 11:26:12 CET")
    (tool "Eeschema 5.1.7-a382d34a8~88~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source LED.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P1)
      (value CONN_01X05)
      (footprint Connector:LEDPCB)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF24F7))
    (comp (ref P2)
      (value CONN_01X05)
      (footprint Connector:LEDPCB)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF2D41))
    (comp (ref D1)
      (value F1)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF4407))
    (comp (ref D2)
      (value F2)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF5055))
    (comp (ref D3)
      (value F3)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF534A))
    (comp (ref R1)
      (value R)
      (footprint R:ciment_SMD)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF5752))
    (comp (ref D7)
      (value B1)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFC1E3))
    (comp (ref D8)
      (value B2)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFC1E9))
    (comp (ref D9)
      (value B3)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFC1EF))
    (comp (ref R3)
      (value R)
      (footprint R:ciment_SMD)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFC1F5))
    (comp (ref D10)
      (value R1)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFD055))
    (comp (ref D11)
      (value R2)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFD05B))
    (comp (ref D12)
      (value R3)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFD061))
    (comp (ref R4)
      (value R)
      (footprint R:ciment_SMD)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFD067))
    (comp (ref D15)
      (value R6)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFDC15))
    (comp (ref D16)
      (value R7)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFDC1B))
    (comp (ref D17)
      (value R8)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFDC21))
    (comp (ref R5)
      (value R)
      (footprint R:ciment_SMD)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFDC27))
    (comp (ref D13)
      (value R4)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFFEE9))
    (comp (ref D14)
      (value R5)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFFEEF))
    (comp (ref D18)
      (value R9)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFFEF5))
    (comp (ref D19)
      (value R10)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFFFEFB))
    (comp (ref U1)
      (value G6K-2F-Y)
      (footprint relay:G6K-2F)
      (libsource (lib relay) (part G6K-2F-Y) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 600045D2))
    (comp (ref U3)
      (value G6K-2F-Y)
      (footprint relay:G6K-2F)
      (libsource (lib relay) (part G6K-2F-Y) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003657C))
    (comp (ref D22)
      (value 1N4148W)
      (footprint D:SOD-123)
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60036587))
    (comp (ref Q3)
      (value NPN)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60036592))
    (comp (ref R8)
      (value 1K)
      (footprint R:0805)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60036598))
    (comp (ref D20)
      (value 1N4148W)
      (footprint D:SOD-123)
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003A19F))
    (comp (ref Q1)
      (value NPN)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003A1AA))
    (comp (ref R6)
      (value 1K)
      (footprint R:0805)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003A1B0))
    (comp (ref D21)
      (value 1N4148W)
      (footprint D:SOD-123)
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003BD65))
    (comp (ref Q2)
      (value NPN)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003BD70))
    (comp (ref R7)
      (value 1K)
      (footprint R:0805)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6003BD76))
    (comp (ref U2)
      (value G6K-2F-Y)
      (footprint relay:G6K-2F)
      (libsource (lib relay) (part G6K-2F-Y) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60003B8C))
    (comp (ref R2)
      (value R)
      (footprint R:ciment_SMD)
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF8AA5))
    (comp (ref D6)
      (value F6)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF8A9F))
    (comp (ref D5)
      (value F5)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF8A99))
    (comp (ref D4)
      (value F4)
      (footprint LED:COB_3W)
      (libsource (lib global) (part LED) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FFF8A93))
    (comp (ref P3)
      (value CONN_01X01)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 600580B4))
    (comp (ref P4)
      (value CONN_01X01)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6005FCF2)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib global) (part D)
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib global) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib global) (part NPN)
      (fields
        (field (name Reference) Q)
        (field (name Value) NPN))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib relay) (part G6K-2F-Y)
      (fields
        (field (name Reference) U)
        (field (name Value) G6K-2F-Y))
      (pins
        (pin (num 1) (name A2) (type input))
        (pin (num 2) (name NC1) (type input))
        (pin (num 3) (name COM1) (type input))
        (pin (num 4) (name NO1) (type output))
        (pin (num 5) (name NO2) (type input))
        (pin (num 6) (name COM2) (type input))
        (pin (num 7) (name NC2) (type input))
        (pin (num 8) (name A2) (type input)))))
  (libraries
    (library (logical conn)
      (uri /home/remy/Projet/Librairie_Kicad//schematic/conn.lib))
    (library (logical global)
      (uri /home/remy/Projet/Librairie_Kicad//schematic/global.lib))
    (library (logical relay)
      (uri /home/remy/Projet/Librairie_Kicad//schematic/relay.lib)))
  (nets
    (net (code 1) (name /flo)
      (node (ref P2) (pin 4))
      (node (ref R6) (pin 2))
      (node (ref P1) (pin 4)))
    (net (code 2) (name /12V)
      (node (ref U3) (pin 6))
      (node (ref P1) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref U3) (pin 3))
      (node (ref D22) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref D21) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref D20) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 1)))
    (net (code 3) (name "Net-(D20-Pad2)")
      (node (ref D20) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 4) (name "Net-(Q1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 5) (name /GND)
      (node (ref Q2) (pin 3))
      (node (ref D9) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref P2) (pin 5))
      (node (ref D19) (pin 1))
      (node (ref D14) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref Q3) (pin 3))
      (node (ref D6) (pin 1)))
    (net (code 6) (name "Net-(D21-Pad2)")
      (node (ref Q2) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref D21) (pin 2)))
    (net (code 7) (name "Net-(D22-Pad2)")
      (node (ref D22) (pin 2))
      (node (ref Q3) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 8) (name "Net-(Q3-Pad2)")
      (node (ref Q3) (pin 2))
      (node (ref R8) (pin 1)))
    (net (code 9) (name /full)
      (node (ref R8) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref P1) (pin 2)))
    (net (code 10) (name "Net-(D4-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 11) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 12) (name "Net-(U2-Pad2)")
      (node (ref U2) (pin 2)))
    (net (code 13) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 14) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 15) (name "Net-(U2-Pad5)")
      (node (ref U2) (pin 5)))
    (net (code 16) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 17) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 18) (name "Net-(D5-Pad1)")
      (node (ref D6) (pin 2))
      (node (ref D5) (pin 1)))
    (net (code 19) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 20) (name /Thermal)
      (node (ref P4) (pin 1))
      (node (ref P3) (pin 1)))
    (net (code 21) (name "Net-(Q2-Pad2)")
      (node (ref Q2) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 22) (name /B1)
      (node (ref U2) (pin 4))
      (node (ref R3) (pin 1)))
    (net (code 23) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 24) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 25) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 26) (name "Net-(D1-Pad1)")
      (node (ref D2) (pin 2))
      (node (ref D1) (pin 1)))
    (net (code 27) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 28) (name "Net-(D7-Pad1)")
      (node (ref D8) (pin 2))
      (node (ref D7) (pin 1)))
    (net (code 29) (name "Net-(D7-Pad2)")
      (node (ref D7) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 30) (name "Net-(D8-Pad1)")
      (node (ref D8) (pin 1))
      (node (ref D9) (pin 2)))
    (net (code 31) (name "Net-(D10-Pad1)")
      (node (ref D11) (pin 2))
      (node (ref D10) (pin 1)))
    (net (code 32) (name "Net-(D10-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref D10) (pin 2)))
    (net (code 33) (name "Net-(D11-Pad1)")
      (node (ref D12) (pin 2))
      (node (ref D11) (pin 1)))
    (net (code 34) (name "Net-(D12-Pad1)")
      (node (ref D12) (pin 1))
      (node (ref D13) (pin 2)))
    (net (code 35) (name /cro)
      (node (ref R7) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref P2) (pin 3)))
    (net (code 36) (name /R1)
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 37) (name /R2)
      (node (ref R5) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 38) (name /F2)
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 39) (name /F1)
      (node (ref U3) (pin 5))
      (node (ref R1) (pin 1)))
    (net (code 40) (name "Net-(D15-Pad1)")
      (node (ref D16) (pin 2))
      (node (ref D15) (pin 1)))
    (net (code 41) (name "Net-(D15-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref D15) (pin 2)))
    (net (code 42) (name "Net-(D16-Pad1)")
      (node (ref D17) (pin 2))
      (node (ref D16) (pin 1)))
    (net (code 43) (name "Net-(D17-Pad1)")
      (node (ref D18) (pin 2))
      (node (ref D17) (pin 1)))
    (net (code 44) (name "Net-(D13-Pad1)")
      (node (ref D13) (pin 1))
      (node (ref D14) (pin 2)))
    (net (code 45) (name "Net-(D18-Pad1)")
      (node (ref D18) (pin 1))
      (node (ref D19) (pin 2)))))