{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Feuil1","IO"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Feuil1","index":0,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Type","Nom","Lib arduino"]
["RTC","DS3231","https://github.com/NorthernWidget/DS3231/blob/master/DS3231.h"]
["Temp","DS18B20 "]

{"sheet":"IO","index":1,"n_rows":13,"n_cols":3,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Type","Nom","Desc"]
["O","Led1","croiss mer"]
["O","Led2","Croiss 2"]
["O","Led3","Flo 1"]
["O","Arrosage"]
["O","Ventilation"]
["O","Extraction"]
["Int","InterRTC"]
["I","Inter1","allum croiss mere"]
["I","Inter2","allum croiss"]
["I","Inter3","allum flo"]
["AI","tmp"]
["I","Hydro1","Hydro1"]