(module SK12D07VG4 (layer F.Cu) (tedit 613F323B)
  (fp_text reference REF** (at 0 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SK12D07VG4 (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6 1) (end -6 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -2) (end 6 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 -2) (end 6 1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 1) (end 6 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 2) (end 3 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 3 2) (end 3 4) (layer F.SilkS) (width 0.12))
  (fp_line (start 3 4) (end 1 4) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 4) (end 1 2) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 2) (end -6 2) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 2) (end -6 1) (layer F.SilkS) (width 0.12))
  (pad "" thru_hole circle (at -4.1 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 4.1 0) (size 1.95 1.95) (drill 1.25) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
  (model ${MY_PATH}/3D/SW.3dshapes/SK12D07VG4.step
    (offset (xyz -4.25 -2.25 4.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
