(module TO-252 (layer F.Cu) (tedit 60798D6E)
  (fp_text reference REF** (at -4 6 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TO-252 (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 -3) (end 4 -3) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 4) (end 3 4) (layer F.SilkS) (width 0.12))
  (fp_line (start 3 4) (end 3 8) (layer F.SilkS) (width 0.12))
  (fp_line (start 3 8) (end -3 8) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 8) (end -3 4) (layer F.SilkS) (width 0.12))
  (fp_line (start -3 4) (end -4 4) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 4) (end -4 -3) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 -3) (end 4 4) (layer F.SilkS) (width 0.12))
  (pad 2 smd rect (at 0 0) (size 6.4 5.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.28 6.3 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.28 6.3 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask))
)
