(export (version D)
  (design
    (source C:\Users\e_rcluze\Documents\Autres\Projet\ordinateur_aquarium\Eda\Fille\Fille.sch)
    (date "25/09/2019 12:30:47")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Fille.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref K5)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89C6C3))
    (comp (ref U1)
      (value ULN2803A)
      (footprint U:SOP18)
      (fields
        (field (name Partkeepr) 2400))
      (libsource (lib TI) (part ULN2803A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88F542))
    (comp (ref U2)
      (value PCF8574)
      (footprint U:SO16)
      (fields
        (field (name Partkeepr) 1501))
      (libsource (lib NXP) (part PCF8574) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88C7B3))
    (comp (ref JP1)
      (value CONN_02X01)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88D1B7))
    (comp (ref JP2)
      (value CONN_02X01)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88D524))
    (comp (ref JP3)
      (value CONN_02X01)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88D584))
    (comp (ref R1)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88D89F))
    (comp (ref R2)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88DCE9))
    (comp (ref R3)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D88DDED))
    (comp (ref P2)
      (value OUT_1_1)
      (footprint Connector:Bornier5.08_1X4)
      (fields
        (field (name Partkeepr) 7))
      (libsource (lib conn) (part CONN_01X04) (description "Connector 01x04"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D891229))
    (comp (ref P3)
      (value OUT_1_2)
      (footprint Connector:Bornier5.08_1X4)
      (fields
        (field (name Partkeepr) 7))
      (libsource (lib conn) (part CONN_01X04) (description "Connector 01x04"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89141F))
    (comp (ref K6)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D894B7B))
    (comp (ref K1)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D895001))
    (comp (ref K2)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D895017))
    (comp (ref K7)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D895734))
    (comp (ref K8)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89574A))
    (comp (ref K3)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D895760))
    (comp (ref K4)
      (value SRD-03VDC-SL-C)
      (footprint relay:SRD-03VDC-SL-C)
      (fields
        (field (name Partkeepr) 350))
      (libsource (lib relay) (part SRD-03VDC-SL-C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D895776))
    (comp (ref MH1)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description "Connector 01x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89F2F5))
    (comp (ref MH2)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description "Connector 01x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89F5F1))
    (comp (ref MH3)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description "Connector 01x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89F659))
    (comp (ref MH4)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description "Connector 01x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D89F6B3))
    (comp (ref JP4)
      (value 230V_relais0)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8AE36D))
    (comp (ref JP5)
      (value 12V_relais0)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8AE453))
    (comp (ref JP6)
      (value 230V_relais2)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8AEF02))
    (comp (ref JP7)
      (value 12V_relais2)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8AEF09))
    (comp (ref JP8)
      (value 230V_relais4)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B02EC))
    (comp (ref JP9)
      (value 12V_relais4)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B02F3))
    (comp (ref JP10)
      (value 230V_relais6)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B02FE))
    (comp (ref JP11)
      (value 12V_relais6)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0305))
    (comp (ref JP12)
      (value 230V_relais1)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0651))
    (comp (ref JP13)
      (value 12V_relais1)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0658))
    (comp (ref JP14)
      (value 230V_relais3)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0663))
    (comp (ref JP15)
      (value 12V_relais3)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B066A))
    (comp (ref JP16)
      (value 230V_relais5)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0677))
    (comp (ref JP17)
      (value 12V_relais5)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B067E))
    (comp (ref JP18)
      (value 230V_relais7)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0689))
    (comp (ref JP19)
      (value 12V_relais7)
      (footprint Jumper:SolderStrap2.5mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_02X01) (description "Connector 02x01"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8B0690))
    (comp (ref P7)
      (value 230V)
      (footprint Connector:Bornier5_1x2)
      (fields
        (field (name Partkeepr) 0))
      (libsource (lib conn) (part CONN_01X02) (description "Connector 01x02"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8A139E))
    (comp (ref P8)
      (value 12V)
      (footprint Connector:Bornier5_1x2)
      (fields
        (field (name Partkeepr) 0))
      (libsource (lib conn) (part CONN_01X02) (description "Connector 01x02"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8A13A9))
    (comp (ref P1)
      (value Carte_Carte)
      (footprint Connector:PinHeader2.54_1X6)
      (libsource (lib conn) (part CONN_01X06) (description "Connector 01x06"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8A2BCE))
    (comp (ref P6)
      (value Carte_Carte)
      (footprint Connector:PinHeader2.54_1X6)
      (libsource (lib conn) (part CONN_01X06) (description "Connector 01x06"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8A2F10)))
  (libparts
    (libpart (lib NXP) (part PCF8574)
      (fields
        (field (name Reference) U)
        (field (name Value) PCF8574))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name P0) (type output))
        (pin (num 5) (name P1) (type output))
        (pin (num 6) (name P2) (type output))
        (pin (num 7) (name P3) (type output))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name P4) (type output))
        (pin (num 10) (name P5) (type output))
        (pin (num 11) (name P6) (type output))
        (pin (num 12) (name P7) (type output))
        (pin (num 13) (name INT) (type input))
        (pin (num 14) (name SCL) (type BiDi))
        (pin (num 15) (name SDA) (type BiDi))
        (pin (num 16) (name VDD) (type power_in))))
    (libpart (lib TI) (part ULN2803A)
      (fields
        (field (name Reference) U)
        (field (name Value) ULN2803A))
      (pins
        (pin (num 1) (name 1B) (type input))
        (pin (num 2) (name 2B) (type input))
        (pin (num 3) (name 3B) (type input))
        (pin (num 4) (name 4B) (type input))
        (pin (num 5) (name 5B) (type input))
        (pin (num 6) (name 6B) (type input))
        (pin (num 7) (name 7B) (type input))
        (pin (num 8) (name 8B) (type input))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name COM) (type power_in))
        (pin (num 11) (name 8C) (type output))
        (pin (num 12) (name 7C) (type output))
        (pin (num 13) (name 6C) (type output))
        (pin (num 14) (name 5C) (type output))
        (pin (num 15) (name 4C) (type output))
        (pin (num 16) (name 3C) (type output))
        (pin (num 17) (name 2C) (type output))
        (pin (num 18) (name 1C) (type output))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_02X01)
      (description "Connector 02x01")
      (footprints
        (fp Pin_Header_Straight_2X01)
        (fp Pin_Header_Angled_2X01)
        (fp Socket_Strip_Straight_2X01)
        (fp Socket_Strip_Angled_2X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X01))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib relay) (part SRD-03VDC-SL-C)
      (fields
        (field (name Reference) K)
        (field (name Value) SRD-03VDC-SL-C))
      (pins
        (pin (num 1) (name A1) (type input))
        (pin (num 2) (name A2) (type input))
        (pin (num 3) (name COM) (type input))
        (pin (num 4) (name NO) (type input))
        (pin (num 5) (name NC) (type input)))))
  (libraries
    (library (logical NXP)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/NXP.lib))
    (library (logical TI)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/TI.lib))
    (library (logical conn)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/conn.lib))
    (library (logical global)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/global.lib))
    (library (logical relay)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/relay.lib)))
  (nets
    (net (code 1) (name /12V)
      (node (ref JP13) (pin 1))
      (node (ref JP15) (pin 1))
      (node (ref JP5) (pin 1))
      (node (ref P8) (pin 2))
      (node (ref JP7) (pin 1))
      (node (ref P8) (pin 1))
      (node (ref JP17) (pin 1))
      (node (ref JP11) (pin 1))
      (node (ref JP9) (pin 1))
      (node (ref JP19) (pin 1)))
    (net (code 2) (name /230V)
      (node (ref JP12) (pin 1))
      (node (ref JP16) (pin 1))
      (node (ref JP18) (pin 1))
      (node (ref P7) (pin 1))
      (node (ref P7) (pin 2))
      (node (ref JP4) (pin 1))
      (node (ref JP6) (pin 1))
      (node (ref JP14) (pin 1))
      (node (ref JP10) (pin 1))
      (node (ref JP8) (pin 1)))
    (net (code 3) (name "Net-(K8-Pad5)")
      (node (ref K8) (pin 5)))
    (net (code 4) (name /BOBINE_6)
      (node (ref K4) (pin 1))
      (node (ref U1) (pin 12)))
    (net (code 5) (name "Net-(K3-Pad5)")
      (node (ref K3) (pin 5)))
    (net (code 6) (name /BOBINE_4)
      (node (ref U1) (pin 14))
      (node (ref K3) (pin 1)))
    (net (code 7) (name /BOBINE_7)
      (node (ref K8) (pin 1))
      (node (ref U1) (pin 11)))
    (net (code 8) (name "Net-(K7-Pad5)")
      (node (ref K7) (pin 5)))
    (net (code 9) (name "Net-(MH2-Pad1)")
      (node (ref MH2) (pin 1)))
    (net (code 10) (name "Net-(MH4-Pad1)")
      (node (ref MH4) (pin 1)))
    (net (code 11) (name "Net-(MH3-Pad1)")
      (node (ref MH3) (pin 1)))
    (net (code 12) (name "Net-(MH1-Pad1)")
      (node (ref MH1) (pin 1)))
    (net (code 13) (name "Net-(K4-Pad5)")
      (node (ref K4) (pin 5)))
    (net (code 14) (name /SDA)
      (node (ref P6) (pin 3))
      (node (ref U2) (pin 15))
      (node (ref P1) (pin 3)))
    (net (code 15) (name /SCL)
      (node (ref P6) (pin 5))
      (node (ref P1) (pin 5))
      (node (ref U2) (pin 14)))
    (net (code 16) (name /GND)
      (node (ref P6) (pin 6))
      (node (ref P6) (pin 4))
      (node (ref JP3) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref JP2) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref P1) (pin 6))
      (node (ref P1) (pin 4))
      (node (ref JP1) (pin 1)))
    (net (code 17) (name /230_2)
      (node (ref JP7) (pin 2))
      (node (ref K2) (pin 3))
      (node (ref JP6) (pin 2)))
    (net (code 18) (name /230_1)
      (node (ref K5) (pin 3))
      (node (ref JP12) (pin 2))
      (node (ref JP13) (pin 2)))
    (net (code 19) (name /230_0)
      (node (ref JP4) (pin 2))
      (node (ref JP5) (pin 2))
      (node (ref K1) (pin 3)))
    (net (code 20) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 21) (name /230_3)
      (node (ref JP15) (pin 2))
      (node (ref JP14) (pin 2))
      (node (ref K6) (pin 3)))
    (net (code 22) (name /230_6)
      (node (ref JP11) (pin 2))
      (node (ref JP10) (pin 2))
      (node (ref K4) (pin 3)))
    (net (code 23) (name /230_5)
      (node (ref JP17) (pin 2))
      (node (ref JP16) (pin 2))
      (node (ref K7) (pin 3)))
    (net (code 24) (name /230_7)
      (node (ref K8) (pin 3))
      (node (ref JP19) (pin 2))
      (node (ref JP18) (pin 2)))
    (net (code 25) (name /230_4)
      (node (ref JP9) (pin 2))
      (node (ref K3) (pin 3))
      (node (ref JP8) (pin 2)))
    (net (code 26) (name /A0)
      (node (ref JP1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 27) (name /IO_4)
      (node (ref U1) (pin 5))
      (node (ref U2) (pin 9)))
    (net (code 28) (name /IO_3)
      (node (ref U2) (pin 7))
      (node (ref U1) (pin 4)))
    (net (code 29) (name /IO_2)
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 6)))
    (net (code 30) (name /3.3V)
      (node (ref U2) (pin 16))
      (node (ref K8) (pin 2))
      (node (ref K5) (pin 2))
      (node (ref K6) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref K7) (pin 2))
      (node (ref K3) (pin 2))
      (node (ref K2) (pin 2))
      (node (ref K4) (pin 2))
      (node (ref K1) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref P6) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref U1) (pin 10))
      (node (ref P6) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 31) (name /IO_0)
      (node (ref U1) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 32) (name "Net-(K5-Pad5)")
      (node (ref K5) (pin 5)))
    (net (code 33) (name /IO_1)
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 2)))
    (net (code 34) (name /A2)
      (node (ref U2) (pin 3))
      (node (ref R3) (pin 2))
      (node (ref JP3) (pin 2)))
    (net (code 35) (name /A1)
      (node (ref JP2) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 36) (name /IO_7)
      (node (ref U2) (pin 12))
      (node (ref U1) (pin 8)))
    (net (code 37) (name /IO_6)
      (node (ref U1) (pin 7))
      (node (ref U2) (pin 11)))
    (net (code 38) (name /IO_5)
      (node (ref U2) (pin 10))
      (node (ref U1) (pin 6)))
    (net (code 39) (name /BOBINE_3)
      (node (ref K6) (pin 1))
      (node (ref U1) (pin 15)))
    (net (code 40) (name "Net-(K6-Pad5)")
      (node (ref K6) (pin 5)))
    (net (code 41) (name /BOBINE_5)
      (node (ref U1) (pin 13))
      (node (ref K7) (pin 1)))
    (net (code 42) (name "Net-(K2-Pad5)")
      (node (ref K2) (pin 5)))
    (net (code 43) (name /BOBINE_2)
      (node (ref K2) (pin 1))
      (node (ref U1) (pin 16)))
    (net (code 44) (name "Net-(K1-Pad5)")
      (node (ref K1) (pin 5)))
    (net (code 45) (name /BOBINE_0)
      (node (ref K1) (pin 1))
      (node (ref U1) (pin 18)))
    (net (code 46) (name /OUT7)
      (node (ref P3) (pin 4))
      (node (ref K8) (pin 4)))
    (net (code 47) (name /BOBINE_1)
      (node (ref K5) (pin 1))
      (node (ref U1) (pin 17)))
    (net (code 48) (name /OUT6)
      (node (ref P3) (pin 3))
      (node (ref K4) (pin 4)))
    (net (code 49) (name /OUT5)
      (node (ref P3) (pin 2))
      (node (ref K7) (pin 4)))
    (net (code 50) (name /OUT4)
      (node (ref P3) (pin 1))
      (node (ref K3) (pin 4)))
    (net (code 51) (name /OUT3)
      (node (ref P2) (pin 4))
      (node (ref K6) (pin 4)))
    (net (code 52) (name /OUT2)
      (node (ref K2) (pin 4))
      (node (ref P2) (pin 3)))
    (net (code 53) (name /OUT1)
      (node (ref P2) (pin 2))
      (node (ref K5) (pin 4)))
    (net (code 54) (name /OUT0)
      (node (ref K1) (pin 4))
      (node (ref P2) (pin 1)))))