(export (version D)
  (design
    (source C:\Users\e_rcluze\Documents\Autres\projet\Ordinateur_Aquarium\Eda\Ordinateur\Ordinateur.sch)
    (date "14/02/2020 10:37:36")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Ordinateur.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P6)
      (value TemperatureEau)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AE70BC))
    (comp (ref J1)
      (value Micro_USB)
      (footprint Connector:Micro-USB)
      (fields
        (field (name Partkeepr) 50))
      (libsource (lib conn) (part Micro_USB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFACA99))
    (comp (ref Y1)
      (value Crystal)
      (footprint Y:5032)
      (fields
        (field (name Partkeepr) 1650))
      (libsource (lib global) (part Crystal) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFADCC2))
    (comp (ref C3)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFADE87))
    (comp (ref C6)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFADF5D))
    (comp (ref C7)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE0D9))
    (comp (ref SW2)
      (value SW_PUSH)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib global) (part SW_PUSH) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE368))
    (comp (ref SW1)
      (value SW_PUSH)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib global) (part SW_PUSH) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE461))
    (comp (ref C11)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE512))
    (comp (ref C10)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE5F9))
    (comp (ref R13)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE6C4))
    (comp (ref R7)
      (value 10K)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE837))
    (comp (ref C1)
      (value C)
      (footprint C:0603)
      (fields
        (field (name Partkeepr) 600))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB0814))
    (comp (ref C2)
      (value C)
      (footprint C:0603)
      (fields
        (field (name Partkeepr) 600))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB08E5))
    (comp (ref C5)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB4DDE))
    (comp (ref C9)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB4EA5))
    (comp (ref C4)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB547F))
    (comp (ref C8)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB5DDF))
    (comp (ref U3)
      (value M24C32)
      (footprint U:SO8N)
      (fields
        (field (name Partkeepr) 1700))
      (libsource (lib ST) (part M24C32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB6B89))
    (comp (ref P15)
      (value I2C)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC4271))
    (comp (ref R12)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC8C4D))
    (comp (ref R14)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC8D8E))
    (comp (ref R15)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFC8E58))
    (comp (ref R24)
      (value 100)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 912))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAF333))
    (comp (ref BT1)
      (value Battery)
      (footprint Connector:batterie)
      (fields
        (field (name Partkeepr) 3))
      (libsource (lib global) (part Battery) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE8A3))
    (comp (ref R6)
      (value 10K)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAF4AC))
    (comp (ref SW3)
      (value mt-OO8a)
      (footprint SW:MT-008a)
      (fields
        (field (name Partkeepr) 201))
      (libsource (lib global) (part mt-OO8a) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFEAC87))
    (comp (ref R16)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFED7CC))
    (comp (ref R17)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFEE164))
    (comp (ref R18)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFEE35C))
    (comp (ref R19)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFEE591))
    (comp (ref R20)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFEE68F))
    (comp (ref U4)
      (value HD44780)
      (footprint Connector:PinHeader2.54_1X16)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib afficheur) (part HD44780) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFAE1CC))
    (comp (ref P17)
      (value CONN_01X05)
      (footprint Connector:PinHeader2.54_1X5)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B5832B2))
    (comp (ref VR1)
      (value 10K)
      (footprint R:3296)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Poten) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B58DB3E))
    (comp (ref Q1)
      (value N_MOSFET)
      (footprint U:SOT-223)
      (fields
        (field (name Partkeepr) 2002))
      (libsource (lib global) (part N_MOSFET) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B576977))
    (comp (ref R27)
      (value 510)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 913))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B4B))
    (comp (ref R29)
      (value 330)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 914))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B53))
    (comp (ref C16)
      (value 10µF)
      (footprint C:CP_CMS5X5.8)
      (fields
        (field (name Partkeepr) 609))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B5B))
    (comp (ref C14)
      (value 100nF)
      (footprint C:3216-18)
      (fields
        (field (name Partkeepr) 610))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B65))
    (comp (ref U7)
      (value LM317)
      (footprint U:LM317)
      (fields
        (field (name Partkeepr) 1800))
      (libsource (lib global) (part LM317) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B6D))
    (comp (ref C18)
      (value 1µF)
      (footprint C:CP_CMS4X5.8)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B8B))
    (comp (ref D10)
      (value D)
      (footprint D:SMA)
      (fields
        (field (name Partkeepr) 1302))
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18B9A))
    (comp (ref R26)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BA6))
    (comp (ref R28)
      (value 330)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 914))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BAE))
    (comp (ref C15)
      (value 10µF)
      (footprint C:CP_CMS5X5.8)
      (fields
        (field (name Partkeepr) 609))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BB6))
    (comp (ref C13)
      (value 100nF)
      (footprint C:3216-18)
      (fields
        (field (name Partkeepr) 610))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BC0))
    (comp (ref U5)
      (value LM317)
      (footprint U:LM317)
      (fields
        (field (name Partkeepr) 1800))
      (libsource (lib global) (part LM317) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BC8))
    (comp (ref C17)
      (value 1µF)
      (footprint C:CP_CMS4X5.8)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BE6))
    (comp (ref D9)
      (value D)
      (footprint D:SMA)
      (fields
        (field (name Partkeepr) 1302))
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF18BF5))
    (comp (ref R30)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CDE7))
    (comp (ref R31)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CDEF))
    (comp (ref C20)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE05))
    (comp (ref R32)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE0F))
    (comp (ref R33)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE19))
    (comp (ref C19)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE3A))
    (comp (ref P18)
      (value ProgESP)
      (footprint Connector:PinHeader2.54_1X3)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE43))
    (comp (ref P19)
      (value CONN_01X01)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D0CCC09))
    (comp (ref P20)
      (value CONN_01X01)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D0D5B33))
    (comp (ref P21)
      (value CONN_01X01)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D0D5C25))
    (comp (ref P22)
      (value CONN_01X01)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D0D5D13))
    (comp (ref P8)
      (value Carte_Carte)
      (footprint Connector:PinHeader2.54_1X6)
      (fields
        (field (name Partkeepr) 102))
      (libsource (lib conn) (part CONN_01X06) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8BE836))
    (comp (ref P7)
      (value Carte_Carte)
      (footprint Connector:PinHeader2.54_1X6)
      (fields
        (field (name Partkeepr) 101))
      (libsource (lib conn) (part CONN_01X06) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8BF7A1))
    (comp (ref P1)
      (value TechniqueBas)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D98357A))
    (comp (ref SJ2)
      (value TechBas5V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D983584))
    (comp (ref SJ3)
      (value TechBasGND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D98358B))
    (comp (ref P2)
      (value TechniqueHaut)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9DF563))
    (comp (ref SJ4)
      (value TechHaut5V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9DF56C))
    (comp (ref SJ5)
      (value TechHautGND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9DF572))
    (comp (ref P3)
      (value CuveHaut)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E40))
    (comp (ref SJ6)
      (value CuveHaut5V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E49))
    (comp (ref SJ7)
      (value CuveBasGND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E4F))
    (comp (ref P4)
      (value ReserveBas)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E59))
    (comp (ref SJ8)
      (value ReseBas5V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E62))
    (comp (ref SJ9)
      (value ReseBasGND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E3E68))
    (comp (ref P5)
      (value CapteurAutres2)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC2A))
    (comp (ref SJ10)
      (value Autres25V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC33))
    (comp (ref SJ11)
      (value Autres2GND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC39))
    (comp (ref P9)
      (value CapteurAutres1)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC43))
    (comp (ref SJ12)
      (value Autres15V)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC4C))
    (comp (ref SJ13)
      (value Autres1GND)
      (footprint Jumper:SolderStrap0603)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9FBC52))
    (comp (ref P10)
      (value TemperatureAir)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA5D609))
    (comp (ref P11)
      (value BNC)
      (footprint Connector:BNC)
      (fields
        (field (name Partkeepr) 150))
      (libsource (lib conn) (part CONN_01X02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA726A1))
    (comp (ref U9)
      (value LM2663)
      (footprint U:SOP8)
      (fields
        (field (name Partkeepr) 1803))
      (libsource (lib TI) (part LM2663) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA78963))
    (comp (ref C21)
      (value 47µF)
      (footprint C:2312_pola)
      (fields
        (field (name Partkeepr) 611))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAA3244))
    (comp (ref U6)
      (value TLC272)
      (footprint U:SOP8)
      (fields
        (field (name Partkeepr) 2401))
      (libsource (lib TI) (part TLC272) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB06FB))
    (comp (ref R3)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB79DF))
    (comp (ref C12)
      (value 47µF)
      (footprint C:2312_pola)
      (fields
        (field (name Partkeepr) 611))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB9AD4))
    (comp (ref R8)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DABA3C1))
    (comp (ref R5)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DABA4AD))
    (comp (ref R4)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DABA5B3))
    (comp (ref R9)
      (value 27K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 918))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAD93B2))
    (comp (ref R10)
      (value 27K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 918))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAF2F9F))
    (comp (ref R2)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAF39BF))
    (comp (ref R1)
      (value 43K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 919))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB139EC))
    (comp (ref P16)
      (value Alim)
      (footprint Connector:Bornier5_1x2)
      (fields
        (field (name Partkeepr) 0))
      (libsource (lib conn) (part CONN_01X02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B573EE1))
    (comp (ref SJ1)
      (value Mode)
      (footprint Jumper:Jumper_2.54mm)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CE26))
    (comp (ref U8)
      (value ESP-12F)
      (footprint Module:ESP-12F)
      (fields
        (field (name Partkeepr) 2800))
      (libsource (lib Module) (part ESP-12F) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF5CDD9))
    (comp (ref U2)
      (value M41T83)
      (footprint U:SOX18)
      (fields
        (field (name Partkeepr) 1600))
      (libsource (lib ST) (part M41T83) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFB6C98))
    (comp (ref P12)
      (value Ventilo_1)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9A4041))
    (comp (ref P13)
      (value Ventilo_2)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9A417D))
    (comp (ref Q2)
      (value 2222A)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9B7C9F))
    (comp (ref R22)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9B7E20))
    (comp (ref R25)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9B7F5E))
    (comp (ref C22)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9B8114))
    (comp (ref R11)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9B824D))
    (comp (ref Q3)
      (value 2222A)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E4BC3))
    (comp (ref R23)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E4BCA))
    (comp (ref R34)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E4BD1))
    (comp (ref C23)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E4BD8))
    (comp (ref R21)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D9E4BDF))
    (comp (ref P14)
      (value Ventilo_3)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA13A0A))
    (comp (ref P23)
      (value Ventilo_4)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA13A11))
    (comp (ref P24)
      (value Ventilo_5)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA1B48A))
    (comp (ref P25)
      (value Ventilo_6)
      (footprint Connector:JST_2.54_4)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X04) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA1B491))
    (comp (ref Q4)
      (value 2222A)
      (footprint U:SOT23-3)
      (libsource (lib global) (part NPN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA42413))
    (comp (ref R36)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA4241A))
    (comp (ref R37)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA42421))
    (comp (ref C24)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA42428))
    (comp (ref R35)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA4242F))
    (comp (ref U1)
      (value STM32F401RC)
      (footprint U:LQFP64)
      (fields
        (field (name Partkeepr) 2102))
      (libsource (lib ST) (part STM32F401RC) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59AE71DE))
    (comp (ref R38)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAA64C1))
    (comp (ref R39)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAA6670))
    (comp (ref R40)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAD452D))
    (comp (ref R41)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAD4535))
    (comp (ref R42)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAE4856))
    (comp (ref R43)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAE485E))
    (comp (ref R44)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAECAA6))
    (comp (ref R45)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAECAAE))
    (comp (ref R46)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAF4BCE))
    (comp (ref R47)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAF4BD6))
    (comp (ref R48)
      (value 4.7K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 917))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAFCD32))
    (comp (ref R49)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAFCD3A))
    (comp (ref R52)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E431E17))
    (comp (ref R53)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4328A6))
    (comp (ref R51)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E432ADC))
    (comp (ref R50)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E432C12)))
  (libparts
    (libpart (lib Module) (part ESP-12F)
      (fields
        (field (name Reference) U)
        (field (name Value) ESP-12F))
      (pins
        (pin (num 1) (name RST) (type input))
        (pin (num 2) (name ADC) (type input))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name GPIO16) (type input))
        (pin (num 5) (name GPIO14) (type input))
        (pin (num 6) (name GPIO12) (type input))
        (pin (num 7) (name GPIO13) (type input))
        (pin (num 8) (name VCC) (type input))
        (pin (num 9) (name CS0) (type input))
        (pin (num 10) (name MISO) (type input))
        (pin (num 11) (name GPIO9) (type input))
        (pin (num 12) (name GPIO10) (type input))
        (pin (num 13) (name MOSI) (type input))
        (pin (num 14) (name SCLK) (type input))
        (pin (num 15) (name GND) (type input))
        (pin (num 16) (name GPIO15) (type input))
        (pin (num 17) (name GPIO2) (type input))
        (pin (num 18) (name GPIO0) (type input))
        (pin (num 19) (name GPIO4) (type input))
        (pin (num 20) (name GPIO5) (type input))
        (pin (num 21) (name RXD) (type input))
        (pin (num 22) (name TXD) (type input))))
    (libpart (lib ST) (part M24C32)
      (fields
        (field (name Reference) U)
        (field (name Value) M24C32))
      (pins
        (pin (num 1) (name E0) (type input))
        (pin (num 2) (name E1) (type input))
        (pin (num 3) (name E2) (type input))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name ~WC) (type input))
        (pin (num 7) (name SCL) (type input))
        (pin (num 8) (name SDA) (type BiDi))))
    (libpart (lib ST) (part M41T83)
      (fields
        (field (name Reference) U)
        (field (name Value) M41T83))
      (pins
        (pin (num 1) (name NC) (type input))
        (pin (num 2) (name NF) (type input))
        (pin (num 3) (name NF) (type input))
        (pin (num 4) (name NC) (type input))
        (pin (num 5) (name ~RST) (type input))
        (pin (num 6) (name DU) (type input))
        (pin (num 7) (name SQW) (type input))
        (pin (num 8) (name VBAT) (type input))
        (pin (num 9) (name VSS) (type input))
        (pin (num 10) (name SDA) (type input))
        (pin (num 11) (name SCL) (type input))
        (pin (num 12) (name ~IRQ1~/FT/OUT) (type input))
        (pin (num 13) (name NC) (type input))
        (pin (num 14) (name ~IRQ2) (type input))
        (pin (num 15) (name VCC) (type input))
        (pin (num 16) (name NF) (type input))
        (pin (num 17) (name NF) (type input))
        (pin (num 18) (name NC) (type input))))
    (libpart (lib ST) (part STM32F401RC)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F401RC))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PH0) (type BiDi))
        (pin (num 6) (name PH1) (type BiDi))
        (pin (num 7) (name NRST) (type BiDi))
        (pin (num 8) (name PC0) (type BiDi))
        (pin (num 9) (name PC1) (type BiDi))
        (pin (num 10) (name PC2) (type BiDi))
        (pin (num 11) (name PC3) (type BiDi))
        (pin (num 12) (name VSSA) (type power_in))
        (pin (num 13) (name VDDA) (type power_in))
        (pin (num 14) (name PA0) (type BiDi))
        (pin (num 15) (name PA1) (type BiDi))
        (pin (num 16) (name PA2) (type BiDi))
        (pin (num 17) (name PA3) (type BiDi))
        (pin (num 18) (name VSS) (type power_in))
        (pin (num 19) (name VDD) (type power_in))
        (pin (num 20) (name PA4) (type BiDi))
        (pin (num 21) (name PA5) (type BiDi))
        (pin (num 22) (name PA6) (type BiDi))
        (pin (num 23) (name PA7) (type BiDi))
        (pin (num 24) (name PC4) (type BiDi))
        (pin (num 25) (name PC5) (type BiDi))
        (pin (num 26) (name PB0) (type BiDi))
        (pin (num 27) (name PB1) (type BiDi))
        (pin (num 28) (name PB2) (type BiDi))
        (pin (num 29) (name PB10) (type BiDi))
        (pin (num 30) (name VCAP1) (type power_in))
        (pin (num 31) (name VSS) (type power_in))
        (pin (num 32) (name VDD) (type power_in))
        (pin (num 33) (name PB12) (type BiDi))
        (pin (num 34) (name PB13) (type BiDi))
        (pin (num 35) (name PB14) (type BiDi))
        (pin (num 36) (name PB15) (type BiDi))
        (pin (num 37) (name PC6) (type BiDi))
        (pin (num 38) (name PC7) (type BiDi))
        (pin (num 39) (name PC8) (type BiDi))
        (pin (num 40) (name PC9) (type BiDi))
        (pin (num 41) (name PA8) (type BiDi))
        (pin (num 42) (name PA9) (type BiDi))
        (pin (num 43) (name PA10) (type BiDi))
        (pin (num 44) (name PA11) (type BiDi))
        (pin (num 45) (name PA12) (type BiDi))
        (pin (num 46) (name PA13) (type BiDi))
        (pin (num 47) (name VDD) (type power_in))
        (pin (num 48) (name VSS) (type power_in))
        (pin (num 49) (name PA14) (type BiDi))
        (pin (num 50) (name PA15) (type BiDi))
        (pin (num 51) (name PC10) (type BiDi))
        (pin (num 52) (name PC11) (type BiDi))
        (pin (num 53) (name PC12) (type BiDi))
        (pin (num 54) (name PD2) (type BiDi))
        (pin (num 55) (name PB3) (type BiDi))
        (pin (num 56) (name PB4) (type BiDi))
        (pin (num 57) (name PB5) (type BiDi))
        (pin (num 58) (name PB6) (type BiDi))
        (pin (num 59) (name PB7) (type BiDi))
        (pin (num 60) (name BOOT0) (type input))
        (pin (num 61) (name PB8) (type BiDi))
        (pin (num 62) (name PB9) (type BiDi))
        (pin (num 63) (name VSS) (type power_in))
        (pin (num 64) (name VDD) (type power_in))))
    (libpart (lib TI) (part LM2663)
      (fields
        (field (name Reference) U)
        (field (name Value) LM2663))
      (pins
        (pin (num 1) (name SD) (type input))
        (pin (num 2) (name CAP+) (type passive))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name CAP-) (type passive))
        (pin (num 5) (name Out) (type power_out))
        (pin (num 6) (name LV) (type input))
        (pin (num 7) (name OSC) (type input))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib TI) (part TLC272)
      (fields
        (field (name Reference) U)
        (field (name Value) TLC272))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name IN-) (type input))
        (pin (num 3) (name IN+) (type input))
        (pin (num 4) (name -) (type input))
        (pin (num 5) (name IN+) (type input))
        (pin (num 6) (name IN-) (type input))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name +) (type input))))
    (libpart (lib afficheur) (part HD44780)
      (fields
        (field (name Reference) U)
        (field (name Value) HD44780))
      (pins
        (pin (num 1) (name VSS) (type input))
        (pin (num 2) (name VDD) (type input))
        (pin (num 3) (name Vee) (type input))
        (pin (num 4) (name RS) (type input))
        (pin (num 5) (name R/W) (type input))
        (pin (num 6) (name E) (type input))
        (pin (num 7) (name D0) (type input))
        (pin (num 8) (name D1) (type input))
        (pin (num 9) (name D2) (type input))
        (pin (num 10) (name D3) (type input))
        (pin (num 11) (name D4) (type input))
        (pin (num 12) (name D5) (type input))
        (pin (num 13) (name D6) (type input))
        (pin (num 14) (name D7) (type input))
        (pin (num 15) (name A) (type input))
        (pin (num 16) (name K) (type input))))
    (libpart (lib conn) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part Micro_USB)
      (fields
        (field (name Reference) J)
        (field (name Value) Micro_USB))
      (pins
        (pin (num 0) (name USB_SH) (type input))
        (pin (num 1) (name USB_VBUS) (type input))
        (pin (num 2) (name USB_N) (type input))
        (pin (num 3) (name USB_P) (type input))
        (pin (num 4) (name USB_ID) (type input))
        (pin (num 5) (name USB_GND) (type input))))
    (libpart (lib global) (part Battery)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part C)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part CP)
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part Crystal)
      (footprints
        (fp Crystal_*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib global) (part D)
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib global) (part Jumper)
      (fields
        (field (name Reference) SJ)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part LM317)
      (fields
        (field (name Reference) U)
        (field (name Value) LM317))
      (pins
        (pin (num 1) (name Adj) (type input))
        (pin (num 2) (name Vout) (type power_out))
        (pin (num 3) (name Vin) (type power_in))))
    (libpart (lib global) (part NPN)
      (fields
        (field (name Reference) Q)
        (field (name Value) NPN))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))))
    (libpart (lib global) (part N_MOSFET)
      (fields
        (field (name Reference) Q)
        (field (name Value) N_MOSFET))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name S) (type input))))
    (libpart (lib global) (part Poten)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) VR)
        (field (name Value) Poten))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part SW_PUSH)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib global) (part mt-OO8a)
      (fields
        (field (name Reference) SW)
        (field (name Value) mt-OO8a))
      (pins
        (pin (num 1) (name Left) (type input))
        (pin (num 2) (name Select) (type input))
        (pin (num 3) (name Down) (type input))
        (pin (num 4) (name Right) (type input))
        (pin (num 5) (name Com) (type input))
        (pin (num 6) (name Up) (type input)))))
  (libraries
    (library (logical Module)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/Module.lib))
    (library (logical ST)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/ST.lib))
    (library (logical TI)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/TI.lib))
    (library (logical afficheur)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/afficheur.lib))
    (library (logical conn)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/conn.lib))
    (library (logical global)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/global.lib)))
  (nets
    (net (code 1) (name "Net-(C12-Pad2)")
      (node (ref C12) (pin 2))
      (node (ref U9) (pin 4)))
    (net (code 2) (name /PH)
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref U6) (pin 7)))
    (net (code 3) (name "Net-(R3-Pad1)")
      (node (ref R3) (pin 1))
      (node (ref U6) (pin 6))
      (node (ref R8) (pin 2)))
    (net (code 4) (name "Net-(R4-Pad2)")
      (node (ref U6) (pin 5))
      (node (ref R5) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 5) (name /5V)
      (node (ref P2) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref D9) (pin 1))
      (node (ref P4) (pin 1))
      (node (ref SJ6) (pin 2))
      (node (ref P3) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref SJ4) (pin 2))
      (node (ref R28) (pin 1))
      (node (ref R23) (pin 1))
      (node (ref R22) (pin 1))
      (node (ref R36) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref P9) (pin 1))
      (node (ref SJ10) (pin 2))
      (node (ref P5) (pin 1))
      (node (ref SJ8) (pin 2))
      (node (ref SJ12) (pin 2))
      (node (ref SJ2) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref U9) (pin 8))
      (node (ref U6) (pin 8))
      (node (ref VR1) (pin 3))
      (node (ref R9) (pin 1)))
    (net (code 6) (name "Net-(R10-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 7) (name /GND)
      (node (ref SJ11) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref U9) (pin 6))
      (node (ref P9) (pin 3))
      (node (ref SW3) (pin 5))
      (node (ref C1) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref J1) (pin 5))
      (node (ref P6) (pin 3))
      (node (ref P10) (pin 3))
      (node (ref C9) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref P11) (pin 2))
      (node (ref U9) (pin 1))
      (node (ref U9) (pin 3))
      (node (ref P4) (pin 3))
      (node (ref SJ9) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref P5) (pin 3))
      (node (ref R41) (pin 2))
      (node (ref P13) (pin 1))
      (node (ref P23) (pin 1))
      (node (ref P14) (pin 1))
      (node (ref C23) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref U1) (pin 48))
      (node (ref R47) (pin 2))
      (node (ref R45) (pin 2))
      (node (ref R43) (pin 2))
      (node (ref R49) (pin 2))
      (node (ref R50) (pin 2))
      (node (ref R51) (pin 1))
      (node (ref R53) (pin 2))
      (node (ref R52) (pin 1))
      (node (ref P25) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref Q4) (pin 3))
      (node (ref U1) (pin 63))
      (node (ref R39) (pin 2))
      (node (ref P24) (pin 1))
      (node (ref U1) (pin 18))
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 31))
      (node (ref C22) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref C20) (pin 2))
      (node (ref P8) (pin 6))
      (node (ref P8) (pin 4))
      (node (ref U8) (pin 15))
      (node (ref U8) (pin 16))
      (node (ref P18) (pin 1))
      (node (ref C19) (pin 2))
      (node (ref P2) (pin 3))
      (node (ref C18) (pin 2))
      (node (ref SJ5) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref VR1) (pin 1))
      (node (ref U2) (pin 16))
      (node (ref P17) (pin 3))
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref U4) (pin 16))
      (node (ref U2) (pin 9))
      (node (ref P12) (pin 1))
      (node (ref SJ1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref SJ3) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref P15) (pin 3))
      (node (ref U3) (pin 4))
      (node (ref C21) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref SJ13) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref SJ7) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref U2) (pin 17))
      (node (ref R27) (pin 2))
      (node (ref P3) (pin 3))
      (node (ref C13) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref P7) (pin 6))
      (node (ref P7) (pin 4)))
    (net (code 8) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref U6) (pin 1)))
    (net (code 9) (name "Net-(U9-Pad7)")
      (node (ref U9) (pin 7)))
    (net (code 10) (name /-5V)
      (node (ref U6) (pin 4))
      (node (ref C21) (pin 1))
      (node (ref U9) (pin 5)))
    (net (code 11) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref U9) (pin 2)))
    (net (code 12) (name "Net-(R1-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref U6) (pin 2)))
    (net (code 13) (name "Net-(P11-Pad1)")
      (node (ref U6) (pin 3))
      (node (ref P11) (pin 1)))
    (net (code 14) (name "Net-(R31-Pad1)")
      (node (ref R31) (pin 1))
      (node (ref U8) (pin 3)))
    (net (code 15) (name "Net-(U8-Pad4)")
      (node (ref U8) (pin 4)))
    (net (code 16) (name "Net-(U8-Pad5)")
      (node (ref U8) (pin 5)))
    (net (code 17) (name "Net-(U8-Pad6)")
      (node (ref U8) (pin 6)))
    (net (code 18) (name "Net-(U8-Pad7)")
      (node (ref U8) (pin 7)))
    (net (code 19) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 20) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 21) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 22) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 23) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 24) (name "Net-(U2-Pad5)")
      (node (ref U2) (pin 5)))
    (net (code 25) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 26) (name "Net-(BT1-Pad1)")
      (node (ref U2) (pin 8))
      (node (ref BT1) (pin 1)))
    (net (code 27) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 28) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 29) (name /12V)
      (node (ref Q1) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref P13) (pin 2))
      (node (ref P23) (pin 2))
      (node (ref P24) (pin 2))
      (node (ref P25) (pin 2))
      (node (ref P16) (pin 2))
      (node (ref P12) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref U7) (pin 3))
      (node (ref P14) (pin 2))
      (node (ref C14) (pin 1)))
    (net (code 30) (name "Net-(P12-Pad3)")
      (node (ref P12) (pin 3)))
    (net (code 31) (name "Net-(P16-Pad1)")
      (node (ref Q1) (pin 2))
      (node (ref P16) (pin 1)))
    (net (code 32) (name "Net-(R30-Pad1)")
      (node (ref U8) (pin 1))
      (node (ref R30) (pin 1)))
    (net (code 33) (name "Net-(U8-Pad11)")
      (node (ref U8) (pin 11)))
    (net (code 34) (name "Net-(U8-Pad12)")
      (node (ref U8) (pin 12)))
    (net (code 35) (name "Net-(U8-Pad19)")
      (node (ref U8) (pin 19)))
    (net (code 36) (name "Net-(U8-Pad2)")
      (node (ref U8) (pin 2)))
    (net (code 37) (name "Net-(U8-Pad20)")
      (node (ref U8) (pin 20)))
    (net (code 38) (name "Net-(P1-Pad4)")
      (node (ref SJ3) (pin 1))
      (node (ref P1) (pin 4))
      (node (ref SJ2) (pin 1)))
    (net (code 39) (name "Net-(P2-Pad4)")
      (node (ref SJ4) (pin 1))
      (node (ref SJ5) (pin 1))
      (node (ref P2) (pin 4)))
    (net (code 40) (name "Net-(P3-Pad4)")
      (node (ref SJ6) (pin 1))
      (node (ref SJ7) (pin 1))
      (node (ref P3) (pin 4)))
    (net (code 41) (name "Net-(U1-Pad54)")
      (node (ref U1) (pin 54)))
    (net (code 42) (name /3.3V)
      (node (ref U2) (pin 15))
      (node (ref C6) (pin 2))
      (node (ref P8) (pin 1))
      (node (ref P8) (pin 2))
      (node (ref P10) (pin 1))
      (node (ref U1) (pin 47))
      (node (ref C18) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref C10) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U1) (pin 64))
      (node (ref C20) (pin 1))
      (node (ref P17) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref R6) (pin 1))
      (node (ref R30) (pin 2))
      (node (ref D10) (pin 1))
      (node (ref U1) (pin 19))
      (node (ref C4) (pin 2))
      (node (ref P7) (pin 1))
      (node (ref R33) (pin 1))
      (node (ref P7) (pin 2))
      (node (ref U1) (pin 13))
      (node (ref C8) (pin 2))
      (node (ref P6) (pin 1))
      (node (ref R29) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref R13) (pin 1))
      (node (ref U1) (pin 32)))
    (net (code 43) (name /SDA)
      (node (ref U3) (pin 8))
      (node (ref R12) (pin 1))
      (node (ref P8) (pin 3))
      (node (ref U2) (pin 10))
      (node (ref P7) (pin 3))
      (node (ref U1) (pin 55)))
    (net (code 44) (name /SCL)
      (node (ref R14) (pin 1))
      (node (ref U3) (pin 7))
      (node (ref U1) (pin 29))
      (node (ref P7) (pin 5))
      (node (ref P8) (pin 5))
      (node (ref U2) (pin 11)))
    (net (code 45) (name "Net-(U1-Pad53)")
      (node (ref U1) (pin 53)))
    (net (code 46) (name "Net-(U1-Pad52)")
      (node (ref U1) (pin 52)))
    (net (code 47) (name "Net-(U1-Pad51)")
      (node (ref U1) (pin 51)))
    (net (code 48) (name /TechniqueBas5V)
      (node (ref P1) (pin 2))
      (node (ref R38) (pin 1)))
    (net (code 49) (name "Net-(U1-Pad41)")
      (node (ref U1) (pin 41)))
    (net (code 50) (name "Net-(P9-Pad4)")
      (node (ref SJ12) (pin 1))
      (node (ref SJ13) (pin 1))
      (node (ref P9) (pin 4)))
    (net (code 51) (name "Net-(P4-Pad4)")
      (node (ref P4) (pin 4))
      (node (ref SJ8) (pin 1))
      (node (ref SJ9) (pin 1)))
    (net (code 52) (name /CapteurAutres25V)
      (node (ref R46) (pin 1))
      (node (ref P5) (pin 2)))
    (net (code 53) (name /VentiloPWM5V_1)
      (node (ref P13) (pin 4))
      (node (ref C22) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref P12) (pin 4)))
    (net (code 54) (name "Net-(P5-Pad4)")
      (node (ref SJ11) (pin 1))
      (node (ref P5) (pin 4))
      (node (ref SJ10) (pin 1)))
    (net (code 55) (name /ReserveBas)
      (node (ref R45) (pin 1))
      (node (ref R44) (pin 2))
      (node (ref U1) (pin 9)))
    (net (code 56) (name /I2C2_SDL)
      (node (ref P15) (pin 1))
      (node (ref U1) (pin 58)))
    (net (code 57) (name /I2C2_SDA)
      (node (ref P15) (pin 2))
      (node (ref U1) (pin 59)))
    (net (code 58) (name /TechniqueBas)
      (node (ref R38) (pin 2))
      (node (ref R39) (pin 1))
      (node (ref U1) (pin 61)))
    (net (code 59) (name /TechniqueHaut)
      (node (ref R41) (pin 1))
      (node (ref U1) (pin 62))
      (node (ref R40) (pin 2)))
    (net (code 60) (name /CuveHaut)
      (node (ref U1) (pin 8))
      (node (ref R43) (pin 1))
      (node (ref R42) (pin 2)))
    (net (code 61) (name "Net-(P25-Pad3)")
      (node (ref P25) (pin 3)))
    (net (code 62) (name "Net-(P24-Pad3)")
      (node (ref P24) (pin 3)))
    (net (code 63) (name "Net-(P23-Pad3)")
      (node (ref P23) (pin 3)))
    (net (code 64) (name "Net-(P14-Pad3)")
      (node (ref P14) (pin 3)))
    (net (code 65) (name "Net-(P13-Pad3)")
      (node (ref P13) (pin 3)))
    (net (code 66) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3))
      (node (ref VR1) (pin 2)))
    (net (code 67) (name "Net-(C7-Pad1)")
      (node (ref U1) (pin 30))
      (node (ref C7) (pin 1)))
    (net (code 68) (name /Left)
      (node (ref U1) (pin 33))
      (node (ref R18) (pin 2))
      (node (ref SW3) (pin 1)))
    (net (code 69) (name /MFP)
      (node (ref U1) (pin 38))
      (node (ref U2) (pin 12))
      (node (ref R15) (pin 1)))
    (net (code 70) (name /USB_OTG_FS_ID)
      (node (ref J1) (pin 4))
      (node (ref U1) (pin 43)))
    (net (code 71) (name /USB_OTG_FS_P)
      (node (ref U1) (pin 45))
      (node (ref J1) (pin 3)))
    (net (code 72) (name /SWDIO)
      (node (ref U1) (pin 46))
      (node (ref P17) (pin 4)))
    (net (code 73) (name /SWCLK)
      (node (ref P17) (pin 2))
      (node (ref U1) (pin 49)))
    (net (code 74) (name /CapteurAutres15V)
      (node (ref P9) (pin 2))
      (node (ref R48) (pin 1)))
    (net (code 75) (name "Net-(R52-Pad2)")
      (node (ref U4) (pin 10))
      (node (ref R52) (pin 2)))
    (net (code 76) (name "Net-(R53-Pad1)")
      (node (ref R53) (pin 1))
      (node (ref U4) (pin 9)))
    (net (code 77) (name "Net-(R51-Pad2)")
      (node (ref U4) (pin 8))
      (node (ref R51) (pin 2)))
    (net (code 78) (name "Net-(R50-Pad1)")
      (node (ref R50) (pin 1))
      (node (ref U4) (pin 7)))
    (net (code 79) (name /TechniqueHaut5V)
      (node (ref P2) (pin 2))
      (node (ref R40) (pin 1)))
    (net (code 80) (name /CuveHaut5V)
      (node (ref P3) (pin 2))
      (node (ref R42) (pin 1)))
    (net (code 81) (name /ReserveBas5V)
      (node (ref P4) (pin 2))
      (node (ref R44) (pin 1)))
    (net (code 82) (name "Net-(Q3-Pad2)")
      (node (ref Q3) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 83) (name "Net-(Q3-Pad1)")
      (node (ref Q3) (pin 1))
      (node (ref R34) (pin 2))
      (node (ref R23) (pin 2)))
    (net (code 84) (name /VentiloPWM_2)
      (node (ref U1) (pin 56))
      (node (ref R21) (pin 2)))
    (net (code 85) (name /VentiloPWM5V_2)
      (node (ref P14) (pin 4))
      (node (ref R34) (pin 1))
      (node (ref P23) (pin 4))
      (node (ref C23) (pin 1)))
    (net (code 86) (name "Net-(Q2-Pad2)")
      (node (ref R11) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 87) (name "Net-(Q2-Pad1)")
      (node (ref R25) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref Q2) (pin 1)))
    (net (code 88) (name /VentiloPWM_1)
      (node (ref R11) (pin 2))
      (node (ref U1) (pin 57)))
    (net (code 89) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 90) (name /VentiloPWM_3)
      (node (ref R35) (pin 2))
      (node (ref U1) (pin 50)))
    (net (code 91) (name "Net-(Q4-Pad1)")
      (node (ref R37) (pin 2))
      (node (ref R36) (pin 2))
      (node (ref Q4) (pin 1)))
    (net (code 92) (name /VentiloPWM5V_3)
      (node (ref P25) (pin 4))
      (node (ref C24) (pin 1))
      (node (ref R37) (pin 1))
      (node (ref P24) (pin 4)))
    (net (code 93) (name "Net-(Q4-Pad2)")
      (node (ref R35) (pin 1))
      (node (ref Q4) (pin 2)))
    (net (code 94) (name /CapteurAutres2)
      (node (ref U1) (pin 10))
      (node (ref R47) (pin 1))
      (node (ref R46) (pin 2)))
    (net (code 95) (name /CapteurAutres1)
      (node (ref R49) (pin 1))
      (node (ref U1) (pin 11))
      (node (ref R48) (pin 2)))
    (net (code 96) (name /TempAir)
      (node (ref P10) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 97) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 98) (name /CS_ESP)
      (node (ref U1) (pin 20))
      (node (ref U8) (pin 9)))
    (net (code 99) (name /CLK)
      (node (ref U1) (pin 21))
      (node (ref U8) (pin 14)))
    (net (code 100) (name /MOSI)
      (node (ref U1) (pin 22))
      (node (ref U8) (pin 13)))
    (net (code 101) (name /MISO)
      (node (ref U1) (pin 23))
      (node (ref U8) (pin 10)))
    (net (code 102) (name "Net-(R24-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref U4) (pin 15)))
    (net (code 103) (name /boot0)
      (node (ref U1) (pin 60))
      (node (ref SW1) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 104) (name /Right)
      (node (ref R16) (pin 2))
      (node (ref SW3) (pin 4))
      (node (ref U1) (pin 36)))
    (net (code 105) (name /UP)
      (node (ref R17) (pin 2))
      (node (ref U1) (pin 37))
      (node (ref SW3) (pin 6)))
    (net (code 106) (name /Down)
      (node (ref R19) (pin 2))
      (node (ref SW3) (pin 3))
      (node (ref U1) (pin 35)))
    (net (code 107) (name /Select)
      (node (ref U1) (pin 34))
      (node (ref SW3) (pin 2))
      (node (ref R20) (pin 2)))
    (net (code 108) (name /RS)
      (node (ref U4) (pin 4))
      (node (ref U1) (pin 39)))
    (net (code 109) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 110) (name "Net-(C2-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref Y1) (pin 2))
      (node (ref C2) (pin 1)))
    (net (code 111) (name /TempEau)
      (node (ref U1) (pin 14))
      (node (ref P6) (pin 2)))
    (net (code 112) (name "Net-(J1-Pad0)")
      (node (ref J1) (pin 0)))
    (net (code 113) (name /USB_OTG_FS_VBUS)
      (node (ref U1) (pin 42))
      (node (ref J1) (pin 1)))
    (net (code 114) (name /USB_OTG_FS_N)
      (node (ref U1) (pin 44))
      (node (ref J1) (pin 2)))
    (net (code 115) (name /nrst)
      (node (ref P17) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref R13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref SW2) (pin 1)))
    (net (code 116) (name /wc)
      (node (ref U1) (pin 4))
      (node (ref R6) (pin 2))
      (node (ref U3) (pin 6)))
    (net (code 117) (name /R/W)
      (node (ref U1) (pin 40))
      (node (ref U4) (pin 5)))
    (net (code 118) (name "Net-(C15-Pad1)")
      (node (ref R26) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref D9) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref C15) (pin 1)))
    (net (code 119) (name "Net-(P20-Pad1)")
      (node (ref P20) (pin 1)))
    (net (code 120) (name /RX)
      (node (ref P18) (pin 2))
      (node (ref U8) (pin 21)))
    (net (code 121) (name /TX)
      (node (ref P18) (pin 3))
      (node (ref U8) (pin 22)))
    (net (code 122) (name "Net-(P19-Pad1)")
      (node (ref P19) (pin 1)))
    (net (code 123) (name "Net-(P21-Pad1)")
      (node (ref P21) (pin 1)))
    (net (code 124) (name "Net-(P22-Pad1)")
      (node (ref P22) (pin 1)))
    (net (code 125) (name "Net-(R32-Pad2)")
      (node (ref U8) (pin 17))
      (node (ref R32) (pin 2)))
    (net (code 126) (name /mode)
      (node (ref U8) (pin 18))
      (node (ref R33) (pin 2))
      (node (ref SJ1) (pin 1)))
    (net (code 127) (name /E)
      (node (ref U4) (pin 6))
      (node (ref U1) (pin 28)))
    (net (code 128) (name /D4)
      (node (ref U4) (pin 11))
      (node (ref U1) (pin 27)))
    (net (code 129) (name /D5)
      (node (ref U4) (pin 12))
      (node (ref U1) (pin 26)))
    (net (code 130) (name /D6)
      (node (ref U1) (pin 25))
      (node (ref U4) (pin 13)))
    (net (code 131) (name /D7)
      (node (ref U1) (pin 24))
      (node (ref U4) (pin 14)))
    (net (code 133) (name "Net-(C16-Pad1)")
      (node (ref U7) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref R29) (pin 2))
      (node (ref R27) (pin 1))
      (node (ref D10) (pin 2)))))