{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Ordinateur","Amperage Relais"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ordinateur","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,0,0,4],[8,0,8,4]]}
["Ordinateur"]
["Numero",1,2,3,4]
["P1","Niveau1","Niveau2","5V","GND"]
["P2","Niveau3","Niveau4","5V","GND"]
["P3","Niveau5","Niveau6","5V","GND"]
["P4","TMP1","TMP2","3V3","GND"]
["P5"]
["P6"]
["Fille",{"$nulls":5},"Apres ces de l'optimisation et du "]
["Numero",1,2,3,4]
["P1","12VIN","12VIN","GND","GND"]
["P2","230V","230V"]
["P3","Out0","Out1","Out2","Out3"]
["P4","Out4","Out5","Out6","Out7"]
["P5","Vent1","Vent2","GND","12V"]
["P6"]
[{"$nulls":6},"m"]

{"sheet":"Amperage Relais","index":1,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,2],[7,0,7,2]]}
[230]
["Nom","Watt","Ampere"]
["Max",300]
[]
[]
[]
[]
["12V"]