{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["résolution PT1000 sans AOP","Degree pt1000"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"résolution PT1000 sans AOP","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,0,0,2],[5,0,5,3],[14,0,14,3]]}
[]
["tension de ref","nb bit","résolution volt","tension alim pt1000","résistance série PT1000 ",null,"mini résitance serie","maxi résitance série"]
[3.3,12,{"$f":"A3/POWER(2,B3)","v":8.0566406249999996E-4},3.3,43000,null,{"$f":"(D3/0.0001)-1000","v":32000},{"$f":"(D3/0.00001)-1000","v":328999.99999999994}]
[]
[]
[]
[null,null,null,"résolution max",null,null,"auto echauffement","K*R*I2"]
[{"$f":"D20+C3","v":8.2921575921049151E-2},{"$f":"A8*(E3/(D3-D20))","v":1108.0659423828124},{"$f":"B8-1097.3","v":10.765942382812455},{"$f":"1/(3.9/C8)","v":2.7604980468749885}]
{"$rows_empty":7}
["résolution voulue","résolution ohmique (PT1000)"]
[0.01,{"$f":"3.9*A17","v":3.9E-2}]
[]
[null,null,null,"mV"]
[null,null,1097.3,{"$f":"(D3*C20)/(E3+C20)","v":8.2115911858549148E-2}]
[null,null,{"$f":"C20+B17","v":1097.3389999999999},{"$f":"(D3*C21)/(E3+C21)","v":8.2118757778105372E-2}]
[null,null,"diff",{"$f":"D21-D20","v":2.8459195562241524E-6}]
[null,null,"doit etre sup a 1",{"$f":"D22/C3","v":3.5323898491800391E-3}]

{"sheet":"Degree pt1000","index":1,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Température (°C)","résistance","tension diviseur","Sortie AOP"]
[0,{"$f":"(A2*1000*0.00385)+1000","v":1000},{"$f":"(3.3*B2)/(16200+B2)","v":0.19186046511627908},{"$f":"C2*(43/4.7)","v":1.7553191489361701}]
[10,{"$f":"(A3*1000*0.00385)+1000","v":1038.5},{"$f":"(3.3*B3)/(16200+B3)","v":0.19880209995069176},{"$f":"C3*(43/4.7)","v":1.8188277229531373}]
[20,{"$f":"(A4*1000*0.00385)+1000","v":1077},0.2057127973606529,{"$f":"C4*(43/4.7)","v":1.8820532524485265}]
[21,1080.8499999999999,0.20640217350419682,1.8883603107830771]
[23,1088.55,0.20778000468518179,1.9009660003112376]
[24,1092.4000000000001,0.20846846013277509,1.9072646352573039]
[24.5,1094.325,0.20881257291047786,1.9104129010958613,{"$f":"D9-D8","v":6.2956906691891135E-4},null,"62,5µV"]
[24.6,1094.71,0.20888138627360622,1.9110424701627802]
[24.7,1095.095,0.20895019657307459,1.9116720112004697]
[24.8,1095.48,0.20901900380908769,1.9123015242108024]
[24.9,1095.865,0.20908780798184998,1.9129310091956486]
[25,1096.25,0.20915660909156608,1.913560466156881]
[25.1,1096.635,0.20922540713844051,1.9141898950963705]
[25.2,1097.02,0.20929420212267777,1.914819296015988]
[25.3,1097.405,0.20936299404448239,1.9154486689176047]
[25.4,1097.79,0.20943178290405881,1.9160780138030913]
[25.5,1098.175,0.20950056870161157,1.9167073306743185]
[26,1100.0999999999999,0.20984445176617475,1.9198534948820243]
[27,1103.95,0.21053198836103892,1.926143723303122]
[28,1107.8,0.21121921908041461,1.9324311532888996]
[29,1111.6500000000001,0.21190614412837597,1.9387157867064184]
[30,1115.5,0.21259276370881577,1.9449976254210803]
[40,1154,0.21944220352656446,2.0076627131153768]
[50,1192.5,0.22626131953428202,2.070050370207261]
[100,1385,0.25990901336366223,2.3778909733271223]
[150,1577.5,0.29282801293770216,2.6790647992172749]
[200,1770,0.32504173622704507,2.9737860973963697]
[250,1962.5,0.35657260839642119,3.2622600342651298]