(export (version D)
  (design
    (source C:\Users\e_rcluze\Documents\Autres\projet\Peristatique\EDA\Peristatique.sch)
    (date "17/02/2020 17:06:48")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Peristatique.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R16)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455AD4))
    (comp (ref R17)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455ADC))
    (comp (ref C14)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 0605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455AF2))
    (comp (ref R23)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455AFC))
    (comp (ref R24)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455B06))
    (comp (ref SJ1)
      (value Mode)
      (footprint Jumper:Jumper_2.54mm)
      (fields
        (field (name Partkeepr) 0100))
      (libsource (lib global) (part Jumper) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455B13))
    (comp (ref C13)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 0607))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455B27))
    (comp (ref P6)
      (value ProgESP)
      (footprint Connector:PinHeader2.54_1X3)
      (fields
        (field (name Partkeepr) 0100))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455B31))
    (comp (ref U8)
      (value ESP-12F)
      (footprint Module:ESP-12F)
      (fields
        (field (name Partkeepr) 2800))
      (libsource (lib Module) (part ESP-12F) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E455B39))
    (comp (ref R21)
      (value 510)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 913))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456BC2))
    (comp (ref R22)
      (value 330)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 914))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456BCA))
    (comp (ref C16)
      (value 10µF)
      (footprint C:CP_CMS5X5.8)
      (fields
        (field (name Partkeepr) 609))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456BD2))
    (comp (ref C15)
      (value 100nF)
      (footprint C:3216-18)
      (fields
        (field (name Partkeepr) 0610))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456BDC))
    (comp (ref U9)
      (value LM317)
      (footprint U:LM317)
      (fields
        (field (name Partkeepr) 1800))
      (libsource (lib global) (part LM317) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456BE4))
    (comp (ref C18)
      (value 1µF)
      (footprint C:CP_CMS4X5.8)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C02))
    (comp (ref D2)
      (value D)
      (footprint D:SMA)
      (fields
        (field (name Partkeepr) 1302))
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C11))
    (comp (ref R12)
      (value 1K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0915))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C1D))
    (comp (ref R15)
      (value 330)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 914))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C25))
    (comp (ref C11)
      (value 10µF)
      (footprint C:CP_CMS5X5.8)
      (fields
        (field (name Partkeepr) 609))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C2D))
    (comp (ref C10)
      (value 100nF)
      (footprint C:3216-18)
      (fields
        (field (name Partkeepr) 0610))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C37))
    (comp (ref U6)
      (value LM317)
      (footprint U:LM317)
      (fields
        (field (name Partkeepr) 1800))
      (libsource (lib global) (part LM317) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C3F))
    (comp (ref C12)
      (value 1µF)
      (footprint C:CP_CMS4X5.8)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib global) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C5D))
    (comp (ref D1)
      (value D)
      (footprint D:SMA)
      (fields
        (field (name Partkeepr) 1302))
      (libsource (lib global) (part D) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E456C6C))
    (comp (ref R5)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4580FC))
    (comp (ref R4)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E458104))
    (comp (ref R3)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45810C))
    (comp (ref BT1)
      (value Battery)
      (footprint Connector:batterie)
      (fields
        (field (name Partkeepr) 3))
      (libsource (lib global) (part Battery) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E458123))
    (comp (ref U4)
      (value M41T83)
      (footprint U:SOX18)
      (fields
        (field (name Partkeepr) 1600))
      (libsource (lib ST) (part M41T83) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45812C))
    (comp (ref SW1)
      (value boot)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib global) (part SW_PUSH) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A99A))
    (comp (ref R2)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9A2))
    (comp (ref C1)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9AB))
    (comp (ref R1)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9B6))
    (comp (ref C9)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9C0))
    (comp (ref SW2)
      (value reset)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib global) (part SW_PUSH) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9D2))
    (comp (ref C6)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9E9))
    (comp (ref C7)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9F1))
    (comp (ref C5)
      (value 10nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45A9FB))
    (comp (ref C4)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45AA05))
    (comp (ref P1)
      (value CONN_01X05)
      (footprint Connector:PinHeader2.54_1X5)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45AA10))
    (comp (ref U2)
      (value STM32F030C8)
      (footprint U:LQFP48)
      (fields
        (field (name Partkeepr) 2100))
      (libsource (lib ST) (part STM32F030C8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45AA1D))
    (comp (ref C3)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E45AA25))
    (comp (ref R20)
      (value 100)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 912))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476162))
    (comp (ref U7)
      (value HD44780)
      (footprint Connector:PinHeader2.54_1X16)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib afficheur) (part HD44780) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E47616C))
    (comp (ref VR1)
      (value 10K)
      (footprint R:3296)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part Poten) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476175))
    (comp (ref R18)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476181))
    (comp (ref R19)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476189))
    (comp (ref R14)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476191))
    (comp (ref R13)
      (value 100K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 0916))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E476199))
    (comp (ref U10)
      (value 74HC541)
      (footprint U:SO20)
      (fields
        (field (name Partkeepr) 1502))
      (libsource (lib NXP) (part 74HC541) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4761A5))
    (comp (ref C17)
      (value 0.1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 0605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4761BF))
    (comp (ref R11)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4DC14F))
    (comp (ref U5)
      (value M24C32)
      (footprint U:SO8N)
      (fields
        (field (name Partkeepr) 1700))
      (libsource (lib ST) (part M24C32) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4DC158))
    (comp (ref SW3)
      (value mt-OO8a)
      (footprint SW:MT-008a)
      (fields
        (field (name Partkeepr) 201))
      (libsource (lib global) (part mt-OO8a) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D01))
    (comp (ref R6)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D15))
    (comp (ref R7)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D1D))
    (comp (ref R8)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D25))
    (comp (ref R9)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D2D))
    (comp (ref R10)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4E5D35))
    (comp (ref U1)
      (value ULN2803A)
      (footprint U:SOIC18)
      (fields
        (field (name Partkeepr) 2500))
      (libsource (lib TI) (part ULN2803A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E51BC58))
    (comp (ref U3)
      (value ULN2803A)
      (footprint U:SOIC18)
      (fields
        (field (name Partkeepr) 2500))
      (libsource (lib TI) (part ULN2803A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E51BF23))
    (comp (ref P2)
      (value M1)
      (footprint Connector:PinHeader2.54_1X5)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E54B070))
    (comp (ref P3)
      (value M2)
      (footprint Connector:PinHeader2.54_1X5)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E54B12E))
    (comp (ref P4)
      (value M3)
      (footprint Connector:PinHeader2.54_1X5)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E54B5EF))
    (comp (ref P5)
      (value M4)
      (footprint Connector:PinHeader2.54_1X5)
      (libsource (lib conn) (part CONN_01X05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E54B5F6))
    (comp (ref C2)
      (value 10nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5C2F19))
    (comp (ref C8)
      (value 10nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib global) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5C326C))
    (comp (ref P7)
      (value CONN_01X02)
      (footprint "Connector:DC jack")
      (fields
        (field (name Partkeepr) 0152))
      (libsource (lib conn) (part CONN_01X02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E68794E))
    (comp (ref P8)
      (value MH)
      (footprint MH:MH3mm)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4B09A9))
    (comp (ref P11)
      (value MH)
      (footprint MH:MH3mm)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4B9DFF))
    (comp (ref P10)
      (value MH)
      (footprint MH:MH3mm)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4BE538))
    (comp (ref P9)
      (value MH)
      (footprint MH:MH3mm)
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4BE540)))
  (libparts
    (libpart (lib Module) (part ESP-12F)
      (fields
        (field (name Reference) U)
        (field (name Value) ESP-12F))
      (pins
        (pin (num 1) (name RST) (type input))
        (pin (num 2) (name ADC) (type input))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name GPIO16) (type input))
        (pin (num 5) (name GPIO14) (type input))
        (pin (num 6) (name GPIO12) (type input))
        (pin (num 7) (name GPIO13) (type input))
        (pin (num 8) (name VCC) (type input))
        (pin (num 9) (name CS0) (type input))
        (pin (num 10) (name MISO) (type input))
        (pin (num 11) (name GPIO9) (type input))
        (pin (num 12) (name GPIO10) (type input))
        (pin (num 13) (name MOSI) (type input))
        (pin (num 14) (name SCLK) (type input))
        (pin (num 15) (name GND) (type input))
        (pin (num 16) (name GPIO15) (type input))
        (pin (num 17) (name GPIO2) (type input))
        (pin (num 18) (name GPIO0) (type input))
        (pin (num 19) (name GPIO4) (type input))
        (pin (num 20) (name GPIO5) (type input))
        (pin (num 21) (name RXD) (type input))
        (pin (num 22) (name TXD) (type input))))
    (libpart (lib NXP) (part 74HC541)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC541))
      (pins
        (pin (num 1) (name ~OE1) (type input))
        (pin (num 2) (name A0) (type input))
        (pin (num 3) (name A1) (type input))
        (pin (num 4) (name A2) (type input))
        (pin (num 5) (name A3) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A5) (type input))
        (pin (num 8) (name A6) (type input))
        (pin (num 9) (name A7) (type input))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name Y7) (type output))
        (pin (num 12) (name Y6) (type output))
        (pin (num 13) (name Y5) (type output))
        (pin (num 14) (name Y4) (type output))
        (pin (num 15) (name Y3) (type output))
        (pin (num 16) (name Y2) (type output))
        (pin (num 17) (name Y1) (type output))
        (pin (num 18) (name Y0) (type output))
        (pin (num 19) (name ~OE2) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib ST) (part M24C32)
      (fields
        (field (name Reference) U)
        (field (name Value) M24C32))
      (pins
        (pin (num 1) (name E0) (type input))
        (pin (num 2) (name E1) (type input))
        (pin (num 3) (name E2) (type input))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name ~WC) (type input))
        (pin (num 7) (name SCL) (type input))
        (pin (num 8) (name SDA) (type BiDi))))
    (libpart (lib ST) (part M41T83)
      (fields
        (field (name Reference) U)
        (field (name Value) M41T83))
      (pins
        (pin (num 1) (name NC) (type input))
        (pin (num 2) (name NF) (type input))
        (pin (num 3) (name NF) (type input))
        (pin (num 4) (name NC) (type input))
        (pin (num 5) (name ~RST) (type input))
        (pin (num 6) (name DU) (type input))
        (pin (num 7) (name SQW) (type input))
        (pin (num 8) (name VBAT) (type input))
        (pin (num 9) (name VSS) (type input))
        (pin (num 10) (name SDA) (type input))
        (pin (num 11) (name SCL) (type input))
        (pin (num 12) (name ~IRQ1~/FT/OUT) (type input))
        (pin (num 13) (name NC) (type input))
        (pin (num 14) (name ~IRQ2) (type input))
        (pin (num 15) (name VCC) (type input))
        (pin (num 16) (name NF) (type input))
        (pin (num 17) (name NF) (type input))
        (pin (num 18) (name NC) (type input))))
    (libpart (lib ST) (part STM32F030C8)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030C8))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14/OSC32_IN) (type BiDi))
        (pin (num 4) (name PC15/OSC32_OUT) (type BiDi))
        (pin (num 5) (name PF0/OSC_IN) (type BiDi))
        (pin (num 6) (name PF1/OSC_OUT) (type BiDi))
        (pin (num 7) (name ~NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name PB11) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name PF6) (type BiDi))
        (pin (num 36) (name PF7) (type BiDi))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib TI) (part ULN2803A)
      (fields
        (field (name Reference) U)
        (field (name Value) ULN2803A))
      (pins
        (pin (num 1) (name 1B) (type input))
        (pin (num 2) (name 2B) (type input))
        (pin (num 3) (name 3B) (type input))
        (pin (num 4) (name 4B) (type input))
        (pin (num 5) (name 5B) (type input))
        (pin (num 6) (name 6B) (type input))
        (pin (num 7) (name 7B) (type input))
        (pin (num 8) (name 8B) (type input))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name COM) (type power_in))
        (pin (num 11) (name 8C) (type output))
        (pin (num 12) (name 7C) (type output))
        (pin (num 13) (name 6C) (type output))
        (pin (num 14) (name 5C) (type output))
        (pin (num 15) (name 4C) (type output))
        (pin (num 16) (name 3C) (type output))
        (pin (num 17) (name 2C) (type output))
        (pin (num 18) (name 1C) (type output))))
    (libpart (lib afficheur) (part HD44780)
      (fields
        (field (name Reference) U)
        (field (name Value) HD44780))
      (pins
        (pin (num 1) (name VSS) (type input))
        (pin (num 2) (name VDD) (type input))
        (pin (num 3) (name Vee) (type input))
        (pin (num 4) (name RS) (type input))
        (pin (num 5) (name R/W) (type input))
        (pin (num 6) (name E) (type input))
        (pin (num 7) (name D0) (type input))
        (pin (num 8) (name D1) (type input))
        (pin (num 9) (name D2) (type input))
        (pin (num 10) (name D3) (type input))
        (pin (num 11) (name D4) (type input))
        (pin (num 12) (name D5) (type input))
        (pin (num 13) (name D6) (type input))
        (pin (num 14) (name D7) (type input))
        (pin (num 15) (name A) (type input))
        (pin (num 16) (name K) (type input))))
    (libpart (lib conn) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib global) (part Battery)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part C)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part CP)
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part D)
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib global) (part Jumper)
      (fields
        (field (name Reference) SJ)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part LM317)
      (fields
        (field (name Reference) U)
        (field (name Value) LM317))
      (pins
        (pin (num 1) (name Adj) (type input))
        (pin (num 2) (name Vout) (type power_out))
        (pin (num 3) (name Vin) (type power_in))))
    (libpart (lib global) (part Poten)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) VR)
        (field (name Value) Poten))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part SW_PUSH)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib global) (part mt-OO8a)
      (fields
        (field (name Reference) SW)
        (field (name Value) mt-OO8a))
      (pins
        (pin (num 1) (name Left) (type input))
        (pin (num 2) (name Select) (type input))
        (pin (num 3) (name Down) (type input))
        (pin (num 4) (name Right) (type input))
        (pin (num 5) (name Com) (type input))
        (pin (num 6) (name Up) (type input)))))
  (libraries
    (library (logical Module)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/Module.lib))
    (library (logical NXP)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/NXP.lib))
    (library (logical ST)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/ST.lib))
    (library (logical TI)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/TI.lib))
    (library (logical afficheur)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/afficheur.lib))
    (library (logical conn)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/conn.lib))
    (library (logical global)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/global.lib)))
  (nets
    (net (code 1) (name "Net-(U10-Pad11)")
      (node (ref U10) (pin 11)))
    (net (code 2) (name "Net-(U10-Pad9)")
      (node (ref U10) (pin 9)))
    (net (code 3) (name /5V)
      (node (ref U10) (pin 20))
      (node (ref U3) (pin 10))
      (node (ref P4) (pin 4))
      (node (ref P3) (pin 4))
      (node (ref P5) (pin 4))
      (node (ref U7) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref P2) (pin 4))
      (node (ref R20) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref U6) (pin 2))
      (node (ref VR1) (pin 3))
      (node (ref R15) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 10))
      (node (ref C17) (pin 1)))
    (net (code 4) (name /R/W)
      (node (ref U10) (pin 3))
      (node (ref U2) (pin 21)))
    (net (code 5) (name /E)
      (node (ref U2) (pin 20))
      (node (ref U10) (pin 4)))
    (net (code 6) (name /D4)
      (node (ref U2) (pin 19))
      (node (ref U10) (pin 5)))
    (net (code 7) (name /D5)
      (node (ref U2) (pin 18))
      (node (ref U10) (pin 6)))
    (net (code 8) (name /D6)
      (node (ref U10) (pin 7))
      (node (ref U2) (pin 12)))
    (net (code 9) (name /D7)
      (node (ref U10) (pin 8))
      (node (ref U2) (pin 11)))
    (net (code 10) (name /3.3V)
      (node (ref R17) (pin 2))
      (node (ref U9) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref SW2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 24))
      (node (ref U4) (pin 15))
      (node (ref U4) (pin 6))
      (node (ref R5) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref P1) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref R23) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref U8) (pin 8))
      (node (ref R22) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref U2) (pin 48))
      (node (ref U2) (pin 9))
      (node (ref C3) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 11) (name /Right)
      (node (ref R6) (pin 2))
      (node (ref U2) (pin 28))
      (node (ref SW3) (pin 4)))
    (net (code 12) (name /UP)
      (node (ref R7) (pin 2))
      (node (ref U2) (pin 29))
      (node (ref SW3) (pin 6)))
    (net (code 13) (name /wc)
      (node (ref U2) (pin 2))
      (node (ref U5) (pin 6))
      (node (ref R11) (pin 2)))
    (net (code 14) (name /sdl)
      (node (ref U5) (pin 7))
      (node (ref U2) (pin 42))
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 11)))
    (net (code 15) (name /sda)
      (node (ref R5) (pin 2))
      (node (ref U4) (pin 10))
      (node (ref U5) (pin 8))
      (node (ref U2) (pin 43)))
    (net (code 16) (name /RS)
      (node (ref U2) (pin 22))
      (node (ref U10) (pin 2)))
    (net (code 17) (name /Left)
      (node (ref SW3) (pin 1))
      (node (ref U2) (pin 27))
      (node (ref R8) (pin 2)))
    (net (code 18) (name /Select)
      (node (ref U2) (pin 26))
      (node (ref R10) (pin 2))
      (node (ref SW3) (pin 2)))
    (net (code 19) (name /Down)
      (node (ref SW3) (pin 3))
      (node (ref U2) (pin 25))
      (node (ref R9) (pin 2)))
    (net (code 20) (name "Net-(R20-Pad2)")
      (node (ref R20) (pin 2))
      (node (ref U7) (pin 15)))
    (net (code 21) (name "Net-(R19-Pad1)")
      (node (ref R19) (pin 1))
      (node (ref U7) (pin 9)))
    (net (code 22) (name "Net-(R14-Pad2)")
      (node (ref R14) (pin 2))
      (node (ref U7) (pin 8)))
    (net (code 23) (name "Net-(R13-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref U7) (pin 7)))
    (net (code 24) (name "Net-(R18-Pad2)")
      (node (ref R18) (pin 2))
      (node (ref U7) (pin 10)))
    (net (code 25) (name /GND)
      (node (ref C7) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U8) (pin 15))
      (node (ref U2) (pin 47))
      (node (ref C3) (pin 2))
      (node (ref U7) (pin 16))
      (node (ref VR1) (pin 1))
      (node (ref U10) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref R12) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U1) (pin 9))
      (node (ref P6) (pin 1))
      (node (ref C16) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref U8) (pin 16))
      (node (ref C13) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref SJ1) (pin 2))
      (node (ref U10) (pin 10))
      (node (ref C8) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref P7) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 9))
      (node (ref BT1) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref U10) (pin 19))
      (node (ref U4) (pin 16))
      (node (ref U4) (pin 17))
      (node (ref U4) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref U2) (pin 23))
      (node (ref C11) (pin 2))
      (node (ref U5) (pin 4))
      (node (ref U5) (pin 3))
      (node (ref U5) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref SW3) (pin 5))
      (node (ref U4) (pin 9)))
    (net (code 26) (name /D7_OUT)
      (node (ref U7) (pin 14))
      (node (ref U10) (pin 12)))
    (net (code 27) (name /D6_OUT)
      (node (ref U7) (pin 13))
      (node (ref U10) (pin 13)))
    (net (code 28) (name /D5_OUT)
      (node (ref U7) (pin 12))
      (node (ref U10) (pin 14)))
    (net (code 29) (name /D4_OUT)
      (node (ref U10) (pin 15))
      (node (ref U7) (pin 11)))
    (net (code 30) (name /E_OUT)
      (node (ref U10) (pin 16))
      (node (ref U7) (pin 6)))
    (net (code 31) (name /R/W_OUT)
      (node (ref U10) (pin 17))
      (node (ref U7) (pin 5)))
    (net (code 32) (name /RS_OUT)
      (node (ref U7) (pin 4))
      (node (ref U10) (pin 18)))
    (net (code 33) (name "Net-(U7-Pad3)")
      (node (ref VR1) (pin 2))
      (node (ref U7) (pin 3)))
    (net (code 34) (name "Net-(P8-Pad1)")
      (node (ref P8) (pin 1)))
    (net (code 35) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 36) (name "Net-(U4-Pad1)")
      (node (ref U4) (pin 1)))
    (net (code 37) (name "Net-(U4-Pad18)")
      (node (ref U4) (pin 18)))
    (net (code 38) (name /12V)
      (node (ref P7) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref U9) (pin 3))
      (node (ref U6) (pin 3))
      (node (ref C10) (pin 1)))
    (net (code 39) (name "Net-(P11-Pad1)")
      (node (ref P11) (pin 1)))
    (net (code 40) (name "Net-(P10-Pad1)")
      (node (ref P10) (pin 1)))
    (net (code 41) (name "Net-(P9-Pad1)")
      (node (ref P9) (pin 1)))
    (net (code 42) (name /M3_IN1)
      (node (ref U3) (pin 5))
      (node (ref U2) (pin 46)))
    (net (code 43) (name /M4_B2)
      (node (ref U3) (pin 15))
      (node (ref P5) (pin 5)))
    (net (code 44) (name /M4_A2)
      (node (ref P5) (pin 3))
      (node (ref U3) (pin 16)))
    (net (code 45) (name /M4_B1)
      (node (ref U3) (pin 17))
      (node (ref P5) (pin 2)))
    (net (code 46) (name /M4_A1)
      (node (ref P5) (pin 1))
      (node (ref U3) (pin 18)))
    (net (code 47) (name /M4_IN2)
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 2)))
    (net (code 48) (name /M4_IN3)
      (node (ref U2) (pin 4))
      (node (ref U3) (pin 3)))
    (net (code 49) (name /M4_IN4)
      (node (ref U2) (pin 3))
      (node (ref U3) (pin 4)))
    (net (code 50) (name /M3_IN2)
      (node (ref U3) (pin 6))
      (node (ref U2) (pin 45)))
    (net (code 51) (name /M3_IN3)
      (node (ref U3) (pin 7))
      (node (ref U2) (pin 41)))
    (net (code 52) (name /M3_IN4)
      (node (ref U3) (pin 8))
      (node (ref U2) (pin 40)))
    (net (code 53) (name /M2_A1)
      (node (ref P3) (pin 1))
      (node (ref U1) (pin 18)))
    (net (code 54) (name /M2_IN1)
      (node (ref U1) (pin 1))
      (node (ref U2) (pin 39)))
    (net (code 55) (name /M1_A2)
      (node (ref P2) (pin 3))
      (node (ref U1) (pin 12)))
    (net (code 56) (name /M1_B1)
      (node (ref P2) (pin 2))
      (node (ref U1) (pin 13)))
    (net (code 57) (name /M1_A1)
      (node (ref P2) (pin 1))
      (node (ref U1) (pin 14)))
    (net (code 58) (name /M2_B2)
      (node (ref P3) (pin 5))
      (node (ref U1) (pin 15)))
    (net (code 59) (name /M2_A2)
      (node (ref P3) (pin 3))
      (node (ref U1) (pin 16)))
    (net (code 60) (name /M2_B1)
      (node (ref U1) (pin 17))
      (node (ref P3) (pin 2)))
    (net (code 61) (name /M2_IN2)
      (node (ref U1) (pin 2))
      (node (ref U2) (pin 38)))
    (net (code 62) (name /M2_IN3)
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 36)))
    (net (code 63) (name /M2_IN4)
      (node (ref U1) (pin 4))
      (node (ref U2) (pin 35)))
    (net (code 64) (name /M1_IN1)
      (node (ref U1) (pin 5))
      (node (ref U2) (pin 33)))
    (net (code 65) (name /M1_IN2)
      (node (ref U1) (pin 6))
      (node (ref U2) (pin 32)))
    (net (code 66) (name /M1_IN3)
      (node (ref U1) (pin 7))
      (node (ref U2) (pin 31)))
    (net (code 67) (name /M1_IN4)
      (node (ref U2) (pin 30))
      (node (ref U1) (pin 8)))
    (net (code 68) (name /M4_IN1)
      (node (ref U2) (pin 6))
      (node (ref U3) (pin 1)))
    (net (code 69) (name /M3_A1)
      (node (ref P4) (pin 1))
      (node (ref U3) (pin 14)))
    (net (code 70) (name /M3_B1)
      (node (ref P4) (pin 2))
      (node (ref U3) (pin 13)))
    (net (code 71) (name /M3_A2)
      (node (ref U3) (pin 12))
      (node (ref P4) (pin 3)))
    (net (code 72) (name /M3_B2)
      (node (ref P4) (pin 5))
      (node (ref U3) (pin 11)))
    (net (code 73) (name /M1_B2)
      (node (ref U1) (pin 11))
      (node (ref P2) (pin 5)))
    (net (code 74) (name "Net-(C16-Pad1)")
      (node (ref U9) (pin 1))
      (node (ref R22) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 75) (name "Net-(R23-Pad2)")
      (node (ref U8) (pin 17))
      (node (ref R23) (pin 2)))
    (net (code 76) (name /mode)
      (node (ref U8) (pin 18))
      (node (ref R24) (pin 2))
      (node (ref SJ1) (pin 1)))
    (net (code 77) (name "Net-(R16-Pad1)")
      (node (ref R16) (pin 1))
      (node (ref U8) (pin 1)))
    (net (code 78) (name "Net-(R17-Pad1)")
      (node (ref U8) (pin 3))
      (node (ref R17) (pin 1)))
    (net (code 79) (name "Net-(U8-Pad4)")
      (node (ref U8) (pin 4)))
    (net (code 80) (name "Net-(U8-Pad5)")
      (node (ref U8) (pin 5)))
    (net (code 81) (name "Net-(U8-Pad6)")
      (node (ref U8) (pin 6)))
    (net (code 82) (name "Net-(U8-Pad7)")
      (node (ref U8) (pin 7)))
    (net (code 83) (name "Net-(U8-Pad11)")
      (node (ref U8) (pin 11)))
    (net (code 84) (name "Net-(U8-Pad12)")
      (node (ref U8) (pin 12)))
    (net (code 85) (name "Net-(U8-Pad20)")
      (node (ref U8) (pin 20)))
    (net (code 86) (name "Net-(U8-Pad19)")
      (node (ref U8) (pin 19)))
    (net (code 87) (name "Net-(U8-Pad2)")
      (node (ref U8) (pin 2)))
    (net (code 88) (name /RX)
      (node (ref P6) (pin 2))
      (node (ref U8) (pin 21)))
    (net (code 89) (name /TX)
      (node (ref P6) (pin 3))
      (node (ref U8) (pin 22)))
    (net (code 90) (name "Net-(C11-Pad1)")
      (node (ref D1) (pin 2))
      (node (ref R12) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref R15) (pin 2)))
    (net (code 91) (name /nrst)
      (node (ref U2) (pin 7))
      (node (ref P1) (pin 5))
      (node (ref SW1) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref R1) (pin 2)))
    (net (code 92) (name /swclk)
      (node (ref U2) (pin 37))
      (node (ref P1) (pin 2)))
    (net (code 93) (name /swdio)
      (node (ref U2) (pin 34))
      (node (ref P1) (pin 4)))
    (net (code 94) (name /boot0)
      (node (ref U2) (pin 44))
      (node (ref C9) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref SW2) (pin 1)))
    (net (code 95) (name /MISO)
      (node (ref U8) (pin 10))
      (node (ref U2) (pin 17)))
    (net (code 96) (name /CS_Wifi)
      (node (ref U2) (pin 14))
      (node (ref U8) (pin 9)))
    (net (code 97) (name /CLK)
      (node (ref U8) (pin 14))
      (node (ref U2) (pin 15)))
    (net (code 98) (name /MOSI)
      (node (ref U2) (pin 16))
      (node (ref U8) (pin 13)))
    (net (code 99) (name /mfp)
      (node (ref U2) (pin 10))
      (node (ref U4) (pin 12))
      (node (ref R3) (pin 2)))
    (net (code 100) (name "Net-(U4-Pad13)")
      (node (ref U4) (pin 13)))
    (net (code 101) (name "Net-(U4-Pad14)")
      (node (ref U4) (pin 14)))
    (net (code 102) (name "Net-(U4-Pad4)")
      (node (ref U4) (pin 4)))
    (net (code 103) (name "Net-(U4-Pad5)")
      (node (ref U4) (pin 5)))
    (net (code 104) (name "Net-(U4-Pad7)")
      (node (ref U4) (pin 7)))
    (net (code 105) (name "Net-(BT1-Pad1)")
      (node (ref U4) (pin 8))
      (node (ref BT1) (pin 1)))))