{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Tache","Interruption","TEST","Port Blynk","Protocole SPI","Led erreur","AddEEPROM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tache","index":0,"n_rows":1,"n_cols":4,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Tache",null,null,"Importance"]

{"sheet":"Interruption","index":1,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Type","Ligne","Corespondence","Prio","Reaction"]
["IO",0,"MFP"]
["IO",1]
["IO",2]
["IO",3]
["IO",4]
["IO",5]
["IO",6]
["IO",7]
["IO",8,"Left"]
["IO",9]
["IO",10]
["IO",11]
["IO",12,"Right"]
["IO",13,"Up"]
["IO",14,"Select"]
["IO",15,"Down"]

{"sheet":"TEST","index":2,"n_rows":1,"n_cols":4,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["File","Name","Resultat","Documentation"]

{"sheet":"Port Blynk","index":3,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":false,"merged":[[0,4,0,8],[4,4,4,8]]}
[null,"Port","Type"]

{"sheet":"Protocole SPI","index":4,"n_rows":17,"n_cols":27,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,1,0,8],[0,10,0,17]]}
[null,"ESP",{"$nulls":8},"STM",{"$nulls":8},"Hex","Action",null,"Abreviation ","Nom",null,"Type","ID"]
["sync RTC",0,0,0,0,"X","X","X","X",{"$nulls":10},"0x0X","sync RTC"]
[null,"Y","Y","Y","Y","Y","Y","Y","Y",{"$nulls":10},"0x1X"]
[null,"M","M","M","M","M","M","M","M",{"$nulls":10},"0x2X"]
[null,"J","J","J","J","J","J","J","J",{"$nulls":10},"0x3X"]
[null,"Day","Day","Day","Day","Day","Day","Day","Day",{"$nulls":10},"0x4X"]
[null,"H","H","H","H","H","H","H","H",{"$nulls":10},"0x5X"]
[null,"M","M","M","M","M","M","M","M",{"$nulls":10},"0x6X"]
[null,"S","S","S","S","S","S","S","S",{"$nulls":10},"0x7X"]
[{"$nulls":19},"0x8X"]
[{"$nulls":19},"0x9X"]
[{"$nulls":19},"0xAX"]
[{"$nulls":19},"0xBX"]
[{"$nulls":19},"0xCX"]
[{"$nulls":19},"0xDX"]
[{"$nulls":19},"0xEX"]
[{"$nulls":19},"0xFX"]

{"sheet":"Led erreur","index":5,"n_rows":5,"n_cols":5,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[null,null,"Vert","Orange","Rouge"]
["Erreur","RAS",1,0,0]
[null,"Coupure courant",1,1,0]
[null,"Batterie RTC",1,0,1]
[null,"Oscillator fail",0,0,1]

{"sheet":"AddEEPROM","index":6,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Nom","address Eeprpm"]
["Blanc Max","0x0000"]
["Chaud Max","0x0002"]
["Bleu Max","0x0004"]
["Rouge Max","0x0006"]
["UV Max","0x0008"]
["Vert Max","0x000A"]
["Blanc Pente","0x000C"]
["Chaud Pente","0x000E"]
["Bleu Pente","0x0010"]
["Rouge Pente","0x0012"]
["UV Pente","0x0014"]
["Vert Pente","0x0016"]
["Blanc Demmarage","0x0018"]
["Chaud Demmarage","0x001A"]
["Bleu Demmarage","0x001C"]
["Rouge Demmarage","0x001E"]
["UV Demmarage","0x0020"]
["Vert Demmarage","0x0022"]
["Blanc Arret","0x0024"]
["Chaud Arret","0x0028"]
["Bleu Arret","0x002A"]
["Rouge Arret","0x002C"]
["UV Arret","0x002E"]
["Vert Arret","0x0030"]