(export (version D)
  (design
    (source D:/Projet/rampesLeds/Eda/Drivers/drivers.sch)
    (date "04/07/2018 15:55:18")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source drivers.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P2)
      (value CONN_01X01)
      (footprint MH:MH2mm8)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5704BD0C))
    (comp (ref P3)
      (value CONN_01X01)
      (footprint MH:MH2mm8)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5704C456))
    (comp (ref P1)
      (value CONN_01X03)
      (footprint Connector:Bornier2.54_1x3)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 56BF4595))
    (comp (ref R1)
      (value R)
      (footprint R:ciment)
      (fields
        (field (name vendor) Value)
        (field (name part) SMW52R0JT)
        (field (name p/mouser) Value)
        (field (name p/farnell) Value))
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EB844A))
    (comp (ref Q1)
      (value P_MOSFET)
      (footprint U:SOT-223)
      (libsource (lib global) (part P_MOSFET))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3CD204)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib global) (part P_MOSFET)
      (fields
        (field (name Reference) Q)
        (field (name Value) P_MOSFET))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name S) (type input))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical global)
      (uri D:\Projet\Librairie_Kicad\schematic\global.lib))
    (library (logical conn)
      (uri D:\Projet\Librairie_Kicad\schematic\conn.lib)))
  (nets
    (net (code 1) (name "Net-(Q1-Pad3)")
      (node (ref Q1) (pin 3))
      (node (ref R1) (pin 1)))
    (net (code 2) (name "Net-(P1-Pad2)")
      (node (ref Q1) (pin 1))
      (node (ref P1) (pin 2)))
    (net (code 3) (name "Net-(P1-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref P1) (pin 1)))
    (net (code 4) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3))
      (node (ref Q1) (pin 2)))
    (net (code 5) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 6) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))))