(export (version D)
  (design
    (source C:\Users\e_rcluze\Documents\Autres\Projet\rampesleds\Eda\Drivers\drivers.sch)
    (date "29/05/2019 10:18:14")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source drivers.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref P2)
      (value CONN_01X01)
      (footprint MH:MH2mm8)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5704BD0C))
    (comp (ref P3)
      (value CONN_01X01)
      (footprint MH:MH2mm8)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib conn) (part CONN_01X01) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5704C456))
    (comp (ref P1)
      (value CONN_01X03)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 4))
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56BF4595))
    (comp (ref Q1)
      (value N_MOSFET)
      (footprint U:SOT-223)
      (fields
        (field (name Partkeepr) 2002))
      (libsource (lib global) (part N_MOSFET) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB86B6B))
    (comp (ref R3)
      (value 10k)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC442E))
    (comp (ref R2)
      (value 120)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 911))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCC457C))
    (comp (ref R1)
      (value R)
      (footprint R:ciment)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib global) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EB844A)))
  (libparts
    (libpart (lib conn) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib global) (part N_MOSFET)
      (fields
        (field (name Reference) Q)
        (field (name Value) N_MOSFET))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name S) (type input))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/conn.lib))
    (library (logical global)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/global.lib)))
  (nets
    (net (code 1) (name "Net-(Q1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 2) (name "Net-(P1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref P1) (pin 1)))
    (net (code 3) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 4) (name "Net-(P1-Pad3)")
      (node (ref P1) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref R3) (pin 2)))
    (net (code 5) (name "Net-(P1-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref P1) (pin 2)))
    (net (code 6) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 7) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))))