(export (version D)
  (design
    (source /home/rcluze/Projet/Autres/rampesLeds/eda/Controle/proc.sch)
    (date "mer. 10 mai 2017 16:18:39 CEST")
    (tool "Eeschema 4.0.6-e0-6349~53~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source proc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R5)
      (value 10K)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61BDD))
    (comp (ref R4)
      (value 10K)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61C77))
    (comp (ref R3)
      (value 10K)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61CD4))
    (comp (ref R6)
      (value 510)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84A2E))
    (comp (ref R7)
      (value 330)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84A83))
    (comp (ref C5)
      (value 10µ)
      (footprint C:CP_Alu)
      (libsource (lib proc-cache) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84AD6))
    (comp (ref P7)
      (value Alim)
      (footprint Connector:bornier_2x1)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C85860))
    (comp (ref C1)
      (value 100n)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57054B1D))
    (comp (ref C3)
      (value 10n)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57054C33))
    (comp (ref SW1)
      (value boot)
      (footprint SW:SW)
      (libsource (lib global) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061862))
    (comp (ref R9)
      (value 10K)
      (footprint R:0603)
      (fields
        (field (name vendor) Value)
        (field (name part) Value)
        (field (name p/mouser) Value)
        (field (name p/farnell) Value))
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061F55))
    (comp (ref P8)
      (value Debug)
      (footprint Connector:1X6_2.54)
      (libsource (lib conn) (part CONN_01X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 57062F1C))
    (comp (ref P5)
      (value CONN_01X06)
      (footprint Connector:bornier_6x1)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 570CFB57))
    (comp (ref P6)
      (value CONN_01X06)
      (footprint Connector:bornier_6x1)
      (libsource (lib conn) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 570CFBC4))
    (comp (ref R1)
      (value 100)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E42C5))
    (comp (ref D1)
      (value rouge)
      (footprint Dialight:598-xxxx-107F)
      (fields
        (field (name part) 598-8010-107F))
      (libsource (lib global) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4326))
    (comp (ref R2)
      (value 100)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4510))
    (comp (ref D2)
      (value vert)
      (footprint Dialight:598-xxxx-107F)
      (fields
        (field (name part) 598-8070-107F))
      (libsource (lib global) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4516))
    (comp (ref P3)
      (value MH)
      (footprint MH:MH2mm69)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237B4F))
    (comp (ref P4)
      (value MH)
      (footprint MH:MH2mm69)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237BDA))
    (comp (ref P1)
      (value MH)
      (footprint MH:MH2mm69)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237C51))
    (comp (ref P2)
      (value MH)
      (footprint MH:MH2mm69)
      (libsource (lib conn) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237CC8))
    (comp (ref BT1)
      (value Battery)
      (footprint Connector:batterie)
      (libsource (lib global) (part Battery))
      (sheetpath (names /) (tstamps /))
      (tstamp 5725FA6C))
    (comp (ref R10)
      (value 100K)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5729F1B3))
    (comp (ref U2)
      (value M24C32)
      (footprint U:SO8N)
      (libsource (lib ST) (part M24C32))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E3BDFF))
    (comp (ref U3)
      (value M41T83)
      (footprint U:SOX18)
      (libsource (lib ST) (part M41T83))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E3C0BF))
    (comp (ref U1)
      (value STM32F030C8)
      (footprint U:LQFP48)
      (libsource (lib ST) (part STM32F030C8))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E4E08A))
    (comp (ref C2)
      (value 100n)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57054BC2))
    (comp (ref C6)
      (value 100nF)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E50214))
    (comp (ref R8)
      (value 10K)
      (footprint R:0603)
      (libsource (lib global) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E50DED))
    (comp (ref C7)
      (value 100nF)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E518CC))
    (comp (ref C4)
      (value 100n)
      (footprint C:CP_Alu)
      (libsource (lib proc-cache) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 570673A6))
    (comp (ref C8)
      (value 1µF)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E54C42))
    (comp (ref C9)
      (value 4.7uF)
      (footprint C:0603)
      (libsource (lib global) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E55433))
    (comp (ref U4)
      (value LM317)
      (footprint U:LM317)
      (libsource (lib proc-rescue) (part LM317-RESCUE-proc))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E4F7D8))
    (comp (ref Q1)
      (value P_MOSFET)
      (footprint U:SOT-223)
      (fields
        (field (name vendor) Value)
        (field (name part) Value)
        (field (name p/mouser) Value)
        (field (name p/farnell) Value))
      (libsource (lib global) (part P_MOSFET))
      (sheetpath (names /) (tstamps /))
      (tstamp 58122852))
    (comp (ref SW2)
      (value reset)
      (footprint SW:SW)
      (libsource (lib global) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061F5B)))
  (libparts
    (libpart (lib global) (part Battery)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part C)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X01)
      (description "Connector 01x01")
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X05)
      (description "Connector 01x05")
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib conn) (part CONN_01X06)
      (description "Connector 01x06")
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib proc-cache) (part CP1)
      (footprints
        (fp SMD*_Pol)
        (fp c_elec*)
        (fp C*elec)
        (fp TantalC*)
        (fp Elko*)
        (fp CP*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib global) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib proc-rescue) (part LM317-RESCUE-proc)
      (fields
        (field (name Reference) U)
        (field (name Value) LM317-RESCUE-proc))
      (pins
        (pin (num 0) (name Therm) (type input))
        (pin (num 1) (name Adj) (type input))
        (pin (num 2) (name Vout) (type input))
        (pin (num 3) (name Vin) (type input))))
    (libpart (lib ST) (part M24C32)
      (fields
        (field (name Reference) U)
        (field (name Value) M24C32))
      (pins
        (pin (num 1) (name E0) (type input))
        (pin (num 2) (name E1) (type input))
        (pin (num 3) (name E2) (type input))
        (pin (num 4) (name VSS) (type input))
        (pin (num 5) (name VCC) (type input))
        (pin (num 6) (name ~WC) (type input))
        (pin (num 7) (name SCL) (type input))
        (pin (num 8) (name SDA) (type input))))
    (libpart (lib ST) (part M41T83)
      (fields
        (field (name Reference) U)
        (field (name Value) M41T83))
      (pins
        (pin (num 1) (name NC) (type input))
        (pin (num 2) (name NF) (type input))
        (pin (num 3) (name NF) (type input))
        (pin (num 4) (name NC) (type input))
        (pin (num 5) (name ~RST) (type input))
        (pin (num 6) (name DU) (type input))
        (pin (num 7) (name SQW) (type input))
        (pin (num 8) (name VBAT) (type input))
        (pin (num 9) (name VSS) (type input))
        (pin (num 10) (name SDA) (type input))
        (pin (num 11) (name SCL) (type input))
        (pin (num 12) (name ~IRQ1~/FT/OUT) (type input))
        (pin (num 13) (name NC) (type input))
        (pin (num 14) (name ~IRQ2) (type input))
        (pin (num 15) (name VCC) (type input))
        (pin (num 16) (name NF) (type input))
        (pin (num 17) (name NF) (type input))
        (pin (num 18) (name NC) (type input))))
    (libpart (lib global) (part P_MOSFET)
      (fields
        (field (name Reference) Q)
        (field (name Value) P_MOSFET))
      (pins
        (pin (num 1) (name S) (type input))
        (pin (num 2) (name G) (type input))
        (pin (num 3) (name D) (type input))))
    (libpart (lib global) (part R)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib ST) (part STM32F030C8)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030C8))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14/OSC32_IN) (type BiDi))
        (pin (num 4) (name PC15/OSC32_OUT) (type BiDi))
        (pin (num 5) (name PF0/OSC_IN) (type BiDi))
        (pin (num 6) (name PF1/OSC_OUT) (type BiDi))
        (pin (num 7) (name ~NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name PB11) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name PF6) (type BiDi))
        (pin (num 36) (name PF7) (type BiDi))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib global) (part SW_PUSH)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical proc-rescue)
      (uri /home/rcluze/Projet/Autres/rampesLeds/eda/Controle/proc-rescue.lib))
    (library (logical conn)
      (uri /home/rcluze/Projet/Autres/Librairie_Kicad/schematic/conn.lib))
    (library (logical proc-cache)
      (uri /home/rcluze/Projet/Autres/rampesLeds/eda/Controle/proc-cache.lib))
    (library (logical ST)
      (uri /home/rcluze/Projet/Autres/Librairie_Kicad/schematic/ST.lib))
    (library (logical global)
      (uri /home/rcluze/Projet/Autres/Librairie_Kicad/schematic/global.lib)))
  (nets
    (net (code 1) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 2) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 3) (name "Net-(U1-Pad32)")
      (node (ref U1) (pin 32)))
    (net (code 4) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 5) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 6) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 7) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 8) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 9) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 10) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 11) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 12) (name "Net-(R6-Pad1)")
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 13) (name "Net-(U4-Pad0)")
      (node (ref U4) (pin 0)))
    (net (code 14) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 15) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 16) (name "Net-(U1-Pad20)")
      (node (ref U1) (pin 20)))
    (net (code 17) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 18) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 19) (name "Net-(U1-Pad38)")
      (node (ref U1) (pin 38)))
    (net (code 20) (name /12V)
      (node (ref C4) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 21) (name /GND)
      (node (ref U1) (pin 23))
      (node (ref U3) (pin 16))
      (node (ref U3) (pin 3))
      (node (ref SW2) (pin 2))
      (node (ref U1) (pin 8))
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 17))
      (node (ref C5) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 6))
      (node (ref D2) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref U1) (pin 47))
      (node (ref Q1) (pin 2))
      (node (ref P7) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref C1) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref P8) (pin 3))
      (node (ref C7) (pin 1))
      (node (ref BT1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C8) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref C9) (pin 2)))
    (net (code 22) (name /s1)
      (node (ref U1) (pin 39))
      (node (ref P5) (pin 1)))
    (net (code 23) (name "Net-(R1-Pad2)")
      (node (ref U1) (pin 28))
      (node (ref R1) (pin 2)))
    (net (code 24) (name /swclk)
      (node (ref U1) (pin 37))
      (node (ref P8) (pin 2)))
    (net (code 25) (name "Net-(R2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref U1) (pin 27)))
    (net (code 26) (name /s7)
      (node (ref P6) (pin 1))
      (node (ref U1) (pin 46)))
    (net (code 27) (name /s6)
      (node (ref P5) (pin 6))
      (node (ref U1) (pin 45)))
    (net (code 28) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 29) (name /nrst)
      (node (ref C6) (pin 2))
      (node (ref SW1) (pin 1))
      (node (ref P8) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref R8) (pin 2)))
    (net (code 30) (name "Net-(P7-Pad2)")
      (node (ref Q1) (pin 3))
      (node (ref P7) (pin 2)))
    (net (code 31) (name /boot0)
      (node (ref R9) (pin 2))
      (node (ref SW2) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref U1) (pin 44)))
    (net (code 32) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 33) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 34) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 35) (name /VDD)
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref U3) (pin 15))
      (node (ref U3) (pin 6))
      (node (ref U1) (pin 24))
      (node (ref C5) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref C2) (pin 1))
      (node (ref U1) (pin 48))
      (node (ref C9) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref P8) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref SW1) (pin 2)))
    (net (code 36) (name "Net-(U3-Pad14)")
      (node (ref U3) (pin 14)))
    (net (code 37) (name /s12)
      (node (ref P6) (pin 6))
      (node (ref U1) (pin 6)))
    (net (code 38) (name /s11)
      (node (ref P6) (pin 5))
      (node (ref U1) (pin 5)))
    (net (code 39) (name /s10)
      (node (ref P6) (pin 4))
      (node (ref U1) (pin 4)))
    (net (code 40) (name /s9)
      (node (ref U1) (pin 3))
      (node (ref P6) (pin 3)))
    (net (code 41) (name /s8)
      (node (ref P6) (pin 2))
      (node (ref U1) (pin 2)))
    (net (code 42) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 43) (name "Net-(U3-Pad13)")
      (node (ref U3) (pin 13)))
    (net (code 44) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 45) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 46) (name /swdio)
      (node (ref U1) (pin 34))
      (node (ref P8) (pin 4)))
    (net (code 47) (name /s5)
      (node (ref U1) (pin 43))
      (node (ref P5) (pin 5)))
    (net (code 48) (name /s4)
      (node (ref P5) (pin 4))
      (node (ref U1) (pin 42)))
    (net (code 49) (name /s3)
      (node (ref U1) (pin 41))
      (node (ref P5) (pin 3)))
    (net (code 50) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 51) (name /s2)
      (node (ref P5) (pin 2))
      (node (ref U1) (pin 40)))
    (net (code 52) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 53) (name /mfp)
      (node (ref U1) (pin 10))
      (node (ref U3) (pin 12))
      (node (ref R3) (pin 2)))
    (net (code 54) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 55) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 56) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 57) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 58) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 59) (name /sdl)
      (node (ref R4) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref U3) (pin 11))
      (node (ref U1) (pin 21)))
    (net (code 60) (name /sda)
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 22))
      (node (ref U3) (pin 10))
      (node (ref R5) (pin 2)))
    (net (code 61) (name /wc)
      (node (ref R10) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 13)))))