(export (version D)
  (design
    (source C:\Users\e_rcluze\Documents\Autres\projet\rampesLeds\Eda\Proc\proc.sch)
    (date "11/02/2020 11:25:38")
    (tool "Eeschema (5.0.2)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source proc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R5)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61BDD))
    (comp (ref R4)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61C77))
    (comp (ref R3)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C61CD4))
    (comp (ref R6)
      (value 510)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 913))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84A2E))
    (comp (ref R7)
      (value 330)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 914))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84A83))
    (comp (ref C5)
      (value 10µF)
      (footprint C:CP_CMS5X5.8)
      (fields
        (field (name Partkeepr) 609))
      (libsource (lib proc-rescue) (part CP-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C84AD6))
    (comp (ref P7)
      (value Alim)
      (footprint Connector:Bornier2.54_1x2)
      (fields
        (field (name Partkeepr) 4))
      (libsource (lib proc-rescue) (part CONN_01X02-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 56C85860))
    (comp (ref SW1)
      (value boot)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib proc-rescue) (part SW_PUSH-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061862))
    (comp (ref R9)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061F55))
    (comp (ref P8)
      (value Debug)
      (footprint Connector:PinHeader2.54_1X5)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib proc-rescue) (part CONN_01X05-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57062F1C))
    (comp (ref P5)
      (value CONN_01X06)
      (footprint Connector:Bornier2.54_1x6)
      (fields
        (field (name Partkeepr) 2))
      (libsource (lib proc-rescue) (part CONN_01X06-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570CFB57))
    (comp (ref D1)
      (value rouge)
      (footprint LED:0805)
      (fields
        (field (name Partkeepr) 1103))
      (libsource (lib proc-rescue) (part LED-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4326))
    (comp (ref R2)
      (value 100)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 912))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4510))
    (comp (ref D2)
      (value vert)
      (footprint LED:0805)
      (fields
        (field (name Partkeepr) 1106))
      (libsource (lib proc-rescue) (part LED-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E4516))
    (comp (ref P3)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib proc-rescue) (part CONN_01X01-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237B4F))
    (comp (ref P4)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib proc-rescue) (part CONN_01X01-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237BDA))
    (comp (ref P1)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib proc-rescue) (part CONN_01X01-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237C51))
    (comp (ref P2)
      (value MH)
      (footprint MH:MH3mm)
      (fields
        (field (name Partkeepr) NC))
      (libsource (lib proc-rescue) (part CONN_01X01-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57237CC8))
    (comp (ref BT1)
      (value Battery)
      (footprint Connector:batterie)
      (fields
        (field (name Partkeepr) 3))
      (libsource (lib proc-rescue) (part Battery-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5725FA6C))
    (comp (ref R10)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5729F1B3))
    (comp (ref U2)
      (value M24C32)
      (footprint U:SO8N)
      (fields
        (field (name Partkeepr) 1700))
      (libsource (lib proc-rescue) (part M24C32-ST) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E3BDFF))
    (comp (ref U3)
      (value M41T83)
      (footprint U:SOX18)
      (fields
        (field (name Partkeepr) 1600))
      (libsource (lib proc-rescue) (part M41T83-ST) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E3C0BF))
    (comp (ref C2)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57054BC2))
    (comp (ref C6)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E50214))
    (comp (ref R8)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E50DED))
    (comp (ref C7)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E518CC))
    (comp (ref C4)
      (value 100nF)
      (footprint C:3216-18)
      (fields
        (field (name Partkeepr) 610))
      (libsource (lib proc-rescue) (part CP-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570673A6))
    (comp (ref U4)
      (value LM317)
      (footprint U:SOT-223)
      (fields
        (field (name Partkeepr) 1800))
      (libsource (lib proc-rescue) (part LM317-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E4F7D8))
    (comp (ref SW2)
      (value reset)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib proc-rescue) (part SW_PUSH-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 57061F5B))
    (comp (ref J1)
      (value Micro_USB)
      (footprint Connector:Micro-USB)
      (fields
        (field (name Partkeepr) 50))
      (libsource (lib proc-rescue) (part Micro_USB-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59256A87))
    (comp (ref U1)
      (value STM32F401RC)
      (footprint U:LQFP64)
      (fields
        (field (name Partkeepr) 2102))
      (libsource (lib proc-rescue) (part STM32F401RC-ST) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592DBF4D))
    (comp (ref Y1)
      (value 25Mhz)
      (footprint Y:5032)
      (fields
        (field (name Partkeepr) 1650))
      (libsource (lib proc-rescue) (part Crystal-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1245))
    (comp (ref C10)
      (value 22pF)
      (footprint C:0603)
      (fields
        (field (name Partkeepr) 600))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1B87))
    (comp (ref C11)
      (value 22pF)
      (footprint C:0603)
      (fields
        (field (name Partkeepr) 600))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E1CB0))
    (comp (ref C13)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E7E79))
    (comp (ref C14)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E8599))
    (comp (ref C9)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E893A))
    (comp (ref C8)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E8DCA))
    (comp (ref C3)
      (value 1µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 605))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E902A))
    (comp (ref C12)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E97A8))
    (comp (ref C1)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 592E9BBE))
    (comp (ref P9)
      (value I2C)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib proc-rescue) (part CONN_01X03-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59B166C5))
    (comp (ref U5)
      (value ESP-12F)
      (footprint U:ESP-12F)
      (fields
        (field (name Partkeepr) 2500))
      (libsource (lib Module) (part ESP-12F) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B362B9A))
    (comp (ref P11)
      (value Ventilateur)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib proc-rescue) (part CONN_01X03-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B364CD7))
    (comp (ref R11)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3A483C))
    (comp (ref R12)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3A48BD))
    (comp (ref D3)
      (value Orange)
      (footprint LED:0805)
      (fields
        (field (name Partkeepr) 1102))
      (libsource (lib proc-rescue) (part LED-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3A77C2))
    (comp (ref R13)
      (value 100)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 912))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3A7872))
    (comp (ref R1)
      (value 100)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 912))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 570E42C5))
    (comp (ref P10)
      (value Thermometre)
      (footprint Connector:Bornier2.54_1x3)
      (fields
        (field (name Partkeepr) 5))
      (libsource (lib proc-rescue) (part CONN_01X03-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3AE3C4))
    (comp (ref Q1)
      (value N_MOSFET)
      (footprint U:SOT-223)
      (fields
        (field (name Partkeepr) 2001))
      (libsource (lib proc-rescue) (part N_MOSFET-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3CCE17))
    (comp (ref P6)
      (value CONN_01X04)
      (footprint Connector:Bornier2.54_1x4)
      (fields
        (field (name Partkeepr) 6))
      (libsource (lib proc-rescue) (part CONN_01X04-conn) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3CE1CC))
    (comp (ref R14)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3D4E22))
    (comp (ref C15)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3D4E2B))
    (comp (ref SW3)
      (value aquit)
      (footprint SW:SW)
      (fields
        (field (name Partkeepr) 200))
      (libsource (lib proc-rescue) (part SW_PUSH-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3D4E31))
    (comp (ref C17)
      (value 100nF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 606))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEE290C))
    (comp (ref R15)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEFD47A))
    (comp (ref R16)
      (value 10K)
      (footprint R:0805)
      (fields
        (field (name Partkeepr) 910))
      (libsource (lib proc-rescue) (part R-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF02DB9))
    (comp (ref SJ1)
      (value Mode)
      (footprint Jumper:Jumper_2.54mm)
      (fields
        (field (name Partkeepr) 100))
      (libsource (lib proc-rescue) (part Jumper-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF26828))
    (comp (ref C16)
      (value 4.7µF)
      (footprint C:0805)
      (fields
        (field (name Partkeepr) 607))
      (libsource (lib proc-rescue) (part C-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF79E5C))
    (comp (ref C18)
      (value 1µF)
      (footprint C:CP_CMS4X5.8)
      (fields
        (field (name Partkeepr) 608))
      (libsource (lib proc-rescue) (part CP-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF83309))
    (comp (ref D4)
      (value D)
      (footprint D:SMA)
      (fields
        (field (name Partkeepr) 1302))
      (libsource (lib proc-rescue) (part D-global) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF8B24F))
    (comp (ref P12)
      (value ProgESP)
      (footprint Connector:PinHeader2.54_1X3)
      (libsource (lib conn) (part CONN_01X03) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF95433)))
  (libparts
    (libpart (lib Module) (part ESP-12F)
      (fields
        (field (name Reference) U)
        (field (name Value) ESP-12F))
      (pins
        (pin (num 1) (name RST) (type input))
        (pin (num 2) (name ADC) (type input))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name GPIO16) (type input))
        (pin (num 5) (name GPIO14) (type input))
        (pin (num 6) (name GPIO12) (type input))
        (pin (num 7) (name GPIO13) (type input))
        (pin (num 8) (name VCC) (type input))
        (pin (num 9) (name CS0) (type input))
        (pin (num 10) (name MISO) (type input))
        (pin (num 11) (name GPIO9) (type input))
        (pin (num 12) (name GPIO10) (type input))
        (pin (num 13) (name MOSI) (type input))
        (pin (num 14) (name SCLK) (type input))
        (pin (num 15) (name GND) (type input))
        (pin (num 16) (name GPIO15) (type input))
        (pin (num 17) (name GPIO2) (type input))
        (pin (num 18) (name GPIO0) (type input))
        (pin (num 19) (name GPIO4) (type input))
        (pin (num 20) (name GPIO5) (type input))
        (pin (num 21) (name RXD) (type input))
        (pin (num 22) (name TXD) (type input))))
    (libpart (lib conn) (part CONN_01X03)
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib proc-rescue) (part Battery-global)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery-global))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proc-rescue) (part C-global)
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C-global))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X01-conn)
      (footprints
        (fp Pin_Header_Straight_1X01)
        (fp Pin_Header_Angled_1X01)
        (fp Socket_Strip_Straight_1X01)
        (fp Socket_Strip_Angled_1X01))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X01-conn))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X02-conn)
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X03-conn)
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X04-conn)
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X05-conn)
      (footprints
        (fp Pin_Header_Straight_1X05)
        (fp Pin_Header_Angled_1X05)
        (fp Socket_Strip_Straight_1X05)
        (fp Socket_Strip_Angled_1X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X05-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib proc-rescue) (part CONN_01X06-conn)
      (footprints
        (fp Pin_Header_Straight_1X06)
        (fp Pin_Header_Angled_1X06)
        (fp Socket_Strip_Straight_1X06)
        (fp Socket_Strip_Angled_1X06))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X06-conn))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib proc-rescue) (part CP-global)
      (footprints
        (fp CP*)
        (fp Elko*)
        (fp TantalC*)
        (fp C*elec)
        (fp c_elec*)
        (fp SMD*_Pol))
      (fields
        (field (name Reference) C)
        (field (name Value) CP-global))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proc-rescue) (part Crystal-global)
      (footprints
        (fp Crystal_*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal-global))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib proc-rescue) (part D-global)
      (footprints
        (fp Diode_*)
        (fp D-Pak_TO252AA)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*))
      (fields
        (field (name Reference) D)
        (field (name Value) D-global))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib proc-rescue) (part Jumper-global)
      (fields
        (field (name Reference) SJ)
        (field (name Value) Jumper-global))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proc-rescue) (part LED-global)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED-global))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib proc-rescue) (part LM317-global)
      (fields
        (field (name Reference) U)
        (field (name Value) LM317-global))
      (pins
        (pin (num 1) (name Adj) (type input))
        (pin (num 2) (name Vout) (type input))
        (pin (num 3) (name Vin) (type input))))
    (libpart (lib proc-rescue) (part M24C32-ST)
      (fields
        (field (name Reference) U)
        (field (name Value) M24C32-ST)
        (field (name Partkeepr) 1700))
      (pins
        (pin (num 1) (name E0) (type input))
        (pin (num 2) (name E1) (type input))
        (pin (num 3) (name E2) (type input))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name ~WC) (type input))
        (pin (num 7) (name SCL) (type BiDi))
        (pin (num 8) (name SDA) (type BiDi))))
    (libpart (lib proc-rescue) (part M41T83-ST)
      (fields
        (field (name Reference) U)
        (field (name Value) M41T83-ST)
        (field (name Partkeepr) 1600))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name NF) (type input))
        (pin (num 3) (name NF) (type input))
        (pin (num 4) (name NC) (type input))
        (pin (num 5) (name ~RST) (type input))
        (pin (num 6) (name DU) (type input))
        (pin (num 7) (name SQW) (type input))
        (pin (num 8) (name VBAT) (type input))
        (pin (num 9) (name VSS) (type input))
        (pin (num 10) (name SDA) (type input))
        (pin (num 11) (name SCL) (type input))
        (pin (num 12) (name ~IRQ1~/FT/OUT) (type input))
        (pin (num 13) (name NC) (type input))
        (pin (num 14) (name ~IRQ2) (type input))
        (pin (num 15) (name VCC) (type input))
        (pin (num 16) (name NF) (type input))
        (pin (num 17) (name NF) (type input))
        (pin (num 18) (name NC) (type input))))
    (libpart (lib proc-rescue) (part Micro_USB-conn)
      (fields
        (field (name Reference) J)
        (field (name Value) Micro_USB-conn))
      (pins
        (pin (num 0) (name USB_SH) (type input))
        (pin (num 1) (name USB_VBUS) (type input))
        (pin (num 2) (name USB_N) (type input))
        (pin (num 3) (name USB_P) (type input))
        (pin (num 4) (name USB_ID) (type input))
        (pin (num 5) (name USB_GND) (type input))))
    (libpart (lib proc-rescue) (part N_MOSFET-global)
      (fields
        (field (name Reference) Q)
        (field (name Value) N_MOSFET-global))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name S) (type input))))
    (libpart (lib proc-rescue) (part R-global)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R-global))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proc-rescue) (part STM32F401RC-ST)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F401RC-ST)
        (field (name Partkeepr) 2102))
      (pins
        (pin (num 1) (name VBAT) (type input))
        (pin (num 2) (name PC13) (type input))
        (pin (num 3) (name PC14) (type input))
        (pin (num 4) (name PC15) (type input))
        (pin (num 5) (name PH0) (type input))
        (pin (num 6) (name PH1) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name PC0) (type input))
        (pin (num 9) (name PC1) (type input))
        (pin (num 10) (name PC2) (type input))
        (pin (num 11) (name PC3) (type input))
        (pin (num 12) (name VSSA) (type input))
        (pin (num 13) (name VDDA) (type input))
        (pin (num 14) (name PA0) (type input))
        (pin (num 15) (name PA1) (type input))
        (pin (num 16) (name PA2) (type input))
        (pin (num 17) (name PA3) (type input))
        (pin (num 18) (name VSS) (type input))
        (pin (num 19) (name VDD) (type input))
        (pin (num 20) (name PA4) (type input))
        (pin (num 21) (name PA5) (type input))
        (pin (num 22) (name PA6) (type input))
        (pin (num 23) (name PA7) (type input))
        (pin (num 24) (name PC4) (type input))
        (pin (num 25) (name PC5) (type input))
        (pin (num 26) (name PB0) (type input))
        (pin (num 27) (name PB1) (type input))
        (pin (num 28) (name PB2) (type input))
        (pin (num 29) (name PB10) (type input))
        (pin (num 30) (name VCAP1) (type input))
        (pin (num 31) (name VSS) (type input))
        (pin (num 32) (name VDD) (type input))
        (pin (num 33) (name PB12) (type input))
        (pin (num 34) (name PB13) (type input))
        (pin (num 35) (name PB14) (type input))
        (pin (num 36) (name PB15) (type input))
        (pin (num 37) (name PC6) (type input))
        (pin (num 38) (name PC7) (type input))
        (pin (num 39) (name PC8) (type input))
        (pin (num 40) (name PC9) (type input))
        (pin (num 41) (name PA8) (type input))
        (pin (num 42) (name PA9) (type input))
        (pin (num 43) (name PA10) (type input))
        (pin (num 44) (name PA11) (type input))
        (pin (num 45) (name PA12) (type input))
        (pin (num 46) (name PA13) (type input))
        (pin (num 47) (name VDD) (type input))
        (pin (num 48) (name VSS) (type input))
        (pin (num 49) (name PA14) (type input))
        (pin (num 50) (name PA15) (type input))
        (pin (num 51) (name PC10) (type input))
        (pin (num 52) (name PC11) (type input))
        (pin (num 53) (name PC12) (type input))
        (pin (num 54) (name PD2) (type input))
        (pin (num 55) (name PB3) (type input))
        (pin (num 56) (name PB4) (type input))
        (pin (num 57) (name PB5) (type input))
        (pin (num 58) (name PB6) (type input))
        (pin (num 59) (name PB7) (type input))
        (pin (num 60) (name BOOT0) (type input))
        (pin (num 61) (name PB8) (type input))
        (pin (num 62) (name PB9) (type input))
        (pin (num 63) (name VSS) (type input))
        (pin (num 64) (name VDD) (type input))))
    (libpart (lib proc-rescue) (part SW_PUSH-global)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH-global))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical Module)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/Module.lib))
    (library (logical conn)
      (uri C:\Users\e_rcluze\Documents\Autres\Projet\librairie_kicad/schematic/conn.lib))
    (library (logical proc-rescue)
      (uri C:\Users\e_rcluze\Documents\Autres\projet\rampesLeds\Eda\Proc/proc-rescue.lib)))
  (nets
    (net (code 1) (name "Net-(U5-Pad4)")
      (node (ref U5) (pin 4)))
    (net (code 2) (name "Net-(R15-Pad2)")
      (node (ref U5) (pin 17))
      (node (ref R15) (pin 2)))
    (net (code 3) (name "Net-(U5-Pad19)")
      (node (ref U5) (pin 19)))
    (net (code 4) (name "Net-(U5-Pad2)")
      (node (ref U5) (pin 2)))
    (net (code 5) (name "Net-(U5-Pad20)")
      (node (ref U5) (pin 20)))
    (net (code 6) (name "Net-(R12-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref U5) (pin 3)))
    (net (code 7) (name "Net-(U5-Pad5)")
      (node (ref U5) (pin 5)))
    (net (code 8) (name "Net-(U5-Pad6)")
      (node (ref U5) (pin 6)))
    (net (code 9) (name "Net-(U5-Pad7)")
      (node (ref U5) (pin 7)))
    (net (code 10) (name /3.3V)
      (node (ref U3) (pin 15))
      (node (ref U2) (pin 5))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 64))
      (node (ref R8) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref P8) (pin 1))
      (node (ref U1) (pin 13))
      (node (ref U1) (pin 32))
      (node (ref C9) (pin 1))
      (node (ref U1) (pin 19))
      (node (ref C8) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U3) (pin 6))
      (node (ref R16) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref U5) (pin 8))
      (node (ref R12) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref P10) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref C14) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref U1) (pin 48)))
    (net (code 11) (name /CS_Wifi)
      (node (ref U5) (pin 9))
      (node (ref U1) (pin 20)))
    (net (code 12) (name /12V)
      (node (ref C4) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref P7) (pin 2))
      (node (ref P11) (pin 1)))
    (net (code 13) (name "Net-(U1-Pad51)")
      (node (ref U1) (pin 51)))
    (net (code 14) (name "Net-(U1-Pad50)")
      (node (ref U1) (pin 50)))
    (net (code 15) (name /I2C2_SDL)
      (node (ref U1) (pin 29))
      (node (ref P9) (pin 3)))
    (net (code 16) (name "Net-(R11-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref U5) (pin 1)))
    (net (code 17) (name /MISO)
      (node (ref U5) (pin 10))
      (node (ref U1) (pin 23)))
    (net (code 18) (name "Net-(U5-Pad11)")
      (node (ref U5) (pin 11)))
    (net (code 19) (name "Net-(U5-Pad12)")
      (node (ref U5) (pin 12)))
    (net (code 20) (name /MOSI)
      (node (ref U5) (pin 13))
      (node (ref U1) (pin 22)))
    (net (code 21) (name /GND)
      (node (ref Q1) (pin 3))
      (node (ref C17) (pin 2))
      (node (ref P8) (pin 3))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 4))
      (node (ref U3) (pin 16))
      (node (ref U3) (pin 17))
      (node (ref R6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref U1) (pin 47))
      (node (ref U1) (pin 18))
      (node (ref U1) (pin 31))
      (node (ref J1) (pin 5))
      (node (ref U1) (pin 12))
      (node (ref U1) (pin 63))
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref C4) (pin 2))
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref P10) (pin 3))
      (node (ref C8) (pin 2))
      (node (ref U5) (pin 15))
      (node (ref P11) (pin 3))
      (node (ref C9) (pin 2))
      (node (ref P9) (pin 1))
      (node (ref U5) (pin 16))
      (node (ref C11) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref SJ1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref P12) (pin 1))
      (node (ref C18) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref SW3) (pin 2))
      (node (ref C12) (pin 2)))
    (net (code 22) (name "Net-(D3-Pad2)")
      (node (ref R13) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 23) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref D1) (pin 2)))
    (net (code 24) (name /Themp)
      (node (ref P10) (pin 2))
      (node (ref U1) (pin 27)))
    (net (code 25) (name "Net-(U1-Pad52)")
      (node (ref U1) (pin 52)))
    (net (code 26) (name "Net-(C10-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref C10) (pin 1))
      (node (ref Y1) (pin 2)))
    (net (code 27) (name "Net-(U1-Pad36)")
      (node (ref U1) (pin 36)))
    (net (code 28) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 29) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 30) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 31) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 32) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 33) (name "Net-(U1-Pad35)")
      (node (ref U1) (pin 35)))
    (net (code 34) (name "Net-(U1-Pad34)")
      (node (ref U1) (pin 34)))
    (net (code 35) (name "Net-(U1-Pad33)")
      (node (ref U1) (pin 33)))
    (net (code 36) (name "Net-(C11-Pad1)")
      (node (ref Y1) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 37) (name "Net-(J1-Pad0)")
      (node (ref J1) (pin 0)))
    (net (code 38) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 39) (name "Net-(U1-Pad57)")
      (node (ref U1) (pin 57)))
    (net (code 40) (name "Net-(U1-Pad54)")
      (node (ref U1) (pin 54)))
    (net (code 41) (name "Net-(U1-Pad53)")
      (node (ref U1) (pin 53)))
    (net (code 42) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref U1) (pin 30)))
    (net (code 43) (name /mode)
      (node (ref U5) (pin 18))
      (node (ref SJ1) (pin 1))
      (node (ref R16) (pin 2)))
    (net (code 44) (name /RX)
      (node (ref U5) (pin 21))
      (node (ref P12) (pin 2)))
    (net (code 45) (name /TX)
      (node (ref P12) (pin 3))
      (node (ref U5) (pin 22)))
    (net (code 46) (name /aquit)
      (node (ref U1) (pin 14))
      (node (ref R14) (pin 2))
      (node (ref SW3) (pin 1))
      (node (ref C15) (pin 2)))
    (net (code 47) (name /s9)
      (node (ref P6) (pin 3))
      (node (ref U1) (pin 61)))
    (net (code 48) (name "Net-(P7-Pad1)")
      (node (ref Q1) (pin 2))
      (node (ref P7) (pin 1)))
    (net (code 49) (name /s7)
      (node (ref U1) (pin 58))
      (node (ref P6) (pin 1)))
    (net (code 50) (name /s8)
      (node (ref U1) (pin 59))
      (node (ref P6) (pin 2)))
    (net (code 51) (name /s10)
      (node (ref P6) (pin 4))
      (node (ref U1) (pin 62)))
    (net (code 52) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 53) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 54) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 55) (name "Net-(U3-Pad13)")
      (node (ref U3) (pin 13)))
    (net (code 56) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 57) (name "Net-(U3-Pad14)")
      (node (ref U3) (pin 14)))
    (net (code 58) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 59) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1)))
    (net (code 60) (name "Net-(P4-Pad1)")
      (node (ref P4) (pin 1)))
    (net (code 61) (name "Net-(P2-Pad1)")
      (node (ref P2) (pin 1)))
    (net (code 62) (name "Net-(P1-Pad1)")
      (node (ref P1) (pin 1)))
    (net (code 63) (name "Net-(D2-Pad2)")
      (node (ref R2) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 64) (name /s4)
      (node (ref U1) (pin 38))
      (node (ref P5) (pin 4)))
    (net (code 65) (name /s5)
      (node (ref U1) (pin 39))
      (node (ref P5) (pin 5)))
    (net (code 66) (name /s6)
      (node (ref P5) (pin 6))
      (node (ref U1) (pin 40)))
    (net (code 67) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 68) (name "Net-(BT1-Pad1)")
      (node (ref U3) (pin 8))
      (node (ref BT1) (pin 1)))
    (net (code 69) (name /nrst)
      (node (ref U1) (pin 7))
      (node (ref C6) (pin 2))
      (node (ref P8) (pin 5))
      (node (ref SW1) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 70) (name /s3)
      (node (ref U1) (pin 37))
      (node (ref P5) (pin 3)))
    (net (code 71) (name "Net-(C5-Pad1)")
      (node (ref U4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 72) (name /mfp)
      (node (ref R3) (pin 2))
      (node (ref U3) (pin 12))
      (node (ref U1) (pin 28)))
    (net (code 73) (name /boot0)
      (node (ref C7) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U1) (pin 60))
      (node (ref SW2) (pin 1)))
    (net (code 74) (name /s1)
      (node (ref U1) (pin 16))
      (node (ref P5) (pin 1)))
    (net (code 75) (name /s2)
      (node (ref U1) (pin 17))
      (node (ref P5) (pin 2)))
    (net (code 76) (name /L_orange)
      (node (ref U1) (pin 26))
      (node (ref R13) (pin 2)))
    (net (code 77) (name /CLK)
      (node (ref U1) (pin 21))
      (node (ref U5) (pin 14)))
    (net (code 78) (name /L_rouge)
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 24)))
    (net (code 79) (name /L_vert)
      (node (ref U1) (pin 25))
      (node (ref R2) (pin 2)))
    (net (code 80) (name /wc)
      (node (ref U1) (pin 3))
      (node (ref U2) (pin 6))
      (node (ref R10) (pin 2)))
    (net (code 82) (name /CMD)
      (node (ref P11) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 83) (name /I2C2_SDA)
      (node (ref U1) (pin 55))
      (node (ref P9) (pin 2)))
    (net (code 84) (name /sda)
      (node (ref U1) (pin 56))
      (node (ref U3) (pin 10))
      (node (ref U2) (pin 8))
      (node (ref R5) (pin 2)))
    (net (code 85) (name /USB_OTG_FS_VBUS)
      (node (ref U1) (pin 42))
      (node (ref J1) (pin 1)))
    (net (code 86) (name /sdl)
      (node (ref U3) (pin 11))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 41))
      (node (ref U2) (pin 7)))
    (net (code 87) (name /USB_OTG_FS_ID)
      (node (ref U1) (pin 43))
      (node (ref J1) (pin 4)))
    (net (code 88) (name /USB_OTG_FS_N)
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 44)))
    (net (code 89) (name /USB_OTG_FS_P)
      (node (ref J1) (pin 3))
      (node (ref U1) (pin 45)))
    (net (code 90) (name /swdio)
      (node (ref U1) (pin 46))
      (node (ref P8) (pin 4)))
    (net (code 91) (name /swclk)
      (node (ref U1) (pin 49))
      (node (ref P8) (pin 2)))))