{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Tache","Interruption","TEST","Port Blynk","Protocole SPI","Led erreur","AddEEPROM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tache","index":0,"n_rows":4,"n_cols":7,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Tache",null,null,"Importance",null,"Obligatoire","La rampes a led e peu pas fonctionné sans "]
[{"$nulls":5},"Erreur","La rampes a led peu fonctionné sans mais pas de détection d'erreur"]
[{"$nulls":5},"Confort","Confort d'utilisation de la rampes a led"]
[{"$nulls":5},"Surplus"]

{"sheet":"Interruption","index":1,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Type","Ligne","Corespondence","Prio","Reaction"]
["IO",0,"Aquit"]
["IO",1]
["IO",2,"MFP"]
["IO",3]
["IO",4]
["IO",5]
["IO",6]
["IO",7]
["IO",8]
["IO",9]
["IO",10]
["IO",11]
["IO",12]
["IO",13]
["IO",14]
["IO",15]
["TIM4"]

{"sheet":"TEST","index":2,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["File","Name","Resultat","Documentation"]
["PWM","void PWMSetDutyCycle(uint32_t sortie, uint16_t value);"]
["PWM","void PWMSetZero(uint32_t sortie);"]
["PWM","void PWMSetMAX(uint32_t sortie);"]
["PWM","void PWMStart(uint8_t sortie);"]
["PWM","uint16_t PWMvalue(uint8_t heure);"]
[]
["Freertos","void TimerTask(void const * argument);"]
["Freertos","void init();"]
["Freertos","uint16_t minimum(uint16_t a,uint16_t b);"]
[]
["Tab","uint8_t readCase(uint8_t sortie, uint8_t heure);"]
[]
["RTC","void readRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","void writeRTC(uint8_t add, uint8_t *tab, int len);"]
["RTC","uint8_t readMinute();"]
["RTC","uint8_t readHeure();"]
["RTC","void readDate(Date *date);"]
["RTC","void redemareRTC();"]

{"sheet":"Port Blynk","index":3,"n_rows":12,"n_cols":9,"rows_kept":12,"cut":false,"hidden":false,"merged":[[4,4,4,8],[0,4,0,8]]}
[null,"Port","Type",null,"TYPE du tableau"]
["Blanc","V0","Scrole",null,null,"Max","Pente","Demmarage","Arret"]
["Chaud","V1","Scrole",null,"Type","Value Imput","Value Imput","Time input","Time input"]
["Bleu","V2","Scrole"]
["Rouge","V3","Scrole",null,"Port du tableau"]
["UV","V4","Scrole",null,null,"Max","Pente","Demmarage","Arret"]
["Vert","V5","Scrole",null,"Blanc","V8","V9","V10","V11"]
["Eteint","V6","ON/OFF",null,"Chaud","V12","V13","V14","V15"]
["Rétablir normal","V7","Push",null,"Bleu","V16","V17","V18","V19"]
[{"$nulls":4},"Rouge","V20","V21","V22","V23"]
[{"$nulls":4},"UV","V24","V25","V26","V27"]
[{"$nulls":4},"Vert","V28","V29","V30","V31"]

{"sheet":"Protocole SPI","index":4,"n_rows":31,"n_cols":27,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,1,0,8],[0,10,0,17]]}
[null,"ESP",{"$nulls":8},"STM",{"$nulls":8},"Hex","Action",null,"Abreviation ","Nom",null,"Type","ID"]
["Write Tab Heure",0,0,0,1,"ID","ID","ID","ID",null,0,0,0,1,"ID","ID","ID","ID",null,"0x0X","Write Tab Heure",null,"V1","Ventilateur",null,"Blanc Max","0x01"]
[null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"HEU","HEU","HEU","HEU","HEU","HEU","HEU","HEU",null,"0x1X","Write Tab Value",null,"LED","Type de led",null,"Chaud Max","0x02"]
[null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ","MIN ",null,"0x2X",null,null,"PM","Puissance",null,"Bleu Max","0x03"]
[{"$nulls":19},"0x3X","Read Ventilation",{"$nulls":4},"Rouge Max","0x04"]
["Write Tab Value",0,0,1,0,"ID","ID","ID","ID",null,0,0,1,0,"ID","ID","ID","ID",null,"0x4X","Write Ventilation",{"$nulls":4},"UV Max","0x05"]
[null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"VAL","VAL","VAL","VAL","VAL","VAL","VAL","VAL",null,"0x5X","acknowledge erreur",{"$nulls":4},"Vert Max","0x06"]
[{"$nulls":19},"0x6X","WriteValue",{"$nulls":4},"Blanc Pente","0x08"]
["Read Ventilation",0,0,1,1,"X","X","X","X",null,0,0,1,1,"V1","V1","V1","V1",null,"0x7X","Stop",{"$nulls":4},"Chaud Pente","0x09"]
[{"$nulls":19},"0x8X","Rétablir",{"$nulls":4},"Bleu Pente","0x0A"]
["Write Ventilation",0,1,0,0,"V1","V1","V1","V1",null,0,1,0,0,"V1","V1","V1","V1",null,"0x9X","sync RTC",{"$nulls":4},"Rouge Pente","0X0B"]
[{"$nulls":19},"0xAX",{"$nulls":5},"UV Pente","0x0C"]
["acknowledge erreur",0,1,0,1,"X","X","X","X",null,0,1,0,1,"X","X","X","X",null,"0xBX",{"$nulls":5},"Vert Pente","0x0D"]
[null,"E","R","R","E","U","R",null,1,null,"E","R","R","E","U","R",null,1,null,"0xCX",{"$nulls":5},"Blanc Demmarage","0x01"]
[null,"E","R","R","E","U","R",null,2,null,"E","R","R","E","U","R",null,2,null,"0xDX",{"$nulls":5},"Chaud Demmarage","0x02"]
[{"$nulls":19},"0xEX",{"$nulls":5},"Bleu Demmarage","0x03"]
["WriteValue",0,1,1,0,"ID","ID","ID","ID",null,0,1,1,0,"ID","ID","ID","ID",null,"0xFX",{"$nulls":5},"Rouge Demmarage","0x04"]
[null,"PM","PM","PM","PM","PM","PM","PM","PM",null,"PM","PM","PM","PM","PM","PM","PM","PM",{"$nulls":7},"UV Demmarage","0x05"]
[{"$nulls":25},"Vert Demmarage","0x06"]
["Stop",0,1,1,1,"X","X","X","X",null,0,1,1,1,"X","X","X","X",{"$nulls":7},"Blanc Arret","0x08"]
[{"$nulls":25},"Chaud Arret","0x09"]
["Rétablir",1,0,0,0,"X","X","X","X",null,1,0,0,0,"X","X","X","X",{"$nulls":7},"Bleu Arret","0x0A"]
[{"$nulls":25},"Rouge Arret","0X0B"]
["sync RTC",1,0,0,0,"X","X","X","X",{"$nulls":16},"UV Arret","0x0C"]
[null,"Y","Y","Y","Y","Y","Y","Y","Y",{"$nulls":16},"Vert Arret","0x0D"]
[null,"M","M","M","M","M","M","M","M"]
[null,"J","J","J","J","J","J","J","J"]
[null,"Day","Day","Day","Day","Day","Day","Day","Day"]
[null,"H","H","H","H","H","H","H","H"]
[null,"M","M","M","M","M","M","M","M"]
[null,"S","S","S","S","S","S","S","S"]

{"sheet":"Led erreur","index":5,"n_rows":5,"n_cols":5,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[null,null,"Vert","Orange","Rouge"]
["Erreur","RAS",1,0,0]
[null,"Coupure courant",1,1,0]
[null,"Batterie RTC",1,0,1]
[null,"Oscillator fail",0,0,1]

{"sheet":"AddEEPROM","index":6,"n_rows":25,"n_cols":2,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Nom","address Eeprpm"]
["Blanc Max","0x0000"]
["Chaud Max","0x0002"]
["Bleu Max","0x0004"]
["Rouge Max","0x0006"]
["UV Max","0x0008"]
["Vert Max","0x000A"]
["Blanc Pente","0x000C"]
["Chaud Pente","0x000E"]
["Bleu Pente","0x0010"]
["Rouge Pente","0x0012"]
["UV Pente","0x0014"]
["Vert Pente","0x0016"]
["Blanc Demmarage","0x0018"]
["Chaud Demmarage","0x001A"]
["Bleu Demmarage","0x001C"]
["Rouge Demmarage","0x001E"]
["UV Demmarage","0x0020"]
["Vert Demmarage","0x0022"]
["Blanc Arret","0x0024"]
["Chaud Arret","0x0028"]
["Bleu Arret","0x002A"]
["Rouge Arret","0x002C"]
["UV Arret","0x002E"]
["Vert Arret","0x0030"]